

WS-Biometric Devices Version 1.0

Committee Specification 01

11 July 2017

Specification URIs

This version:

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/cs01/WSBD-v1.0-cs01.pdf> (Authoritative)

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/cs01/WSBD-v1.0-cs01.html>

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/cs01/WSBD-v1.0-cs01.docx>

Previous version:

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/csprd01/WSBD-v1.0-csprd01.pdf> (Authoritative)

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/csprd01/WSBD-v1.0-csprd01.html>

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/csprd01/WSBD-v1.0-csprd01.docx>

Latest version:

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/WSBD-v1.0.pdf> (Authoritative)

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/WSBD-v1.0.html>

<http://docs.oasis-open.org/bioserv/WSBD/v1.0/WSBD-v1.0.docx>

Technical Committee:

[OASIS Biometric Services (BIOSERV) TC](https://www.oasis-open.org/committees/bioserv/)

Chair:

Kevin Mangold (kevin.mangold@nist.gov), [NIST](http://www.nist.gov/)

Editors:

Kevin Mangold (kevin.mangold@nist.gov), [NIST](http://www.nist.gov/)

Kayee Hanaoka (kayee@nist.gov), [NIST](http://www.nist.gov/)

Additional artifacts:

This prose specification is one component of a Work Product that also includes:

* XML schema: <http://docs.oasis-open.org/bioserv/WSBD/v1.0/cs01/schemas/wsbd-v1.0.xsd>

Related work:

This specification replaces or supersedes:

* *Specification for WS-Biometric Devices (WS-BD) Version 1*. <http://www.nist.gov/itl/iad/ig/upload/NIST-SP-500-288-v1.pdf>
* *WS-Biometric Devices Version 1.0*. Edited by Kevin Mangold and Ross J. Micheals. Latest version: <http://docs.oasis-open.org/biometrics/WS-BD/v1.0/WS-BD-v1.0.html>*.*

Declared XML namespace:

* <http://docs.oasis-open.org/bioserv/ns/wsbd-1.0>

Abstract:

WS-Biometric Devices is a protocol for the command and control of biometric sensors using the same protocols that underlie the web.

Status:

This document was last revised or approved by the OASIS Biometric Services (BIOSERV) TC on the above date. The level of approval is also listed above. Check the “Latest version” location noted above for possible later revisions of this document. Any other numbered Versions and other technical work produced by the Technical Committee (TC) are listed at <https://www.oasis-open.org/committees/tc_home.php?wg_abbrev=bioserv#technical>.

TC members should send comments on this specification to the TC’s email list. Others should send comments to the TC’s public comment list, after subscribing to it by following the instructions at the “[Send A Comment](https://www.oasis-open.org/committees/comments/index.php?wg_abbrev=bioserv)” button on the TC’s web page at <https://www.oasis-open.org/committees/bioserv/>.

This Committee Specification is provided under the [RAND](https://www.oasis-open.org/policies-guidelines/ipr#RAND-Mode) Mode of the [OASIS IPR Policy](https://www.oasis-open.org/policies-guidelines/ipr), the mode chosen when the Technical Committee was established. For information on whether any patents have been disclosed that may be essential to implementing this specification, and any offers of patent licensing terms, please refer to the Intellectual Property Rights section of the TC’s web page (<https://www.oasis-open.org/committees/bioserv/ipr.php>).

Note that any machine-readable content ([Computer Language Definitions](https://www.oasis-open.org/policies-guidelines/tc-process#wpComponentsCompLang)) declared Normative for this Work Product is provided in separate plain text files. In the event of a discrepancy between any such plain text file and display content in the Work Product's prose narrative document(s), the content in the separate plain text file prevails.

Citation format:

When referencing this specification the following citation format should be used:

[WSBD-v1.0]

*WS-Biometric Devices Version 1.0.* Edited by Kevin Mangold and Kayee Hanaoka. 11 July 2017. OASIS Committee Specification 01. <http://docs.oasis-open.org/bioserv/WSBD/v1.0/cs01/WSBD-v1.0-cs01.html>. Latest version: <http://docs.oasis-open.org/bioserv/WSBD/v1.0/WSBD-v1.0.html>.

Notices

Copyright © OASIS Open 2017. All Rights Reserved.

All capitalized terms in the following text have the meanings assigned to them in the OASIS Intellectual Property Rights Policy (the "OASIS IPR Policy"). The full [Policy](https://www.oasis-open.org/policies-guidelines/ipr) may be found at the OASIS website.

This document and translations of it may be copied and furnished to others, and derivative works that comment on or otherwise explain it or assist in its implementation may be prepared, copied, published, and distributed, in whole or in part, without restriction of any kind, provided that the above copyright notice and this section are included on all such copies and derivative works. However, this document itself may not be modified in any way, including by removing the copyright notice or references to OASIS, except as needed for the purpose of developing any document or deliverable produced by an OASIS Technical Committee (in which case the rules applicable to copyrights, as set forth in the OASIS IPR Policy, must be followed) or as required to translate it into languages other than English.

The limited permissions granted above are perpetual and will not be revoked by OASIS or its successors or assigns.

This document and the information contained herein is provided on an "AS IS" basis and OASIS DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION HEREIN WILL NOT INFRINGE ANY OWNERSHIP RIGHTS OR ANY IMPLIED WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.

OASIS requests that any OASIS Party or any other party that believes it has patent claims that would necessarily be infringed by implementations of this OASIS Committee Specification or OASIS Standard, to notify OASIS TC Administrator and provide an indication of its willingness to grant patent licenses to such patent claims in a manner consistent with the IPR Mode of the OASIS Technical Committee that produced this specification.

OASIS invites any party to contact the OASIS TC Administrator if it is aware of a claim of ownership of any patent claims that would necessarily be infringed by implementations of this specification by a patent holder that is not willing to provide a license to such patent claims in a manner consistent with the IPR Mode of the OASIS Technical Committee that produced this specification. OASIS may include such claims on its website, but disclaims any obligation to do so.

OASIS takes no position regarding the validity or scope of any intellectual property or other rights that might be claimed to pertain to the implementation or use of the technology described in this document or the extent to which any license under such rights might or might not be available; neither does it represent that it has made any effort to identify any such rights. Information on OASIS' procedures with respect to rights in any document or deliverable produced by an OASIS Technical Committee can be found on the OASIS website. Copies of claims of rights made available for publication and any assurances of licenses to be made available, or the result of an attempt made to obtain a general license or permission for the use of such proprietary rights by implementers or users of this OASIS Committee Specification or OASIS Standard, can be obtained from the OASIS TC Administrator. OASIS makes no representation that any information or list of intellectual property rights will at any time be complete, or that any claims in such list are, in fact, Essential Claims.

The name "OASIS" is a trademark of [OASIS](https://www.oasis-open.org/), the owner and developer of this specification, and should be used only to refer to the organization and its official outputs. OASIS welcomes reference to, and implementation and use of, specifications, while reserving the right to enforce its marks against misleading uses. Please see <https://www.oasis-open.org/policies-guidelines/trademark> for above guidance.

Table of Contents

[1 Introduction 13](#_Toc488327725)

[1.0 IPR Policy 13](#_Toc488327726)

[1.1 Terminology 13](#_Toc488327727)

[1.2 Normative References 14](#_Toc488327728)

[1.3 Document Conventions 18](#_Toc488327729)

[1.3.1 Quotations 18](#_Toc488327730)

[1.3.2 Machine-Readable Code 18](#_Toc488327731)

[1.3.3 Sequence Diagrams 18](#_Toc488327732)

[1.3.4 Examples 19](#_Toc488327733)

[2 Design Concepts and Architecture 19](#_Toc488327734)

[2.1 Interoperability 19](#_Toc488327735)

[2.2 Architectural Components 20](#_Toc488327736)

[2.2.1 Client 20](#_Toc488327737)

[2.2.2 Sensor 20](#_Toc488327738)

[2.2.3 Sensor Service 20](#_Toc488327739)

[2.3 Intended Use 20](#_Toc488327740)

[2.4 General Service Behavior 21](#_Toc488327741)

[2.4.1 Security Model 22](#_Toc488327742)

[2.4.2 HTTP Request-Response Usage 22](#_Toc488327743)

[2.4.3 Client Identity 23](#_Toc488327744)

[2.4.4 Sensor Identity 23](#_Toc488327745)

[2.4.5 Locking 24](#_Toc488327746)

[2.4.5.1 Pending Operations 25](#_Toc488327747)

[2.4.6 Operations Summary 25](#_Toc488327748)

[2.4.7 Idempotency 25](#_Toc488327749)

[2.4.8 Service Lifecycle Behavior 26](#_Toc488327750)

[3 Data Dictionary 27](#_Toc488327751)

[3.1 Namespaces 27](#_Toc488327752)

[3.2 UUID 27](#_Toc488327753)

[3.3 Dictionary 28](#_Toc488327754)

[3.4 Parameter 28](#_Toc488327755)

[3.4.1.1 Element Summary 28](#_Toc488327756)

[3.4.1.2 Supports Multiple 29](#_Toc488327757)

[3.4.1.3 Allowed Values 29](#_Toc488327758)

[3.5 Range 30](#_Toc488327759)

[3.5.1.1 Element Summary 30](#_Toc488327760)

[3.6 Array 31](#_Toc488327761)

[3.7 StringArray 31](#_Toc488327762)

[3.8 UuidArray 31](#_Toc488327763)

[3.9 ResourceArray 32](#_Toc488327764)

[3.10 Resource 32](#_Toc488327765)

[3.11 Resolution 32](#_Toc488327766)

[3.11.1.1 Element Summary 32](#_Toc488327767)

[3.12 Status 33](#_Toc488327768)

[3.12.1.1 Definitions 33](#_Toc488327769)

[3.13 SensorStatus 35](#_Toc488327770)

[3.13.1.1 Definitions 35](#_Toc488327771)

[3.14 Result 35](#_Toc488327772)

[3.14.1 Terminology Shorthand 36](#_Toc488327773)

[3.14.2 Required Elements 36](#_Toc488327774)

[3.14.3 Element Summary 36](#_Toc488327775)

[3.15 Validation 37](#_Toc488327776)

[4 Metadata 38](#_Toc488327777)

[4.1 Service Information 38](#_Toc488327778)

[4.2 Configuration 38](#_Toc488327779)

[4.3 Captured Data 39](#_Toc488327780)

[4.3.1 Minimal Metadata 40](#_Toc488327781)

[4.3.1.1 Capture Date 40](#_Toc488327782)

[4.3.1.2 Modality 40](#_Toc488327783)

[4.3.1.3 Submodality 40](#_Toc488327784)

[4.3.1.4 Content Type 41](#_Toc488327785)

[5 Live Preview 42](#_Toc488327786)

[5.1 Endpoints 42](#_Toc488327787)

[5.2 Heartbeat 43](#_Toc488327788)

[6 Operations 44](#_Toc488327789)

[6.1 General Usage Notes 44](#_Toc488327790)

[6.1.1 Precedence of Status Enumerations 44](#_Toc488327791)

[6.1.2 Parameter Failures 45](#_Toc488327792)

[6.1.3 Visual Summaries 46](#_Toc488327793)

[6.1.3.1 Input & Output 46](#_Toc488327794)

[6.1.3.2 Permitted Status Values 47](#_Toc488327795)

[6.2 Documentation Conventions 48](#_Toc488327796)

[6.2.1 General Information 48](#_Toc488327797)

[6.2.2 Result Summary 49](#_Toc488327798)

[6.2.3 Usage Notes 50](#_Toc488327799)

[6.2.4 Unique Knowledge 50](#_Toc488327800)

[6.2.5 Return Values Detail 50](#_Toc488327801)

[6.3 Register 51](#_Toc488327802)

[6.3.1 Result Summary 51](#_Toc488327803)

[6.3.2 Usage Notes 51](#_Toc488327804)

[6.3.3 Unique Knowledge 51](#_Toc488327805)

[6.3.4 Return Values Detail 51](#_Toc488327806)

[6.3.4.1 Success 51](#_Toc488327807)

[6.3.4.2 Failure 52](#_Toc488327808)

[6.4 Unregister 52](#_Toc488327809)

[6.4.1 Result Summary 52](#_Toc488327810)

[6.4.2 Usage Notes 53](#_Toc488327811)

[6.4.2.1 Inactivity 53](#_Toc488327812)

[6.4.2.2 Sharing Session Ids 53](#_Toc488327813)

[6.4.2.3 Locks & Pending Sensor Operations 53](#_Toc488327814)

[6.4.3 Unique Knowledge 53](#_Toc488327815)

[6.4.4 Return Values Detail 53](#_Toc488327816)

[6.4.4.1 Success 53](#_Toc488327817)

[6.4.4.2 Failure 54](#_Toc488327818)

[6.4.4.3 Sensor Busy 54](#_Toc488327819)

[6.4.4.4 Bad Value 55](#_Toc488327820)

[6.5 Try Lock 55](#_Toc488327821)

[6.5.1 Result Summary 56](#_Toc488327822)

[6.5.2 Usage Notes 56](#_Toc488327823)

[6.5.3 Unique Knowledge 56](#_Toc488327824)

[6.5.4 Return Values Detail 56](#_Toc488327825)

[6.5.4.1 Success 56](#_Toc488327826)

[6.5.4.2 Failure 56](#_Toc488327827)

[6.5.4.3 Lock Held by Another 57](#_Toc488327828)

[6.5.4.4 Bad Value 57](#_Toc488327829)

[6.5.4.5 Invalid Id 58](#_Toc488327830)

[6.6 Steal Lock 58](#_Toc488327831)

[6.6.1 Result Summary 58](#_Toc488327832)

[6.6.2 Usage Notes 58](#_Toc488327833)

[6.6.2.1 Avoid Lock Stealing 59](#_Toc488327834)

[6.6.2.2 Lock Stealing Prevention Period (LSPP) 59](#_Toc488327835)

[6.6.2.3 Cancellation & (Lack of) Client Notification 59](#_Toc488327836)

[6.6.3 Unique Knowledge 59](#_Toc488327837)

[6.6.4 Return Values Detail 59](#_Toc488327838)

[6.6.4.1 Success 59](#_Toc488327839)

[6.6.4.2 Failure 60](#_Toc488327840)

[6.6.4.3 Bad Value 60](#_Toc488327841)

[6.6.4.4 Invalid Id 60](#_Toc488327842)

[6.7 Unlock 61](#_Toc488327843)

[6.7.1 Result Summary 61](#_Toc488327844)

[6.7.2 Usage Notes 61](#_Toc488327845)

[6.7.3 Unique Knowledge 61](#_Toc488327846)

[6.7.4 Return Values Detail 61](#_Toc488327847)

[6.7.4.1 Success 62](#_Toc488327848)

[6.7.4.2 Failure 62](#_Toc488327849)

[6.7.4.3 Sensor Busy 62](#_Toc488327850)

[6.7.4.4 Lock Held by Another 62](#_Toc488327851)

[6.7.4.5 Bad Value 63](#_Toc488327852)

[6.7.4.6 Invalid Id 63](#_Toc488327853)

[6.8 Get Service Info 63](#_Toc488327854)

[6.8.1 Result Summary 64](#_Toc488327855)

[6.8.2 Usage Notes 64](#_Toc488327856)

[6.8.3 Unique Knowledge 65](#_Toc488327857)

[6.8.4 Return Values Detail 65](#_Toc488327858)

[6.8.4.1 Success 65](#_Toc488327859)

[6.8.4.2 Failure 66](#_Toc488327860)

[6.9 Initialize 66](#_Toc488327861)

[6.9.1 Result Summary 66](#_Toc488327862)

[6.9.2 Usage Notes 67](#_Toc488327863)

[6.9.3 Unique Knowledge 67](#_Toc488327864)

[6.9.4 Return Values Detail 67](#_Toc488327865)

[6.9.4.1 Success 67](#_Toc488327866)

[6.9.4.2 Failure 67](#_Toc488327867)

[6.9.4.3 Sensor Timeout 67](#_Toc488327868)

[6.9.4.4 Sensor Failure 68](#_Toc488327869)

[6.9.4.5 Sensor Busy 68](#_Toc488327870)

[6.9.4.6 Lock Not Held 68](#_Toc488327871)

[6.9.4.7 Lock Held by Another 69](#_Toc488327872)

[6.9.4.8 Canceled 69](#_Toc488327873)

[6.9.4.9 Canceled with Sensor Failure 69](#_Toc488327874)

[6.9.4.10 Bad Value 69](#_Toc488327875)

[6.9.4.11 Invalid Id 70](#_Toc488327876)

[6.10 Uninitialize 70](#_Toc488327877)

[6.10.1 Return Values Detail 70](#_Toc488327878)

[6.10.2 Usage Note 71](#_Toc488327879)

[6.10.3 Unique Knowledge 71](#_Toc488327880)

[6.10.4 Return Values Detail 71](#_Toc488327881)

[6.10.4.1 Success 71](#_Toc488327882)

[6.10.4.2 Failure 71](#_Toc488327883)

[6.10.4.3 Sensor Timeout 71](#_Toc488327884)

[6.10.4.4 Sensor Failure 72](#_Toc488327885)

[6.10.4.5 Sensor Busy 72](#_Toc488327886)

[6.10.4.6 Lock Not Held 72](#_Toc488327887)

[6.10.4.7 Lock Held by Another 72](#_Toc488327888)

[6.10.4.8 Canceled 73](#_Toc488327889)

[6.10.4.9 Canceled with Sensor Failure 73](#_Toc488327890)

[6.10.4.10 Bad Value 73](#_Toc488327891)

[6.10.4.11 Invalid Id 74](#_Toc488327892)

[6.11 Get Configuration 74](#_Toc488327893)

[6.11.1 Result Summary 74](#_Toc488327894)

[6.11.2 Usage Notes 75](#_Toc488327895)

[6.11.3 Unique Knowledge 75](#_Toc488327896)

[6.11.4 Return Values Detail 75](#_Toc488327897)

[6.11.4.1 Success 76](#_Toc488327898)

[6.11.4.2 Failure 76](#_Toc488327899)

[6.11.4.3 Configuration Needed 76](#_Toc488327900)

[6.11.4.4 Initialization Needed 76](#_Toc488327901)

[6.11.4.5 Sensor Timeout 77](#_Toc488327902)

[6.11.4.6 Sensor Failure 77](#_Toc488327903)

[6.11.4.7 Sensor Busy 77](#_Toc488327904)

[6.11.4.8 Lock Not Held 78](#_Toc488327905)

[6.11.4.9 Lock Held by Another 78](#_Toc488327906)

[6.11.4.10 Canceled 78](#_Toc488327907)

[6.11.4.11 Canceled with Sensor Failure 78](#_Toc488327908)

[6.11.4.12 Bad Value 79](#_Toc488327909)

[6.11.4.13 Invalid Id 79](#_Toc488327910)

[6.12 Set Configuration 79](#_Toc488327911)

[6.12.1 Result Summary 80](#_Toc488327912)

[6.12.2 Usage Notes 80](#_Toc488327913)

[6.12.2.1 Input Payload Information 80](#_Toc488327914)

[6.12.3 Unique Knowledge 81](#_Toc488327915)

[6.12.4 Return Values Detail 81](#_Toc488327916)

[6.12.4.1 Success 81](#_Toc488327917)

[6.12.4.2 Failure 81](#_Toc488327918)

[6.12.4.3 Initialization Needed 82](#_Toc488327919)

[6.12.4.4 Sensor Timeout 82](#_Toc488327920)

[6.12.4.5 Sensor Failure 82](#_Toc488327921)

[6.12.4.6 Sensor Busy 82](#_Toc488327922)

[6.12.4.7 Lock Not Held 83](#_Toc488327923)

[6.12.4.8 Lock Held by Another 83](#_Toc488327924)

[6.12.4.9 Canceled 83](#_Toc488327925)

[6.12.4.10 Canceled with Sensor Failure 83](#_Toc488327926)

[6.12.4.11 Unsupported 84](#_Toc488327927)

[6.12.4.12 Bad Value 84](#_Toc488327928)

[6.12.4.13 No Such Parameter 85](#_Toc488327929)

[6.12.4.14 Invalid Id 85](#_Toc488327930)

[6.13 Capture 85](#_Toc488327931)

[6.13.1 Result Summary 86](#_Toc488327932)

[6.13.2 Usage Notes 86](#_Toc488327933)

[6.13.2.1 Providing Timing Information 87](#_Toc488327934)

[6.13.3 Unique Knowledge 87](#_Toc488327935)

[6.13.4 Return Values Detail 87](#_Toc488327936)

[6.13.4.1 Success 87](#_Toc488327937)

[6.13.4.2 Failure 87](#_Toc488327938)

[6.13.4.3 Configuration Needed 88](#_Toc488327939)

[6.13.4.4 Initialization Needed 88](#_Toc488327940)

[6.13.4.5 Sensor Timeout 88](#_Toc488327941)

[6.13.4.6 Sensor Failure 88](#_Toc488327942)

[6.13.4.7 Sensor Busy 89](#_Toc488327943)

[6.13.4.8 Lock Not Held 89](#_Toc488327944)

[6.13.4.9 Lock Held by Another 89](#_Toc488327945)

[6.13.4.10 Canceled 89](#_Toc488327946)

[6.13.4.11 Canceled with Sensor Failure 90](#_Toc488327947)

[6.13.4.12 Bad Value 90](#_Toc488327948)

[6.13.4.13 Invalid Id 90](#_Toc488327949)

[6.14 Begin Capture 91](#_Toc488327950)

[6.14.1 Result Summary 91](#_Toc488327951)

[6.14.2 Usage Notes 91](#_Toc488327952)

[6.14.3 Unique Knowledge 92](#_Toc488327953)

[6.14.4 Return Values Detail 92](#_Toc488327954)

[6.14.4.1 Success 92](#_Toc488327955)

[6.14.4.2 Failure 92](#_Toc488327956)

[6.14.4.3 Configuration Needed 92](#_Toc488327957)

[6.14.4.4 Initialization Needed 93](#_Toc488327958)

[6.14.4.5 Sensor Timeout 93](#_Toc488327959)

[6.14.4.6 Sensor Failure 93](#_Toc488327960)

[6.14.4.7 Sensor Busy 94](#_Toc488327961)

[6.14.4.8 Lock Not Held 94](#_Toc488327962)

[6.14.4.9 Lock Held by Another 94](#_Toc488327963)

[6.14.4.10 Canceled 94](#_Toc488327964)

[6.14.4.11 Canceled with Sensor Failure 95](#_Toc488327965)

[6.14.4.12 Bad Value 95](#_Toc488327966)

[6.14.4.13 Invalid Id 95](#_Toc488327967)

[6.15 End Capture 96](#_Toc488327968)

[6.15.1 Result Summary 96](#_Toc488327969)

[6.15.2 Usage Notes 96](#_Toc488327970)

[6.15.2.1 Transferrable Asynchronous Captures 97](#_Toc488327971)

[6.15.2.2 Status Monitoring 97](#_Toc488327972)

[6.15.3 Unique Knowledge 97](#_Toc488327973)

[6.15.4 Return Values Detail 97](#_Toc488327974)

[6.15.4.1 Success 97](#_Toc488327975)

[6.15.4.2 Failure 97](#_Toc488327976)

[6.15.4.3 Sensor Timeout 98](#_Toc488327977)

[6.15.4.4 Sensor Failure 98](#_Toc488327978)

[6.15.4.5 Sensor Busy 98](#_Toc488327979)

[6.15.4.6 Lock Not Held 99](#_Toc488327980)

[6.15.4.7 Lock Held by Another 99](#_Toc488327981)

[6.15.4.8 Canceled 99](#_Toc488327982)

[6.15.4.9 Canceled with Sensor Failure 99](#_Toc488327983)

[6.15.4.10 Bad Value 100](#_Toc488327984)

[6.15.4.11 Invalid Id 100](#_Toc488327985)

[6.16 Download 100](#_Toc488327986)

[6.16.1 Result Summary 101](#_Toc488327987)

[6.16.2 Usage Notes 101](#_Toc488327988)

[6.16.2.1 Capture and Download as Separate Operations 101](#_Toc488327989)

[6.16.2.2 Services with Post-Acquisition Processing 101](#_Toc488327990)

[6.16.2.3 Client Notification 104](#_Toc488327991)

[6.16.3 Unique Knowledge 105](#_Toc488327992)

[6.16.4 Return Values Detail 105](#_Toc488327993)

[6.16.4.1 Success 105](#_Toc488327994)

[6.16.4.2 Failure 105](#_Toc488327995)

[6.16.4.3 Preparing Download 106](#_Toc488327996)

[6.16.4.4 Bad Value 106](#_Toc488327997)

[6.16.4.5 Invalid Id 106](#_Toc488327998)

[6.17 Get Download Info 106](#_Toc488327999)

[6.17.1 Result Summary 107](#_Toc488328000)

[6.17.2 Usage Notes 107](#_Toc488328001)

[6.17.3 Unique Knowledge 107](#_Toc488328002)

[6.17.4 Return Values Detail 107](#_Toc488328003)

[6.17.4.1 Success 107](#_Toc488328004)

[6.17.4.2 Failure 108](#_Toc488328005)

[6.17.4.3 Preparing Download 108](#_Toc488328006)

[6.17.4.4 Bad Value 108](#_Toc488328007)

[6.17.4.5 Invalid Id 108](#_Toc488328008)

[6.18 Thrifty Download 109](#_Toc488328009)

[6.18.1 Result Summary 109](#_Toc488328010)

[6.18.2 Usage Notes 110](#_Toc488328011)

[6.18.3 Unique Knowledge 110](#_Toc488328012)

[6.18.4 Return Values Detail 110](#_Toc488328013)

[6.18.4.1 Success 110](#_Toc488328014)

[6.18.4.2 Failure 111](#_Toc488328015)

[6.18.4.3 Preparing Download 111](#_Toc488328016)

[6.18.4.4 Unsupported 111](#_Toc488328017)

[6.18.4.5 Bad Value 111](#_Toc488328018)

[6.18.4.6 Invalid Id 112](#_Toc488328019)

[6.19 Get Sensor Data 112](#_Toc488328020)

[6.19.1 Result Summary 112](#_Toc488328021)

[6.19.2 Usage Notes 112](#_Toc488328022)

[6.19.3 Unique Knowledge 113](#_Toc488328023)

[6.20 Cancel 113](#_Toc488328024)

[6.20.1 Result Summary 113](#_Toc488328025)

[6.20.2 Usage Notes 113](#_Toc488328026)

[6.20.2.1 Canceling Non-Sensor Operations 114](#_Toc488328027)

[6.20.2.2 Cancellation Triggers 114](#_Toc488328028)

[6.20.3 Unique Knowledge 115](#_Toc488328029)

[6.20.4 Return Values Detail 115](#_Toc488328030)

[6.20.4.1 Success 115](#_Toc488328031)

[6.20.4.2 Failure 115](#_Toc488328032)

[6.20.4.3 Lock Not Held 115](#_Toc488328033)

[6.20.4.4 Lock Held by Another 115](#_Toc488328034)

[6.20.4.5 Bad Value 116](#_Toc488328035)

[6.20.4.6 Invalid Id 116](#_Toc488328036)

[6.21 Get Sensor Status 116](#_Toc488328037)

[6.21.1 Result Summary 117](#_Toc488328038)

[6.21.2 Usage Notes 117](#_Toc488328039)

[6.21.3 Unique Knowledge 117](#_Toc488328040)

[6.21.4 Return Values Detail 117](#_Toc488328041)

[6.21.4.1 Success 117](#_Toc488328042)

[7 Conformance Profiles 118](#_Toc488328043)

[7.1.1 Conformance 118](#_Toc488328044)

[7.1.2 Language 118](#_Toc488328045)

[7.1.3 Operations 118](#_Toc488328046)

[7.1.3.1 Additional Supported Operations 119](#_Toc488328047)

[7.2 Fingerprint 119](#_Toc488328048)

[7.2.1 Service Information 119](#_Toc488328049)

[7.2.1.1 Submodality 119](#_Toc488328050)

[7.2.1.2 Image Size 120](#_Toc488328051)

[7.2.1.3 Image Content Type 120](#_Toc488328052)

[7.2.1.4 Image Density 121](#_Toc488328053)

[7.3 Face 121](#_Toc488328054)

[7.3.1 Service Information 121](#_Toc488328055)

[7.3.1.1 Submodality 121](#_Toc488328056)

[7.3.1.2 Image Size 121](#_Toc488328057)

[7.3.1.3 Image Content Type 122](#_Toc488328058)

[7.4 Iris 122](#_Toc488328059)

[7.4.1 Service Information 122](#_Toc488328060)

[7.4.1.1 Submodality 122](#_Toc488328061)

[7.4.1.2 Image Size 122](#_Toc488328062)

[7.4.1.3 Image Content Type 122](#_Toc488328063)

[7.5 Unknown 123](#_Toc488328064)

[7.5.1 Service Information 123](#_Toc488328065)

[7.5.1.1 Submodality 123](#_Toc488328066)

[7.5.1.2 Image Size 123](#_Toc488328067)

[7.5.1.3 Image Content Type 123](#_Toc488328068)

[Appendix A. Parameter Details 124](#_Toc488328069)

[A.1 Sensor Service 124](#_Toc488328070)

[A.1.1 Modality 124](#_Toc488328071)

[A.1.2 Submodality 125](#_Toc488328072)

[A.2 Connections 125](#_Toc488328073)

[A.2.1 Last Updated 125](#_Toc488328074)

[A.2.2 Inactivity Timeout 125](#_Toc488328075)

[A.2.3 Maximum Concurrent Sessions 126](#_Toc488328076)

[A.2.4 Least Recently Used (LRU) Sessions Automatically Dropped 126](#_Toc488328077)

[A.3 Timeouts 126](#_Toc488328078)

[A.3.1 Initialization Timeout 126](#_Toc488328079)

[A.3.2 Get Configuration Timeout 127](#_Toc488328080)

[A.3.3 Set Configuration Timeout 127](#_Toc488328081)

[A.3.4 Capture Timeout 127](#_Toc488328082)

[A.3.5 Post-Acquisition Processing Time 127](#_Toc488328083)

[A.3.6 Lock Stealing Prevention Period 127](#_Toc488328084)

[A.4 Storage 128](#_Toc488328085)

[A.4.1 Maximum Storage Capacity 128](#_Toc488328086)

[A.4.2 Least-Recently Used Capture Data Automatically Dropped 128](#_Toc488328087)

[Appendix B. Content Type Data 129](#_Toc488328088)

[B.1 General Type 129](#_Toc488328089)

[B.2 Image Formats 129](#_Toc488328090)

[B.3 Video Formats 129](#_Toc488328091)

[B.4 Audio Formats 129](#_Toc488328092)

[B.5 General Biometric Formats 130](#_Toc488328093)

[B.6 ISO / Modality-Specific Formats 130](#_Toc488328094)

[Appendix C. XML Schema 132](#_Toc488328095)

[Appendix D. Security (Informative) 135](#_Toc488328096)

[D.1 References 135](#_Toc488328097)

[D.2 Overview 136](#_Toc488328098)

[D.3 Control Set Determination 136](#_Toc488328099)

[D.3.1 “L” Security Control Criteria 136](#_Toc488328100)

[D.3.2 “M” Security Control Criteria 136](#_Toc488328101)

[D.3.3 “H” Security Control Criteria 137](#_Toc488328102)

[D.4 Recommended & Candidate Security Controls 137](#_Toc488328103)

[D.4.1 “L” Security Controls 137](#_Toc488328104)

[D.4.2 “M” Security Controls 137](#_Toc488328105)

[D.4.3 “H” Security Controls 138](#_Toc488328106)

[Appendix E. Acknowledgments 139](#_Toc488328107)

[Appendix F. Revision History 141](#_Toc488328108)

# Introduction

*The web services framework, has, in essence, begun to create a standard software “communications bus” in support of service-oriented architecture. Applications and services can “plug in” to the bus and begin communicating using standards tools. The emergence of this “bus” has profound implications for identity exchange.*

Jamie Lewis, Burton Group, February 2005
Forward to *Digital Identity* by Phillip J. Windley

As noted by Jamie Lewis, the emergence of web services as a common communications bus has “profound implications.” The next generation of biometric devices will not only need to be intelligent, secure, tamper-proof, and spoof resistant, but first, they will need to be *interoperable****.***

These envisioned devices will require a communications protocol that is secure, globally connected, and free from requirements on operating systems, device drivers, form factors, and low-level communications protocols. WS-Biometric Devices is a protocol designed in the interest of furthering this goal, with a specific focus on the single process shared by all biometric systems—*acquisition*.

## IPR Policy

This Committee Specification is provided under the [RAND](https://www.oasis-open.org/policies-guidelines/ipr#RAND-Mode) Mode of the [OASIS IPR Policy](https://www.oasis-open.org/policies-guidelines/ipr), the mode chosen when the Technical Committee was established.

For information on whether any patents have been disclosed that may be essential to implementing this specification, and any offers of patent licensing terms, please refer to the Intellectual Property Rights section of the TC’s web page (<https://www.oasis-open.org/committees/bioserv/ipr.php>).

## Terminology

This section contains terms and definitions used throughout this document.

The key words “MUST”, “MUST NOT”, “REQUIRED”, “SHALL”, “SHALL NOT”, “SHOULD”, “SHOULD NOT”, “RECOMMENDED”, “MAY”, and “OPTIONAL” in this document are to be interpreted as described in [RFC2119].

biometric capture device

a system component capable of capturing biometric data in digital form

client

a logical endpoint that originates operation requests

HTTP

Hypertext Transfer Protocol. Unless specified, the term HTTP refers to either HTTP as defined in [RFC2616] or HTTPS as defined in [RFC2660].

ISO

International Organization for Standardization

modality

a distinct biometric category or type of biometric—typically a short, high-level description of a human feature or behavioral characteristic (e.g., “fingerprint,” “iris,” “face,” or “gait”)

payload

the content of an HTTP request or response. An **input payload** refers to the XML content of an HTTP *request*. An **output payload** refers to the XML content of an HTTP *response.*

payload parameter

an operation parameter that is passed to a service within an input payload

profile

a list of assertions that a service MUST support

REST

Representational State Transfer

RESTful

a web service which employs REST techniques

sensor or biometric sensor

a single biometric capture device or a logical collection of biometric capture devices

SOAP

Simple Object Access Protocol

submodality

a distinct category or subtype within a biometric modality

target sensor or target biometric sensor

the biometric sensor made available by a particular service

URL parameter

a parameter passed to a web service by embedding it in the URL

Web service or service or WS

a software system designed to support interoperable machine-to-machine interaction over a network [WSGloss]

XML

Extensible Markup Language [XML]

## Normative References

|  |  |
| --- | --- |
| **[3GPP]** | 3GPP, *3GPP TS 26.244 Transparent end-to-end packet switched streaming service (PSS) 3GPP file format (3GP)*, <http://www.3gpp.org/DynaReport/26244.htm>, Retrieved 12 August 2014 |
| **[3GPP2]** | 3GPP2, *C.S0050-B Version 1.0 3GPP2 File Formats for Multimedia Services,* <http://www.3gpp2.org/Public_html/specs/C.S0050-B_v1.0_070521.pdf>, 18 May 2007 |
| **[AIFF]** | Apple Computer, Inc., *Audio Interchange File Format: "AIFF". A Standard for Sampled Sound Files Version 1.3,* <http://www-mmsp.ece.mcgill.ca/Documents/AudioFormats/AIFF/Docs/AIFF-1.3.pdf>, January 4, 1989 |
| **[AN2K]** | *Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial, & Scar Mark & Tattoo (SMT) Information*, <http://www.nist.gov/customcf/get_pdf.cfm?pub_id=151453>, 27 July 2000. |
| **[AN2K11]** | B. Wing, *Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial & Other Biometric Information*, <http://www.nist.gov/customcf/get_pdf.cfm?pub_id=910136>, November 2011. |
| **[AN2K7]** | R. McCabe, E. Newton, *Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial, & Other Biometric Information – Part 1*, <http://www.nist.gov/customcf/get_pdf.cfm?pub_id=51174>, 20 April 2007. |
| **[AN2K8]** | E. Newton et al., *Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial, & Other Biometric Information – Part 2: XML Version*, <http://www.nist.gov/customcf/get_pdf.cfm?pub_id=890062>, 12 August 2008. |
| **[ASF]** | *Overview of the ASF Format,* [http://msdn.microsoft.com/en-us/library/windows/desktop/dd757562%28v=vs.85%29.aspx](http://msdn.microsoft.com/en-us/library/windows/desktop/dd757562%28v%3Dvs.85%29.aspx), Retrieved 13 August 2014 |
| **[ASX]** | *Windows Media Metafile Elements Reference,* <http://msdn.microsoft.com/en-us/library/dd564668%28VS.85%29.aspx>*,* Retrieved 13 August 2014 |
| **[AVI]** | *AVI RIFF File Format,* <http://msdn.microsoft.com/en-us/library/ms779636.aspx>,Retrieved 12 August 2014 |
| **[BDIF1007]** | ISO/IEC 19794-10:2007: Information technology – Biometric data interchange formats – Part 10: Hand geometry silhouette data |
| **[BDIF205]** | ISO/IEC 19794-2:2005/Cor 1:2009/Amd 1:2010: Information technology – Biometric data interchange formats – Part 2: Finger minutia data |
| **[BDIF215]** | ISO/IEC 19794-2:2011/Amd 2:2015: Information technology – Biometric data interchange formats – Part 2: Finger minutia data |
| **[BDIF306]** | ISO/IEC 19794-3:2006: Information technology – Biometric data interchange formats – Part 3: Finger pattern spectral data |
| **[BDIF405]** | ISO/IEC 19794-4:2005: Information technology – Biometric data interchange formats – Part 4: Finger image data |
| **[BDIF415]** | ISO/IEC 19794-4:2011/Amd 2:2015: Information technology – Biometric data interchange formats – Part 4: Finger image data |
| **[BDIF505]** | ISO/IEC 19794-5:2005: Information technology – Biometric data interchange formats – Part 5: Face image data |
| **[BDIF515]** | ISO/IEC 19794-5:2011/Amd 2:2015: Information technology – Biometric data interchange formats – Part 5: Face image data |
| **[BDIF605]** | ISO/IEC 19794-6:2005: Information technology – Biometric data interchange formats – Part 6: Iris image data |
| **[BDIF611]** | ISO/IEC 19794-6:2011: Information technology – Biometric data interchange formats – Part 6: Iris image data |
| **[BDIF615]** | ISO/IEC 19794-6:2011/Amd 1:2015: Information technology – Biometric data interchange formats – Part 6: Iris image data |
| **[BDIF707]** | ISO/IEC 19794-7:2007/Cor 1:2009: Information technology – Biometric data interchange formats – Part 7: Signature/sign time series data |
| **[BDIF715]** | ISO/IEC 19794-7:2014/Amd 1:2015: Information technology – Biometric data interchange formats – Part 7: Signature/sign time series data |
| **[BDIF806]** | ISO/IEC 19794-8:2006/Cor 1:2011: Information technology – Biometric data interchange formats – Part 8: Finger pattern skeletal data |
| **[BDIF806]** | ISO/IEC 19794-8:2011/Amd 1:2014: Information technology – Biometric data interchange formats – Part 8: Finger pattern skeletal data |
| **[BDIF907]** | ISO/IEC 19794-9:2007: Information technology – Biometric data interchange formats – Part 9: Vascular image data |
| **[BMP]** | *BMP File Format*, <http://www.digicamsoft.com/bmp/bmp.html> |
| **[CBEFF2010]** | ISO/IEC 19785-3:2007/Amd 1:2010: Information technology – Common Biometric Exchange Formats Framework – Part 3: Patron format specifications with Support for Additional Data Elements |
| **[CBEFF2015]** | ISO/IEC 19785-3:2015: Information technology – Common Biometric Exchange Formats Framework – Part 3: Patron format specifications with Support for Additional Data Elements |
| **[CMediaType]** | *Media Types*, <http://www.iana.org/assignments/media-types/media-types.xhtml>*, 8 August 2014* |
| **[H264]** | Y.-K. Wang et al., *RTP Payload Format for H.264 Video*, <http://www.ietf.org/rfc/rfc6184.txt>*,* IETF RFC 6184, May 2011. |
| **[HTML5]** | *HTML5, I. Hickson, R. Berjon, S. Faulkner, T. Leithead, E. Doyle Navara, T., S. Pfeiffer, Editors, W3C Recommendation, 28 October 2014,* [*http://www.w3.org/TR/2014/REC-html5-20141028/*](http://www.w3.org/TR/2014/REC-html5-20141028/)*. Latest version available at* <http://www.w3.org/TR/html5/>. |
| **[JPEG]** | E. Hamilton, *JPEG File Interchange Format*, <http://www.w3.org/Graphics/JPEG/jfif3.pdf>, 1 September 1992. |
| **[MPEG]** | ISO/IEC 14496: Information technology – Coding of audio-visual objects |
| **[MPEG1]** | ISO/IEC 11172-3:1993/Cor 1:1996 Information technology – Coding of moving pictures and associated audio for digital storage media at up to about 1.5 Mbit/s -- Part 3: Audio |
| **[OGG]** | Xiph.org,<http://xiph.org/ogg/>,Retrieved 12 August 2014 |
| **[PNG]** | D. Duce et al., *Portable Network Graphics (PNG) Specification (Second Edition)*, <http://www.w3.org/TR/2003/REC-PNG-20031110>, 10 November 2003. |
| **[QTFF]** | *Introduction to Quicktime File Format Specification,* <https://developer.apple.com/library/mac/documentation/QuickTime/QTFF/QTFFPreface/qtffPreface.html>,Retrieved 12 August 2014 |
| **[RFC1737]** | K. Sollins, L. Masinter, *Functional Requirements for Uniform Resource Names*, <http://www.ietf.org/rfc/rfc1737.txt>, IETC RFC 1737, December 1994. |
| **[RFC2045]** | N. Freed and N. Borenstein, *Multipurpose Internet Mail Extensions (MIME) Part One: Format of Internet Message Bodies*, <http://www.ietf.org/rfc/rfc2045.txt>, IETF RFC 2045, November 1996. |
| **[RFC2046]** | N. Freed and N. Borenstein, *Multipurpose Internet Mail Extensions (MIME) Part Two: Media Types*, <http://www.ietf.org/rfc/rfc2046.txt>, IETF RFC 2045, November 1996. |
| **[RFC2119]** | S. Bradner, *Key words for use in RFCs to Indicate Requirement Levels*, <http://www.ietf.org/rfc/rfc2119.txt>, IETF RFC 2119, March 1997. |
| **[RFC2141]** | R. Moats, *URN Syntax*, <http://www.ietf.org/rfc/rfc2141.txt>, IETF RFC 2141, May 1997 |
| **[RFC2616]** | R. Fielding, et al., *Hypertext Tranfer Protocol—HTTP/1.1*, <http://www.ietf.org/rfc/rfc2616.txt>, IETF RFC 2616, June 1999. |
| **[RFC2660]** | E. Rescorla et al., *The Secure HyperText Transfer Protocol*, <http://www.ietf.org/rfc/rfc2660.txt>, IETF RFC 2660, August 1999. |
| **[RFC3001]** | M. Mealling, *A URN Namespace of Object Identifiers*, <http://www.ietf.org/rfc/rfc3001.txt>, IETF RFC 3001, November 2000. |
| **[RFC4122]** | P. Leach, M. Mealling, and R. Salz, *A Universally Unique Identifier (UUID) URN Namespace*, <http://www.ietf.org/rfc/rfc4122.txt>, IETF RFC 4122, July 2005. |
| **[SSE]** | Server Sent Events, Ian Hickson, Google, Inc., W3C Recommendation, 29 October 2009, <https://www.w3.org/TR/2009/WD-eventsource-20091029/>, Retrieved 19 January 2017 |
| **[SPHERE]** | National Institute of Standards and Technology*, NIST Speech Header Resources,* <http://www.nist.gov/itl/iad/mig/tools.cfm>, Retrieved 12 August 2014 |
| **[TIFF]** | *TIFF Revision 6.0*, <http://partners.adobe.com/public/developer/en/tiff/TIFF6.pdf>, 3 June 1992. |
| **[WAVE]** | IBM Corporation and Microsoft Corporation, *Multimedia Programming Interface and Data Specifications 1.0,* <http://www.tactilemedia.com/info/MCI_Control_Info.html>, *August 1991* |
| **[WSGloss]** | *Web Services Glossary*, H. Haas, A. Brown, Editors, W3C Working Group Note Interest Group Note Coordination Group Note, 11 February 2004, <http://www.w3.org/TR/2004/NOTE-ws-gloss-20040211/>. Latest version available at <http://www.w3.org/TR/ws-gloss/>. |
| **[WSQ]** | *WSQ Gray-Scale Fingerprint Image Compression Specification Version 3.1*, <https://fbibiospecs.org/docs/WSQ_Gray-scale_Specification_Version_3_1_Final.pdf>, 4 October 2010. |
| **[XML]** | *Extensible Markup Language (XML) 1.0 (Fifth Edition)*, T. Bray, J. Paoli, M., E. Maler, F. Yergeau, Editors, W3C Recommendation. 26 November 2008, <http://www.w3.org/TR/2008/REC-xml-20081126/>. Latest version available at <http://www.w3.org/TR/xml/>. |
| **[XMLNS]** | *Namespaces in XML 1.0 (Third Edition)*, T. Bray, D. Hollander, A. Layman, R. Tobin, H.S. Thompson, Editors, W3C Recommendation. 8 December2009, <http://www.w3.org/TR/2009/REC-xml-names-20091208/>. Latest version available at <http://www.w3.org/TR/xml-names>. |
| **[XSDPart1]** | *XML Schema Part 1: Structures Second Edition*, H. S. Thompson, D. Beech, M. Maloney, M. Mendelsohn, Editors, W3C Recommendation, 28 October 2004, <http://www.w3.org/TR/2004/REC-xmlschema-1-20041028/>. Latest version available at <http://www.w3.org/TR/xml-schema-1/>. |
| **[XSDPart2]** | *XML Schema Part 2: Datatypes Second Edition*, P. Biron, A. Malhotra, Editors, W3C Recommendation, <http://www.w3.org/TR/2004/REC-xmlschema-2-20041028/>. Latest Version available at http:://www.w3.org/TR/xmlschema-2/. |

## Document Conventions

### Quotations

If the inclusion of a period within a quotation might lead to ambiguity as to whether or not the period should be included in the quoted material, the period will be placed outside the trailing quotation mark. For example, a sentence that ends in a quotation would have the trailing period “inside the quotation, like this quotation punctuated like this.” However, a sentence that ends in a URL would have the trailing period outside the quotation mark, such as “http://example.com”.

### Machine-Readable Code

With the exception of some reference URLs, machine-readable information will typically be depicted with a mono-spaced font, such as this.

### Sequence Diagrams

Throughout this document, sequence diagrams are used to help explain various scenarios. These diagrams are informative simplifications and are intended to help explain core specification concepts. Operations are depicted in a functional, remote procedure call style.

The following is an annotated sequence diagram that shows how an example sequence of HTTP request-responses is typically illustrated. The level of abstraction presented in the diagrams, and the details that are shown (or not shown) will vary according to the particular information being illustrated. First time readers may wish to skip this section and return to it as needed.



**Figure 1**. Example of a sequence diagram used in this document.

1. Each actor in the sequence diagram (i.e., a client or a server) has a “swimlane” that chronicles their interactions over time. Communication among the actors is depicted with arrows. In this diagram, there are three actors: “Client A,” a WS-BD “Service,” and “Client B.”
2. State information notable to the example is depicted in an elongated diamond shape within the swimlane of the relevant actor. In this example, it is significant that the initial “lock owner” for the “Service” actor is “(none)” and that the “lock owner” changes to “{A1234567…}” after a communication from Client A.
3. Unless otherwise noted, a solid arrow represents the request (initiation) of an HTTP request; the *opening* of an HTTP socket connection and the transfer of information from a source to its destination. The arrow begins on the swimlane of the originator and ends on the swimlane of the destination. The order of the request and the operation name (§6.3 through §6.21) are shown above the arrow. URL and/or payload parameters significant to the example are shown below the arrow. In this example, the first communication occurs when Client A opens a connection to the Service, initiating a “lock” request, where the “sessionId” parameter is “{A1234567…}.”
4. Unless otherwise noted, a dotted arrow represents the response (completion) of a particular HTTP request; the *closing* of an HTTP socket connection and the transfer of information back from the destination to the source. The arrow startson the originating request’s *destination* and ends on the swimlane of actor that *originated* the request. The order of the request, and the name of the operation that being replied to is shown above the arrow. Significant data “returned” to the source is shown below the arrow in the form of a Result (§3.13). Notice that the source, destination, and operation name provide the means to match the response corresponds to a particular request—there is no other visual indicator. In this example, the second communication is the response to the “lock” request, where the service returns a “status” of “success.

In general, “{A1234567…}” and “{B890B123…}” are used to represent session ids (§2.4.3, §3.14.3, §6.3); “{C1D10123...}” and “{D2E21234...}” represent capture ids (§3.14.3, §6.12.4.14).

### Examples

Unless specified otherwise, all examples and sample code are provided for illustrative purposes and are informative.

# Design Concepts and Architecture

This section describes the major design concepts and overall architecture of WS-BD. The main purpose of a WS-BD service is to expose a target biometric sensor to clients via web services.

This specification provides a framework for deploying and invoking core synchronous operations via lightweight web service protocols for the command and control of biometric sensors. The design of this specification is influenced heavily by the REST architecture; deviations and tradeoffs were made to accommodate the inherent mismatches between the REST design goals and the limitations of devices that are (typically) oriented for a single-user.

## Interoperability

[ISO/IEC 2382](http://en.wikipedia.org/w/index.php?title=ISO/IEC_2382&action=edit&redlink=1)-1 (1993) defines *interoperability* as “*the capability to communicate, execute programs, or transfer data among various functional units in a manner that requires the user to have little to no knowledge of the unique characteristics of those units.”*

Conformance to a standard does not necessarily guarantee interoperability. An example is conformance to an HTML specification. An HTML page may be conformant to the HTML 4.0 specification, but it is not interoperable between web browsers. Each browser has its own interpretation of how the content should be displayed. To overcome this, web developers add a note suggesting which web browsers are compatible for viewing. Interoperable web pages need to have the same visual outcome independent of which browser is used.

A major design goal of WS-BD is to *maximize* interoperability, by *minimizing* the required “knowledge of the unique characteristics” of a component that supports WS-BD. The authors recognize that conformance to this specification alone cannot guarantee interoperability; although a minimum degree of functionality is implied. Sensor *profiles* and accompanying conformance tests will need to be developed to provide better guarantees of interoperability, and will be released in the future.

## Architectural Components

Before discussing the envisioned use of WS-BD, it is useful to distinguish between the various components that comprise a WS-BD implementation. These are *logical*components that may or may not correspond to particular *physical* boundaries. This distinction becomes vital in understanding WS-BD’s operational models.

### Client

A *client* is any software component that originates requests for biometric acquisition. Note that a client might be one of many hosted in a parent (logical or physical) component, and that a client might send requests to a variety of destinations.

|  |  |
| --- | --- |
|  | This icon is used to depict an arbitrary WS-BD client. A personal digital assistant (PDA) is used to serve as a reminder that a client might be hosted on a non-traditional computer. |

### Sensor

A biometric *sensor* is any component that is capable of acquiring a digital biometric sample. Most sensor components are hosted within a dedicated hardware component, but this is not always true. For example, a keyboard is a general input device, but might also be used for a keystroke dynamics biometric.

|  |  |
| --- | --- |
|  | This icon is used to depict a biometric sensor. The icon has a vague similarity to a fingerprint scanner, but should be thought of as an arbitrary biometric sensor. |

The term “sensor” is used in this document in a singular sense, but may in fact be referring to multiple biometric capture devices. Because the term “sensor” may have different interpretations, practitioners are encouraged to detail the physical and logical boundaries that define a “sensor” for their given context.

### Sensor Service

The *sensor service* is the “middleware” software component that exposes a biometric sensor to a client through web services. The sensor service adapts HTTP request-response operations to biometric sensor command & control.

|  |  |
| --- | --- |
|  | This icon is used to depict a sensor service. The icon is abstract and has no meaningful form, just as a sensor service is a piece of software that has no physical form. |

## Intended Use

Each implementation of WS-BD will be realized via a mapping of logical to physical components. A distinguishing characteristic of an implementation will be the physical location of the sensor service component. WS-BD is designed to support two scenarios:

1. **Physically separated.** The sensor service and biometric sensor are hosted by different physical components. A *physically separated service* is one where there is both a physical and logical separation between the biometric sensor and the service that provides access to it.
2. **Physically integrated.** The sensor service and biometric sensor are hosted within the same physical component. A *physically integrated service* is one where the biometric sensor and the service that provides access to it reside within the same physical component.

Figure 2 depicts a physically separated service. In this scenario, a biometric sensor is tethered to a personal computer, workstation, or server. The web service, hosted on the computer, listens for communication requests from clients. An example of such an implementation would be a USB fingerprint scanner attached to a personal computer. A lightweight web service, running on that computer could listen to requests from local (or remote) clients—translating WS-BD requests to and from biometric sensor commands.



**Figure 2**. A physically separated WS-Biometric Devices (WS-BD) implementation.

Figure 3 depicts a physically integrated service. In this scenario, a single hardware device has an embedded biometric sensor, as well as a web service. Analogous (but not identical) functionality is seen in many network printers; it is possible to point a web browser to a local network address, and obtain a web page that displays information about the state of the printer, such as toner and paper levels (WS-BD enabled devices do not provide web pages to a browser). Clients make requests directly to the integrated device; and a web service running within an embedded system translates the WS-BD requests to and from biometric sensor commands.



**Figure 3**. A physically integrated WS-Biometric Devices (WS-BD) implementation.

The “separated” versus “integrated” distinction is a simplification with a potential for ambiguity. For example, one might imagine putting a hardware shell around a USB fingerprint sensor connected to a small form-factor computer. Inside the shell, the sensor service and sensor are on different physical components. Outside the shell, the sensor service and sensor appear integrated. Logical encapsulations, i.e., layers of abstraction, can facilitate analogous “hiding”. The definition of what constitutes the “same” physical component depends on the particular implementation and the intended level of abstraction. Regardless, it is a useful distinction in that it illustrates the flexibility afforded by leveraging interoperable communications protocols. As suggested in §2.2.2practitioners *may* need to clearly define appropriate logical and physical boundaries for their own context of use.

## General Service Behavior

The following section describes the general behavior of WS-BD clients and services.

### Security Model

In this document, it is assumed that if a client is able to establish a connection with the sensor service, then the client is fully authorized to use the service. This implies that all successfully connected clients have equivalent access to the same service. Clients might be required to connect through various HTTP protocols, such as HTTPS with client-side certificates, or a more sophisticated protocol such as Open Id (http://openid.net/) and/or OAuth.

Specific security measures are out of scope of this specification, but should be carefully considered when implementing a WS-BD service. Some recommended solutions to general scenarios are outlined Appendix D.

### HTTP Request-Response Usage

Most biometrics devices are inherently *single user—*i.e., they are designed to sample the biometrics from a single user at a given time. Web services, on the other hand, are intended for *stateless* and *multiuser* use*.* A biometric device exposed via web services *must* therefore provide a mechanism to reconcile these competing viewpoints.

Notwithstanding the native limits of the underlying web server, WS-BD services *must* be capable of handling multiple, concurrent requests. Services MUSTrespond to requests for operations that do not require exclusive control of the biometric sensor and MUSTdo so without waiting until the biometric sensor is in a particular state.

Because there is no well-accepted mechanism for providing asynchronous notification via REST, each individual operation MUSTblock until completion. That is, the web server does not reply to an individual HTTP request until the operation that is triggered by that request is finished.

Individual clients are not expected to poll—rather they make a single HTTP request and block for the corresponding result. Because of this, it is expected that a client would perform WS-BD operations on an independent thread, so not to interfere with the general responsiveness of the client application. WS-BD clients therefore MUSTbe configured in such a manner such that individual HTTP operations have timeouts that are compatible with a particular implementation.

WS-BD operations may take longer than typical REST services. Consequently, there is a clear need to differentiate between service level errors and HTTP communication errors. WS-BD services MUSTpass-through the status codes underlying a particular request. In other words, services MUST NOTuse (or otherwise ‘piggyback’) HTTP status codes to indicate failures that occur within the service. If a service successfully receives a well-formed request, then the service MUSTreturn the HTTP status code 200 indicating such. Failures are described within the contents of the XML data returned to the client for any given operation. The exception to this is when the service receives a poorly-formed request (i.e., the XML payload is not valid), then the service *may* return the HTTP status code 400, indicating a bad request.

This is deliberately different from REST services that override HTTP status codes to provide service-specific error messages. Avoiding the overloading of status codes is a pattern that facilitates the debugging and troubleshooting of communication versus client & service failures.

Design Note: Overriding HTTP status codes is just one example of the rich set of features afforded by HTTP; content negotiation, entity tags (e-tags), and preconditions are other features that could be leveraged instead of “recreated” (to some degree) within this document. However, the authors avoided the use of these advanced HTTP features for several reasons:

* To reduce the overall complexity required for implementation.
* To ease the requirements on clients and servers (particularly since the HTTP capabilities on embedded systems may be limited).
* To avoid dependencies on any HTTP feature that is not required (such as entity tags).

In summary, the goal for this initial version of the specification is to provide common functionality across the broadest set of platforms. As this standard evolves, the authors will continue to evaluate the integration of more advanced HTTP features, as well as welcome feedback on their use from users and/or implementers of the specification.

### Client Identity

Before discussing how WS-BD balances single-user vs. multi-user needs, it is necessary to understand the WS-BD model for how an individual client can easily and consistently identify itself to a service.

HTTP is, by design, a *stateless* protocol. Therefore, any persistence about the originator of a sequence of requests MUSTbe built in artificially to the layer of abstraction above HTTP itself. This is accomplished in WS-BD via a *session*—a collection of operations that originate from the same logical endpoint. To initiate a session, a client performs a *registration* operation and obtains a *session identifier* (or “session id”). During subsequent operations, a client uses this identifier as a parameter to uniquely identify itself to a server. When the client is finished, it is expected to close a session with an *unregistration* operation. To conserve resources, services *may* automatically unregister clients that do not explicitly unregister after a period of inactivity (see §6.4.2.1).

This use of a session id directly implies that the particular sequences that constitute a session are entirely the responsibility of the *client*. A client might opt to create a single session for its entire lifetime, or, might open (and close) a session for a limited sequence of operations. WS-BD supports both scenarios.

It is possible, but discouraged, to implement a client with multiple sessions with the same service simultaneously. For simplicity, and unless otherwise stated, this specification is written in a manner that assumes that a single client maintains a single session id. (This can be assumed without loss of generality, since a client with multiple sessions to a service could be decomposed into “sub-clients”—one sub- client per session id.)

Just as a client might maintain multiple session ids, a single session id might be shared among a collection of clients. By sharing the session id, a biometric sensor may then be put in a particular state by one client, and then handed-off to another client. This specification does not provide guidance on how to perform multi-client collaboration. However, session id sharing is certainly permitted, and a deliberate artifact of the convention of using the session id as the client identifier. Likewise, many-to-many relationships (i.e., multiple session ids being shared among multiple clients) are also possible, but SHOULD be avoided.

### Sensor Identity

In general, implementers SHOULDmap each target biometric sensor to a single endpoint (URI). However, just as it is possible for a client to communicate with multiple services, a host might be responsible for controlling multiple target biometric sensors.

Independent sensors SHOULD be exposed via different URIs.

Example: Figure 4 shows a physically separate implementation where a single host machine controls two biometric sensors—one fingerprint scanner and one digital camera. The devices act independently and are therefore exposed via two different services—one at the URL *http://wsbd/fingerprint* and one at http://wsbd/camera.



**Figure 4**. Independent sensors controlled by separate services

A service that controls multiple biometric devices simultaneously (e.g., an array of cameras with synchronized capture) SHOULD be exposed via the same endpoint.



**Figure 5**. A sensor array controlled by a single service

Example: Figure 5 shows a physically separate implementation where a single host machine controls a pair of cameras used for stereo vision. The cameras act together as a single logical sensor and are both exposed via the same service, http://wsbd/camera\_array.

### Locking

WS-BD uses a *lock* to satisfy two complementary requirements:

1. A service MUSThave exclusive, sovereign control over biometric sensor hardware to perform a particular *sensor operation* such as initialization, configuration, or capture.
2. A client needs to perform an uninterrupted sequence of sensor operations.

Each WS-BD service exposes a *single* lock (one per service) that controls access to the sensor*.* Clients obtain the lock in order to perform a sequence of operations that SHOULD NOT be interrupted. Obtaining the lock is an indication to the server (and indirectly to peer clients) that (1) a series of sensor operations is about to be initiated and (2) that server *may* assume sovereign control of the biometric sensor.

A client releases the lock upon completion of its sequence of tasks. This indicates to the server (and indirectly to peer clients) that the uninterruptable sequence of operations is finished. A client might obtain and release the lock many times within the same session or a client might open and close a session for each pair of lock/unlock operations. This decision is entirely dependent on a particular client.

The statement that a client might “own” or “hold” a lock is a convenient simplification that makes it easier to understand the client-server interaction. In reality, each sensor service maintains a unique global variable that contains a session id. The originator of that session id can be thought of as the client that “holds” the lock to the service. Clients are expected to release the lock after completing their required sensor operations, but there is lock *stealing—*a mechanism for forcefully releasing locks. This feature is necessary to ensure that one client cannot hold a lock indefinitely, denying its peers access to the biometric sensor.

As stated previously (see §2.4.3), it is implied that all successfully connected clients enjoy the same access privileges. Each client is treated the same and are expected to work cooperatively with each other. This is critically important, because it is this implied equivalence of “trust” that affords a lock *stealing* operation.

Design Note: In the early development states of this specification, the authors considered having a single, atomic sensor operation that performed initialization, configuration *and* capture. This would avoid the need for locks entirely, since a client could then be ensured (if successful), the desired operation completed as requested. However, given the high degree of variability of sensor operations across different sensors and modalities, the explicit locking was selected so that clients could have a higher degree of control over a service and a more reliable way to predict timing. Regardless of the enforcement mechanism, it is undesirable if once a “well-behaved” client started an operation and a “rogue” client changed the internal state of the sensor midstream.

#### Pending Operations

Changing the state of the lock MUSThave no effect on pending (i.e., currently running) sensor operations. That is, a client *may* unlock, steal, or even re-obtain the service lock even if the target biometric sensor is busy. When lock ownership is transferred during a sensor operation, overlapping sensor operations are prevented by sensor operations returning sensorBusy.

### Operations Summary

All WS-BD operations fall into one of eight categories:

1. Registration
2. Locking
3. Information
4. Initialization
5. Configuration
6. Capture
7. Download
8. Cancellation

Of these, the initialization, configuration, capture, and cancellation operations are all sensor operations (i.e., they require exclusive sensor control) and require locking. Registration, locking, and download are all non-sensor operations. They do not require locking and (as stated earlier) MUSTbe available to clients regardless of the status of the biometric sensor.

*Download* is not a sensor operation. This allows for a collection of clients to dynamically share acquired biometric data. One client might perform the capture and hand off the download responsibility to a peer.

The following is a brief summary of each type of operation:

* *Registration* operations open and close (unregister) a session.
* *Locking* operations are used by a client to obtain the lock, release the lock, and *steal* the lock.
* *Information* operations query the service for information about the service itself, such as the supported biometric modalities, and service configuration parameters.
* The *initialization* operation prepares the biometric sensor for operation.
* *Configuration* operations get or set sensor parameters.
* The *capture* operation signals to the sensor to acquire a biometric.
* *Download* operations transfer the captured biometric data from the service to the client.
* Sensor operations can be stopped by the *cancellation* operation.

### Idempotency

The W3C Web Services glossary [WSGloss] defines idempotency as:

*[the] property of an interaction whose results and side-effects are the same whether it is done one or multiple times.*

When regarding an operation’s idempotence, it SHOULD be assumed no *other* operations occur in between successive operations, and that each operation is successful. Note that idempotent operations mayhave side-effects—but the final state of the service MUSTbe the same over multiple (uninterrupted) invocations.

The following example illustrates idempotency using an imaginary web service.

Example: A REST-based web service allows clients to create, read, update, and delete customer records from a database. A client executes an operation to update a customer’s address from “123 Main St” to “100 Broad Way.”

Suppose the operation is idempotent. Before the operation, the address is “123 Main St”. After one execution of the update, the server returns “success”, and the address is “100 Broad Way”. If the operation is executed a second time, the server again returns “success,” and the address remains “100 Broad Way”.

Now suppose that when the operation is executed a second time, instead of returning “success”, the server returns “no update made”, since the address was already “100 Broad Way.” Such an operation is *not* idempotent, because executing the operation a second time yielded a different result than the first execution.

The following is an example in the context of WS-BD.

Example: A service has an available lock. A client invokes the lock operation and obtains a “success” result. A subsequent invocation of the operation also returns a “success” result. The operation being idempotent means that the results (“success”) and side-effects (a locked service) of the two sequential operations are identical.

To best support robust communications, WS-BD is designed to offer idempotent services whenever possible.

### Service Lifecycle Behavior

The lifecycle of a service (i.e., when the service starts responding to requests, stops, or is otherwise unavailable) SHOULD be modeled after an integrated implementation. This is because it is significantly easier for a physically separated implementation to emulate the behavior of a fully integrated implementation than it is the other way around. This requirement has a direct effect on the expected behavior of how a physically separated service would handle a change in the target biometric sensor.

Specifically, on a desktop computer, hot-swapping the target biometric sensor is possible through an operating system’s plug-and-play architecture. By design, this specification does not assume that it is possible to replace a biometric sensor within an integrated device. Therefore, having a physically separated implementation emulate an integrated implementation provides a simple means of providing a common level of functionality.

By virtue of the stateless nature of the HTTP protocol, a client has no simple means of detecting if a web service has been restarted. For most web communications, a client SHOULD NOT require this—it is a core capability that constitutes the robustness of the web. Between successive web requests, a web server might be restarted on its host any number of times. In the case of WS-BD, replacing an integrated device with another (configured to respond on the same endpoint) is an *effective* restart of the service. Therefore, by the emulation requirement, replacing the device within a physically separated implementation SHOULD behave similarly.

A client may not be directly affected by a service restart, if the service is written in a robust manner. For example, upon detecting a new target biometric sensor, a robust server could *quiesce* (refusing all new requests until any pending requests are completed) and automatically restart.

Upon restarting, services SHOULD return to a fully reset state—i.e., all sessions SHOULD be dropped, and the lock SHOULD NOT have an owner. However, a high-availability service *may* have a mechanism to preserve state across restarts, but is significantly more complex to implement (particularly when using integrated implementations!). A client that communicated with a service that was restarted would lose both its session and the service lock (if held). With the exception of the get service info operation, through various fault statuses a client would receive indirect notification of a service restart. If needed, a client could use the service’s common info timestamp (§A.2.1) to detect potential changes in the get service info operation.

# Data Dictionary

This section contains descriptions of the data elements that are contained within the WS-BD data model. Each data type is described via an accompanying XML Schema type definition [XSDPart1, XSDPart2].

Refer to Appendix C for a complete XML schema containing all types defined in this document.

## Namespaces

The following namespaces, and corresponding namespace prefixes are used throughout this document.

|  |  |  |
| --- | --- | --- |
| **Prefix** | **Namespace** | **Remarks** |
| xs | http://www.w3.org/2001/XMLSchema | The xs namespace refers to the XML Schema specification. Definitions for the xs data types (i.e., those not explicitly defined here) can be found in [XSDPart2]. |
| xsi | http://www.w3.org/2001/XMLSchema-instance | The xsi namespace allows the schema to refer to other XML schemas in a qualified way. |
| wsbd | http://docs.oasis-open.org/bioserv/ns/wsbd-1.0 | The wsbd namespace is a uniform resource name [RFC1737, RFC2141] consisting of an object identifier [RFC3001] reserved for this specification’s schema. This namespace can be written in ASN.1 notation as {joint-iso-ccitt(2) country(16) us(840) organization(1) gov(101) csor(3) biometrics(9) wsbd(3) version1(1)}. |

All of the datatypes defined in this section (§3) belong to the wsbd namespace defined in the above table. If a datatype is described in the document without a namespace prefix, the wsbd prefix is assumed.

## UUID

A UUID is a unique identifier as defined in [RFC4122]. A service MUSTuse UUIDs that conform to the following XML Schema type definition.

<xs:simpleType name="UUID">

 <xs:restriction base="xs:string">

 <xs:pattern value="[\da-fA-F]{8}-[\da-fA-F]{4}-[\da-fA-F]{4}-[\da-fA-F]{4}-[\da-fA-F]{12}"/>

 </xs:restriction>

</xs:simpleType>

Example: Each of the following code fragments contains a well-formed UUID.

E47991C3-CA4F-406A-8167-53121C0237BA

10fa0553-9b59-4D9e-bbcd-8D209e8d6818

161FdBf5-047F-456a-8373-D5A410aE4595

## Dictionary

A Dictionary is a generic container used to hold an arbitrary collection of name-value pairs.

<xs:complexType name="Dictionary">

 <xs:sequence>

 <xs:element name="item" minOccurs="0" maxOccurs="unbounded">

 <xs:complexType>

 <xs:sequence>

 <xs:element name="key" type="xs:string" nillable="true"/>

 <xs:element name="value" type="xs:anyType" nillable="true"/>

 </xs:sequence>

 </xs:complexType>

 </xs:element>

 </xs:sequence>

</xs:complexType>

**EXAMPLE**: A query to get the metadata of a capture returns a dictionary of supported settings and the values at the time of capture.

<item>

 <key>imageWidth</key>

 <value>640</value>

</item>

<item>

 <key>imageHeight</key>

 <value>640</value>

</item>

<item>

 <key>captureDate</key>

 <value>2011-01-01T01:23:45Z</value>

</item>

Dictionary instances are nestable—i.e., the value element of one Dictionary can contain another Dictionary. The use of xs:anyType allows for an XML element of any structure or definition to be used. Using types not defined in this document or types defined in W3’s XML Schema recommendations [**XSDPart1, XSDPart2**] might require a client to have unique knowledge about the service. Because the requirement of unique knowledge negatively impacts interoperability, using such elements is discouraged.

## Parameter

A Parameter is a container used to describe the parameters or settings of a service or sensor.

<xs:complexType name="Parameter">

 <xs:sequence>

 <xs:element name="name" type="xs:string" nillable="true"/>

 <xs:element name="type" type="xs:QName" nillable="true"/>

 <xs:element name="readOnly" type="xs:boolean" minOccurs="0"/>

 <xs:element name="supportsMultiple" type="xs:boolean" minOccurs="0"/>

 <xs:element name="defaultValue" type="xs:anyType" nillable="true"/>

 <xs:element name="allowedValues" nillable="true" minOccurs="0">

 <xs:complexType>

 <xs:sequence>

 <xs:element name="allowedValue" type="xs:anyType" nillable="true" minOccurs="0" maxOccurs="unbounded"/>

 </xs:sequence>

 </xs:complexType>

 </xs:element>

 </xs:sequence>

</xs:complexType>

See §4 for more information on metadata and the use of Parameter.

#### Element Summary

The following is a brief informative description of each Parameter element.

|  |  |
| --- | --- |
| **Element** | **Description** |
| name | The name of the parameter. |
| type | The fully qualified type of the parameter. |
| readOnly | Whether or not this parameter is read-only. |
| **supportsMultiple** | Whether or not this parameter can support multiple values for this parameter (§3.4.1.2). |
| defaultValue | The default value of this parameter. |
| allowedValues | A list of allowed values for this parameter (§3.4.1.3). |

#### Supports Multiple

In some cases, a parameter might require multiple values. This flag specifies whether the parameter is capable of multiple values.

When supportsMultiple is true, communicating values MUST be done through a defined array type. If a type-specialized array is defined in this document, such as a StringArray (§3.7) for xs:string, such type SHOULD be used. The generic Array (§3.6) type MUSTbe used in all other cases.

The parameter’s type element MUSTbe the qualified name of a single value. For example, if the parameter expects multiple strings during configuration, then the type MUSTbe xs:string and not StringArray.

Example: An iris scanner might have the ability to capture a left iris, right iris, and/or frontal face image simultaneously. This example configures the scanner to capture left and right iris images together. The first code block is what the service exposes to the clients. The second code block is how a client would configure this parameter. The client configures the submodality by supplying a StringArray with two elements: left and right—this tells the service to capture both the left and right iris. It is important to note that in this example, submodality exposes values for two modalities: iris and face. The resulting captured data MUSTspecify the respective modality for each captured item in its metadata.

<name>submodality</name>

<type>xs:string</type>

<readOnly>false</readOnly>

<supportsMultiple>true</supportsMultiple>

<defaultValue xsi:type="wsbd:StringArray">

 <element>leftIris</element>

 <element>rightIris</element>

</defaultValue>

<allowedValues>

 <allowedValue>leftIris</allowedValue>

 <allowedValue>rightIris</allowedValue>

 <allowedValue>frontalFace</allowedValue>

</allowedValues>

<item>

 <key>submodality</key>

 <value xsi:type="wsbd:StringArray">

 <element>leftIris</element>

 <element>rightIris</element>

 </value>

</item>

#### Allowed Values

For parameters that are not read-only and have restrictions on what values it may have, this allows the service to dynamically expose its valid values to clients.

Example: The following code block demonstrates a parameter, “CameraFlash”, with only three valid values.

<name>cameraFlash</name>

<type>xs:string</type>

<readOnly>false</readOnly>

<supportsMultiple>false</supportsMultiple>

<defaultValue>auto</defaultValue>

<allowedValues>

 <allowedValue xsi:type="xs:string">on</allowedValue>

 <allowedValue xsi:type="xs:string">off</allowedValue>

 <allowedValue xsi:type="xs:string">auto</allowedValue>

</allowedValues>

Parameters requiring a range of values SHOULD be described by using Range (§3.5). Because the allowed type is not the same as its parameter type, a service MUSThave logic to check for a Range and any appropriate validation.

Example: The following code block demonstrates a parameter, “CameraZoom”, where the allowed value is of type Range and consists of integers.

<name>cameraZoom</name>

<type>xs:integer</type>

<readOnly>false</readOnly>

<supportsMultiple>false</supportsMultiple>

<defaultValue>0</defaultValue>

<allowedValues>

 <allowedValue xsi:type="wsbd:Range">

 <minimum>0</minimum>

 <maximum>100</maximum>

 </allowedValue>

</allowedValues>

Configurable parameters with no restrictions on its value MUST NOTinclude this element.

## Range

The Range element is a container for elements that define a range and whether its upper and lower bounds are exclusive. Bounds by default are inclusive.

<xs:complexType name="Range">

 <xs:sequence>

 <xs:element name="minimum" type="xs:anyType" nillable="true" minOccurs="0"/>

 <xs:element name="maximum" type="xs:anyType" nillable="true" minOccurs="0"/>

 <xs:element name="minimumIsExclusive" type="xs:boolean" nillable="true" minOccurs="0"/>

 <xs:element name="maximumIsExclusive" type="xs:boolean" nillable="true" minOccurs="0"/>

 </xs:sequence>

</xs:complexType>

Example: An example range of numbers from 0 to 100. The minimum is exclusive while the maximum is inclusive.

 <minimum>0</minimum>

 <maximum>100</maximum>

 <minimumIsExclusive>true</minimumIsExclusive>

 <maximumIsExclusive>false</maximumIsExclusive>

#### Element Summary

The following is a brief informative description of each Range element.

|  |  |
| --- | --- |
| **Element** | **Description** |
| minimum | The lower bound of the range. |
| maximum | The upper bound of the range. |
| minimumIsExclusive | Boolean indicating whether the lower bound is exclusive or not. This is true by default. |
| **maximumIsExclusive** | Boolean indicating whether the upper bound is exclusive or not. This is true by default. |

## Array

An Array is a generic container used to hold a collection of elements.

<xs:complexType name="Array">

 <xs:sequence>

 <xs:element name="element" type="xs:anyType" nillable="true" minOccurs="0" maxOccurs="unbounded"/>

 </xs:sequence>

</xs:complexType>

Example: Each of the following code fragments is an example of a valid Array.

<element>flatLeftThumb</element><element>flatRightThumb</element>

In this fragment (above), the values “flatLeftThumb” and “flatRightThumb” are of type xs:anyType, (and are likely to be deserialized as a generic “object.”

<element xsi:type="xs:boolean">false</element><element xsi:type="xs:int">1024</element>

Notice that in this fragment (above) the two values are of *different* types

<element xsi:type="xs:decimal">2.0</element>

In this fragment (above) the array contains a single element.

## StringArray

A StringArray is a generic container used to hold a collection of strings.

<xs:complexType name="StringArray">

 <xs:sequence>

 <xs:element name="element" type="xs:string" nillable="true" minOccurs="0" maxOccurs="unbounded"/>

 </xs:sequence>

</xs:complexType>

Example: Each of the following code fragments is an example of a valid StringArray.

<element>flatLeftThumb</element><element>flatRightThumb</element>

<element>value1</element><element>value2</element>

<element>sessionId</element>

## UuidArray

A UuidArray is a generic container used to hold a collection of UUIDs.

<xs:complexType name="UuidArray">

 <xs:sequence>

 <xs:element name="element" type="wsbd:UUID" nillable="true" minOccurs="0" maxOccurs="unbounded"/>

 </xs:sequence>

</xs:complexType>

Example: The following code fragment is an example of a *single* UuidArray with three elements.

<element>E47991C3-CA4F-406A-8167-53121C0237BA</element>

<element>10fa0553-9b59-4D9e-bbcd-8D209e8d6818</element>

<element>161FdBf5-047F-456a-8373-D5A410aE4595</element>

## ResourceArray

A ResourceArray is a generic container used to hold a collection of Resources (§3.10).

<xs:complexType name="ResourceArray">

 <xs:sequence>

 <xs:element name="element" type="wsbd:Resource" nillable="true" minOccurs="0" maxOccurs="unbounded"/>

 </xs:sequence>

</xs:complexType>

EXAMPLE: The following code fragment is an example of a *single* ResourceArray with two elements.

<element><uri>file:///tmp/test.png<uri><contentType>image/png</contentType></element>

<element><uri>http://192.168.1.1/robots.txt<uri><contentType>text/plain</contentType></element>

## Resource

Resource is a container to describe a resource at a specified URI.

<xs:complexType name="Resource">

 <xs:sequence>

 <xs:element name="uri" type="xs:anyURI"/>

 <xs:element name="contentType" type="xs:string" nillable="true" minOccurs="0"/>

 <xs:element name="relationship" type="xs:string" nillable="true" minOccurs="0"/>

 </xs:sequence>

</xs:complexType>

## Resolution

Resolution is a generic container to describe values for a width and height and optionally a description of the unit.

<xs:complexType name="Resolution">

 <xs:sequence>

 <xs:element name="width" type="xs:decimal"/>

 <xs:element name="height" type="xs:decimal"/>

 <xs:element name="unit" type="xs:string" nillable="true" minOccurs="0"/>

 </xs:sequence>

</xs:complexType>

#### Element Summary

The following is a brief informative description of each Size element.

|  |  |
| --- | --- |
| **Element** | **Description** |
| width | The decimal value of the width |
| height | The decimal value of the height |
| unit | A string describing the units of the width and height values |

## Status

The Status represents a common enumeration for communicating state information about a service.

<xs:simpleType name="Status">

 <xs:restriction base="xs:string">

 <xs:enumeration value="success"/>

 <xs:enumeration value="failure"/>

 <xs:enumeration value="preparingDownload"/>

 <xs:enumeration value="configurationNeeded"/>

 <xs:enumeration value="initializationNeeded"/>

 <xs:enumeration value="sensorTimeout"/>

 <xs:enumeration value="sensorFailure"/>

 <xs:enumeration value="sensorBusy"/>

 <xs:enumeration value="lockNotHeld"/>

 <xs:enumeration value="lockHeldByAnother"/>

 <xs:enumeration value="canceled"/>

 <xs:enumeration value="canceledWithSensorFailure"/>

 <xs:enumeration value="unsupported"/>

 <xs:enumeration value="badValue"/>

 <xs:enumeration value="noSuchParameter"/>

 <xs:enumeration value="invalidId"/>

 </xs:restriction>

</xs:simpleType>

#### Definitions

The following table defines all of the potential values for the Status enumeration.

|  |  |
| --- | --- |
| **Value** | **Description** |
| *success* | The operation completed successfully. |
| *failure* | The operation failed. The failure was due to a web service (as opposed to a sensor error). |
| *preparingDownload* | The operation could not be performed because the service is currently preparing captured data for download. (See §6.16.2.2) |
| *configurationNeeded* | The operation could not be performed because the sensor requires configuration. |
| *initializationNeeded* | The operation could not be performed because the sensor requires initialization. |
| *sensorTimeout* | The operation was not performed because the biometric sensor experienced a timeout.Note: The most common cause of a sensor timeout would be a lack of interaction with a sensor within an expected timeframe.  |
| *sensorFailure* | The operation could not be performed because of a biometric sensor (as opposed to web service) failure. Note: Clients that receive a status of sensorFailure SHOULD assume that the sensor will need to be reinitialized in order to restore normal operation.  |
| *sensorBusy* | The operation could not be performed because the sensor is currently performing another task.Note: Services *may* self-initiate an activity that triggers a sensorBusy result. That is, it may not be possible for a client to trace back a sensorBusy status to any particular operation. An automated self-check, heartbeat, or other activity such as a data transfer *may* place the target biometric sensor into a “busy” mode. (See §6.16.2.2 for information about post-acquisition processing.) |
| *lockNotHeld* | The operation could not be performed because the client does not hold the lock. Note: This status implies that at the time the lock was queried, no other client currently held the lock. However, this is not a guarantee that any subsequent attempts to obtain the lock will succeed. |
| *lockHeldByAnother* | The operation could not be performed because another client currently holds the lock. |
| *canceled* | The operation was canceled.**NOTE**: A sensor service *may* cancel its own operation, for example, if an operation is taking too long. This can happen if a service maintains its own internal timeout that is shorter than a sensor timeout. |
| *canceledWithSensorFailure* | The operation was canceled, but during (and perhaps because of) cancellation, a sensor failure occurred.This particular status accommodates for hardware that may not natively support cancellation.  |
| *unsupported* | The service does not support the requested operation. (See §6.1.2 for information on parameter failures.) |
| *badValue* | The operation could not be performed because a value provided for a particular parameter was either (a) an incompatible type or (b) outside of an acceptable range. (See §6.1.2 for information on parameter failures.) |
| *noSuchParameter* | The operation could not be performed because the service did not recognize the name of a provided parameter. (See §6.1.2 for information on parameter failures.) |
| *invalidId* | The provided id is not valid. This can occur if the client provides a (session or capture) id that is either:unknown to the server (i.e., does not correspond to a known registration or capture result), orthe session has been closed by the service (§6.4.2.1)(See §6.1.2 for information on parameter failures.) |

Many of the permitted status values have been designed specifically to support physically separate implementations—a scenario where it is easier to distinguish between failures in the web service and failures in the biometric sensor. This is not to say that within an integrated implementation such a distinction is not possible, only that some of the status values are more relevant for physically separate versions.

For example, a robust service would allow all sensor operations to be canceled with no threat of a failure. Unfortunately, not all commercial, off-the-shelf (COTS) sensors natively support cancellation. Therefore, the *canceledWithSensorFailure* status is offered to accommodate this. Implementers can still offer cancellation, but have a mechanism to communicate back to the client that sensor initialization might be required.

## SensorStatus

The SensorStatus represents a common enumeration for communicating state information about a sensor.

<xs:simpleType name="SensorStatus">

 <xs:restriction base="xs:string">

 <xs:enumeration value="ready"/>

 <xs:enumeration value="initializing"/>

 <xs:enumeration value="configuring"/>

 <xs:enumeration value="capturing"/>

 <xs:enumeration value="uninitializing"/>

 <xs:enumeration value="canceling"/>

 </xs:restriction>

</xs:simpleType>

#### Definitions

The following table defines all of the potential values for the Status enumeration.

|  |  |
| --- | --- |
| **Value** | **Description** |
| *ready* | The sensor is ready to start a new operation. |
| *initializing* | The sensor is initializing. |
| *configuring* | The sensor is configuring. |
| *capturing* | The sensor is capturing. |
| *uninitializing* | The sensor is uninitializing.  |
| *canceling* | The sensor is canceling an operation.  |

## Result

Unless a service returns with an HTTP error, all WS-BD operations MUSTreply with an HTTP message that contains an element of a Result type that conforms to the following XML Schema snippet.

<xs:element name="result" type="wsbd:Result" nillable="true"/>

<xs:complexType name="Result">

 <xs:sequence>

 <xs:element name="status" type="wsbd:Status"/>

 <xs:element name="badFields" type="wsbd:StringArray" nillable="true" minOccurs="0"/>

 <xs:element name="captureIds" type="wsbd:UuidArray" nillable="true" minOccurs="0"/>

 <xs:element name="metadata" type="wsbd:Dictionary" nillable="true" minOccurs="0"/>

 <xs:element name="message" type="xs:string" nillable="true" minOccurs="0"/>

 <xs:element name="sensorData" type="xs:base64Binary" nillable="true" minOccurs="0"/>

 <xs:element name="sessionId" type="wsbd:UUID" nillable="true" minOccurs="0"/>

 </xs:sequence>

</xs:complexType>

### Terminology Shorthand

Since a Result is the intended outcome of all requests, this document *may* state that an operation “returns” a particular status value. This is shorthand for a Result output payload with a status element containing that value.

Example: The following result payload “returns success”. A result might contain other child elements depending on the specific operation and result status—see §6 for operations and their respective details.

<result xmlns="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0"

 xmlns:xs="http://www.w3.org/2001/XMLSchema"

 xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">

 <status>success</status>

</result>

Likewise, the same shorthand is implied by a client “receiving” a status, or an operation “yielding” a status.

### Required Elements

Notice that from a XML Schema validation perspective [XSDPart1], a schema-valid Result MUSTcontain a status element, and may contain any of the remaining elements.

The specific permitted elements of a Result are determined via a combination of (a) the operation, and (b) the result’s status. That is, different operations will have different requirements on which elements are permitted or forbidden, depending on that operation’s status.

Example: As will be detailed later (§6.3.4.1 and §6.5.4.1), a register operation returning a status of success MUSTalso populate the sessionId element. However, a try lock operation that returns a status of success cannot populate any element other than status.

Design note: An XML inheritance hierarchy could have been used to help enforce which elements are permitted under which circumstances. However, a de-normalized representation (in which all of the possible elements are valid with respect to a *schema*) was used to simplify client and server implementation. Further, this reduces the burden of managing an object hierarchy for the sake of enforcing simple constraints.

### Element Summary

The following is a brief informative description of each Result element.

|  |  |
| --- | --- |
| **Element** | **Description** |
| status | The disposition of the operation. All Result elements MUSTcontain a status element. (Used in all operations.) |
| badFields | The list of fields that contain invalid or ill-formed values. (Used in almost all operations.) |
| captureIds | Identifiers that *may* be used to obtain data acquired from a capture operation (§6.13, §6.14, §6.15). |
| metadata | This field *may* hold1. metadata for the service (§6.8), or
2. a service and sensor’s configuration (§6.11, §6.12), or
3. metadata relating to a particular capture (§6.12.4.14, §6.14, §6.15, §6.16, §6.17, §6.18)

(See §4 for more information regarding metadata) |
| message | A string providing *informative* detail regarding the output of an operation. (Used in almost all operations.) |
| sensorData | The biometric data corresponding to a particular capture identifier (§6.14, §6.16, §6.18, §6.19). |
| sessionId | A unique session identifier (§6.3). |

## Validation

The provided XML schemas MAY be used for initial XML validation. It should be noted that these are not strict schema definitions and were designed for easy consumption of web service/code generation tools. Additional logic SHOULD be used to evaluate the contents and validity of the data where the schema falls short. For example, additional logic will be necessary to verify the contents of a Result are accurate as there is not a different schema definition for every combination of optional and mandatory fields.

A service MUSThave separate logic validating parameters and their values during configuration. The type of any allowed values might not correspond with the type of the parameter. For example, if the type of the parameter is an integer and an allowed value is a Range, the service MUSThandle this within the service as it may not be appropriately validated using XML schema.

# Metadata

Metadata can be broken down into three smaller categories: service information, sensor information or configuration, and capture information. Metadata can be returned in two forms: as a key/value pair within a Dictionary or a Dictionary of Parameter types.

## Service Information

Service information includes read-only parameters unrelated to the sensor as well as parameters that can be set. Updating the values of a parameter SHOULD be done in the set configuration operation.

Service information consists of the required parameters listed in Appendix A. Optional parameters SHOULD be included. Each parameter MUSTbe exposed as a Parameter (§3.4).

Parameters listed in §A.2, §A.3, and §A.4 MUSTbe exposed as read-only parameters.

Read-only parameters MUSTpopulate the default value field with its current value. Additionally, read-only parameters MUST NOTprovide allowed values. Allowed values are reserved to specify acceptable values which may be passed to the service to set configuration.

Example: An example snippet from a get service info call demonstrating a read-only parameter.

<name>inactivityTimeout</name>

<type>xs:nonNegativeInteger</type>

<readOnly>true</readOnly>

<supportsMultiple>false</supportsMultiple>

<defaultValue>600</defaultValue>

Configurable parameters, or those which are not read only, MUSTprovide information for the default value as well as allowed values. To specify that an allowed value is within range of numbers, refer to Range (§3.5).

Example: An example snippet from a get service info call. The target service supports a configurable parameter called “ImageWidth”.

<name>imageWidth</name>

<type>xs:positiveInteger</type>

<readOnly>false</readOnly>

<supportsMultiple>false</supportsMultiple>

<defaultValue>800</defaultValue>

<allowedValues>

 <allowedValue>640</allowedValue>

 <allowedValue>800</allowedValue>

 <allowedValue>1024</allowedValue>

</allowedValues>

In many cases, an exposed parameter will support multiple values (see §3.4.1.2). When a parameter allows this capability, it MUSTuse a type-specific array, defined in this document, or the generic Array (§3.6) type. The type element within a parameter MUSTbe the qualified name of a single value’s type (see §3.4.1.2 for an example).

## Configuration

A configuration consists of parameters specific to the sensor or post-processing related to the final capture result. This MUSTonly consist of key/value pairs. It MUST NOTinclude other information about the parameters, such as allowed values or read-only status.

Restrictions for each configuration parameter can be discovered through the get service info operation.

Example: The following is an example payload to set configuration consisting of three parameters.

<configuration xmlns="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0"

 xmlns:xs="http://www.w3.org/2001/XMLSchema"

 xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">

 <item>

 <key>imageHeight</key>

 <value xsi:type="xs:int">480</value>

 </item>

 <item>

 <key>imageWidth</key>

 <value xsi:type="xs:int">640</value>

 </item>

 <item>

 <key>frameRate</key>

 <value xsi:type="xs:int">20</value>

 </item>

</configuration>

## Captured Data

Metadata related to a particular capture operation MUSTinclude the configuration of the sensor at the time of capture. Static parameters related to the service SHOULD NOT be included in the metadata for a capture result.

A service MAY perform post-processing steps on any captured information. This information SHOULD be added to the particular capture result’s metadata.

Example: Example metadata for a particular capture. Note that this includes parameters related to the sensor.

<item>

 <key>serialNumber</key>

 <value xsi:type="xs:string">98A8N830LP332-V244</value>

</item>

<item>

 <key>imageHeight</key>

 <value xsi:type="xs:string">600</value>

</item>

<item>

 <key>imageWidth</key>

 <value xsi:type="xs:string">800</value>

</item>

<item>

 <key>captureTime</key>

 <value xsi:type="xs:dateTime">2011-12-02T09:39:10.935-05:00</value>

</item>

<item>

 <key>contentType</key>

 <value xsi:type="xs:string">image/jpeg</value>

</item>

<item>

 <key>modality</key>

 <value xsi:type="xs:string">Finger</value>

</item>

<item>

 <key>submodality</key>

 <value xsi:type="xs:string">LeftIndex</value>

</item>

Example: A service computes the quality score of a captured fingerprint (see previous example). This score is added to the result’s metadata to allow other clients to take advantage of previously completed processes.

<item>

 <key>quality</key>

 <value>78</value>

</item>

<item>

 <key>serialNumber</key>

 <value>98A8N830LP332-V244</value>

</item>

<item>

 <key>captureDate</key>

 <value>2011-01-01T15:30:00Z</value>

</item>

<item>

 <key>modality</key>

 <value>Finger</value>

</item>

<item>

 <key>submodality</key>

 <value>leftIndex</value>

</item>

<item>

 <key>imageHeight</key>

 <value>600</value>

</item>

<item>

 <key>imageWidth</key>

 <value>800</value>

</item>

<item>

 <key>contentType</key>

 <value>image/bmp</value>

</item>

### Minimal Metadata

At a minimum, a sensor or service *must* maintain the following metadata fields for each captured result. Two values are not provided by getConfiguration: captureDate and contentType--these values SHOULD be calculated at the time of capture.

#### Capture Date

|  |  |
| --- | --- |
| **Formal Name** | captureDate |
| **Data Type** | xs:dateTime [XSDPart2] |

This value represents the date and time at which the capture occurred.

#### Modality

|  |  |
| --- | --- |
| **Formal Name** | modality |
| **Data Type** | xs:string [XSDPart2] |

The value of this field MUSTbe present in the list of available modalities exposed by the get service info operation (§6.8) as defined in §A.1.1. This value represents the modality of the captured result.

#### Submodality

|  |  |
| --- | --- |
| **Formal Name** | submodality |
| **Data Type** | xs:anyType [XSDPart2] |

The value of this field MUSTbe present in the list of available submodalities exposed by the get service info operation (§6.8) as defined in §A.1.2. This value represents the submodality of the captured result. If this parameter supports multiple, then the data type MUSTbe a StringArray (§3.7) of values. If submodality does not support multiple, the data type MUSTbe xs:string [XSDPart2].

#### Content Type

|  |  |
| --- | --- |
| **Formal Name** | contentType |
| **Data Type** | xs:string [RFC2045, RFC2046] |

The value of this field represents the content type of the captured data. See A.2 for which content types are supported.

# Live Preview

The ability to provide live preview of a session provides feedback to the client on when to signal a capture and/or what is going on during a capture.

## Endpoints

Exposing endpoint information to a client is done through the service information. If live preview is implemented, a key/value pair SHALL be added where the key is “livePreview” and the value is of type Parameter (§3.4). This MUST be a read-only parameter. The default value SHALL be of type ResourceArray (§3.9). An implementation may expose one or more Resources (§3.10) in the ResourceArray. For the stream parameter, each instance of a Resource SHALL contain the uri, contentType, and the relationship elements. The content type of the stream and the value of each Resource’s contentType element SHOULD be listed in Appendix B. The value of the relationship field MUST begin with “livePreview” and there MUST be at least one entry where the element’s value consists of only “livePreview”. An implementer may provide additional endpoints with a modified relationship. This *may* be done by appending a forward slash immediately after “livePreview” and before any additional content; any additional content MUST *not* occur before the forward slash. Only base-64 characters are allowed in the relationship field.

The following snippet is a skeleton service information entry for a stream parameter.

<item>

 <key>livePreview</key>

 <value xsi:type=”Parameter”>

 <name>livePreview </name>

 <type>Resource</type>

 <readOnly>true</readOnly>

 <defaultValue xsi:type=”ResourceArray”>

 ...

 ...

 </defaultValue>

 </value>

</item>

Example: The following snippet is an example service information entry that exposes a Parameter (§3.4) for live preview resources. This example exposes two different endpoints, each offering a live preview with different content types.

<item>

 <key>livePreview</key>

 <value xsi:type=”Parameter”>

 <name>livePreview</name>

 <type>Resource</type>

 <readOnly>true</readOnly>

 <defaultValue xsi:type=”ResourceArray”>

 <element>

 <uri>http://192.168.1.1/stream</uri>

 <contentType>video/h264</contentType>

 <relationship>livePreview</relationship>

 </element>

 <element>

 <uri>http://192.168.1.1:81/stream</uri>

 <contentType>video/mpeg</contentType>

 <relationship>livePreview</relationship>

 </element>

 </defaultValue>

 </value>

</item>

Example: The following snippet is an example service information entry that exposes a Parameter (§3.4) for live preview resources. This example exposes two different endpoints, one with a modified relationship value. For example, the second entry *may* be describing an endpoint that has live preview of a face at 30 frames per second.

<item>

 <key>livePreview</key>

 <value xsi:type=”Parameter”>

 <name>livePreview</name>

 <type>Resource</type>

 <readOnly>true</readOnly>

 <defaultValue xsi:type=”ResourceArray”>

 <element>

 <uri>http://192.168.1.1/stream</uri>

 <contentType>video/h264</contentType>

 <relationship>livePreview</relationship>

 </element>

 <element>

 <uri>http://192.168.1.1:81/stream</uri>

 <contentType>video/mpeg</contentType>

 <relationship>livePreview/face+fps=30</relationship>

 </element>

 </defaultValue>

 </value>

</item>

A live preview end point *may* only return a single image representing the current frame at the time the operation was called. This SHALL be reflected in the value of the content type.

To increase the security and privacy of an implementation, a registered session id MAY be added to the URL(s) of end points.

## Heartbeat

In many cases, live preview may not be ready to provide actual images until a certain point in a session or the lifetime of a service (e.g., after initialization). The service has two options on how to proceed when streaming is called before it is ready.

1. Immediately close the live preview connection. This is only RECOMMENDED if live preview is not available for the service. It SHALL NOT be expected that a client will make additional calls to the live preview endpoint after a closed connection.
2. Send a heartbeat to the client upon a live preview request. The heartbeat SHALL consist of minimal null information and SHALL be sent to all clients on a fixed time interval.

Example: The follow is an example heartbeat frame sent over a multipart/x-mixed-replace stream. For this example, the boundary indicator is boundaryString. A service MAY send this null frame as a heartbeat to all connected clients every, for example, 10 seconds to alert the client that live preview data is available, but not at the current state of the service, sensor, or session.

--boundaryString

Content-Type: multipart/x-heartbeat

0

--boundaryString

# Operations

This section provides detailed information regarding each WS-BD operation.

## General Usage Notes

The following usage notes apply to all operations, unless the detailed documentation for a particular operation conflicts with these general notes, in which case the detailed documentation takes precedence.

1. Failure messages are informative. If an operation fails, then the message element MAY contain an informative message regarding the nature of that failure. The message is for informational purposes only—the functionality of a client MUST NOTdepend on the contents of the message.
2. Results MUST only contain required and optional elements. Services MUSTonlyreturn elements that are either required or optional. All other elements MUST NOTbe contained in the result, even if they are empty elements. Likewise, to maintain robustness in the face of a non-conformant service, clients SHOULD ignore any element that is not in the list of permitted Result elements for a particular operation call.
3. Sensor operations MUST NOT occur within a non-sensor operation. Services SHOULDonly perform any sensor control within the operations:
	1. initialize,
	2. get configuration,
	3. set configuration,
	4. capture, and
	5. cancel.
4. Sensor operations MUST require locking. Even if a service implements a sensor operation without controlling the target biometric sensor, the service MUST require that a locked service for the operation to be performed.
5. Content Type. Clients MUST make HTTP requests using a content type of application/xml [RFC2616, §14].
6. Namespace. A data type without an explicit namespace or namespace prefix implies it is a member of the wsbd namespace as defined in §3.1.

### Precedence of Status Enumerations

To maximize the amount of information given to a client when an error is obtained, and to prevent different implementations from exhibiting different behaviors, all WS-BD services MUST return status values according to a fixed priority. In other words, when multiple status messages might apply, a higher-priority status MUST always be returned in favor of a lower-priority status.

The status priority, listed from highest priority (“invalidId”) to lowest priority (“success”) is as follows:

1. invalidId
2. noSuchParameter
3. badValue
4. unsupported
5. canceledWithSensorFailure
6. canceled
7. lockHeldByAnother
8. lockNotHeld
9. sensorBusy
10. sensorFailure
11. sensorTimeout
12. initializationNeeded
13. configurationNeeded
14. preparingDownload
15. failure
16. success

Notice that success is the *lowest* priority—an operation SHOULD only be deemed successful if no *other* kinds of (non-successful) statuses apply.

The following example illustrates how this ordering affects the status returned in a situation in which multiple clients are performing operations.

EXAMPLE: Figure 6 illustrates that client a cannot receive a “sensorBusy” status if it does not hold the lock, even if a sensor operation is in progress (recall from §2.4.5 that sensor operations require holding the lock). Suppose there are two clients; Client A and Client B. Client A holds the lock and starts initialization on (Step 1–3). Immediately after Client A initiates capture, Client B (Step 4) tries to obtain the lock while Client A is still capturing. In this situation, the valid statuses that could be returned to Client B are “sensorBusy” (since the sensor is busy performing a capture) and “lockHeldByAnother” (since Client A holds the lock). In this case, the service returns “lockHeldByAnother” (Step 5) since “lockHeldByAnother” is higher priority than “sensorBusy.”



**Figure 6**. Example illustrating how a client cannot receive a "sensorBusy" status if it does not hold the lock.

### Parameter Failures

Services MUSTdistinguish among badValue, invalidId, noSuchParameter, and unsupported according to the following rules. These rules are presented here in the order of precedence that matches the previous subsection.

1. **Is a recognizable UUID provided?** If the operation requires a UUID as an input URL parameter, and the provided value is not an UUID (i.e., the UUID is *not* parseable), then the service MUSTreturn badValue. Additionally, the Result’s badFields list MUSTcontain the name of the offending parameter (sessionId or captureId).

*…otherwise…*

1. **Is the UUID understood?** If an operation requires an UUID as an input URL parameter, and the provided value *is* a UUID, but the service cannot accept the provided value, then the service MUSTreturn invalidId. Additionally, the Result’s badFields list MUSTcontain the name of the offending parameter (sessionId or captureId).

*…otherwise…*

1. **Are the parameter names understood?** If an operation does not recognize a provided input parameter *name*, then the service MUSTreturn noSuchParameter. This behavior may differ from service to service, as different services may recognize (or not recognize) different parameters. The unrecognized parameter(s) MUSTbe listed in the Result’s badFields list.

*…otherwise…*
2. **Are the parameter values acceptable?** If an operation recognizes all of the provided parameter names, but cannot accept a provided *value* because it is (a) and inappropriate type, or (b) outside the range advertised by the service (§4.1), the then service MUSTreturn badValue. The parameter names associated with the MUST values *must* be listed in the Result’s badFields list. Clients are expected to recover the bad values themselves by reconciling the Result corresponding to the offending request.

*…otherwise…*
3. **Is the request supported?** If an operation accepts the parameter names and values, but the particular request is not supported by the service or the target biometric sensor, then the service MUSTreturn unsupported. The parameter names that triggered this determination MUSTbe listed in the Result’s badFields list. By returning multiple fields, a service is able to imply that a particular *combination* of provided values is unsupported.

**NOTE**: It may be helpful to think of invalidId as a special case of badValue reserved for URL parameters of type UUID.

### Visual Summaries

The following two tables provide *informative* visual summaries of WS-BD operations. These visual summaries are an overview; they are not authoritative. (§6.3–§6.21 are authoritative.)

#### Input & Output

The following table represents a visual summary of the inputs and outputs corresponding to each operation.

Operation *inputs* are indicated in the “URL Fragment” and “Input Payload” columns. Operation inputs take the form of either (a) a URL parameter, with the parameter name shown in “curly brackets” (“{“ and “}”) within the URL fragment (first column), and/or, (b) a input payload (defined in §1.1).

Operation *outputs* are provided via Result, which is contained in the body of an operation’s HTTP response.

|  |
| --- |
| **Summary of Operations Input/Output** |
| **Operation** | **URL Fragment****(Includes inputs)** | **Method** | **Input****payload** | **Idempotent** | **Sensor Operation** | **Permitted Result Elements (within output payload)** | **Detailed Documentation (§)**  |
| **status** | **badFields** | **sessionId** | **metadata** | **captureIds** | **sensorData** |
| register | /register | POST | none |  |  | **** |  | **** |  |  |  | 6.3 |
| unregister | /register/{sessionId} | DELETE | none |  |  | **** | **** |  |  |  |  | 6.4 |
| try lock | /lock/{sessionId} | POST | none |  |  | **** | **** |  |  |  |  | 6.5 |
| steal lock | PUT | none |  |  | **** | **** |  |  |  |  | 6.6 |
| unlock | DELETE | none |  |  | **** | **** |  |  |  |  | 6.7 |
| get service info | /info | GET | none |  |  | **** |  |  | **** |  |  | 6.8 |
| initialize | /initialize/{sessionId} | POST | none |  |  | **** | **** |  |  |  |  | 6.9 |
| uninitialize | DELETE | none |  |  | **** | **** |  |  |  |  | 6.10 |
| get configuration | /configure/{sessionId} | GET | none |  |  | **** | **** |  | **** |  |  | 6.11 |
| set configuration | POST | config |  |  | **** | **** |  |  |  |  | 6.12 |
| capture | /capture/{sessionId} | POST | none |  |  | **** | **** |  |  | **** |  | 6.13 |
| begin capture | /capture/{sessionId}/async | POST | none |  |  | **** | **** |  |  |  |  | 6.14 |
| end capture | /capture/{sessionId}/async | PUT | none |  |  | **** | **** |  |  | **** |  | 6.15 |
| download | /download/{captureid} | GET | none |  |  | **** | **** |  | **** |  | **** | 6.16 |
| get download info | /download/{captureid}/info | GET | none |  |  |  |  |  | **** |  |  | 6.17 |
| thrifty download | /download/{captureid}/{maxSize} | GET | none |  |  | **** | **** |  | **** |  | **** | 6.18 |
| get sensor data | /download/{captureid}/raw | GET | none |  |  | **** |  |  |  |  | **** | 6.19 |
| cancel operation | /cancel/{sessionId} | POST | none |  |  | **** | **** |  |  |  |  | 6.20 |
| get sensor status | /status | GET | none |  |  | **** |  |  | **** |  |  | 6.21 |

Presence of a symbol in a table cell indicates that operation is idempotent (), a sensor operation (), and which elements may be present in the operation's Result (****). Likewise, the lack of a symbol in a table cell indicates the operation is not idempotent, not a sensor operation, and which elements of the operation's Result are forbidden.

Example: The capture operation (fifth row from the bottom) is not idempotent, but is a sensor operation. The output may contain the elements status, badFields, and/or captureIds in its Result. The detailed information regarding the Result for capture, (i.e., which elements are specifically permitted under what circumstances) is found in §6.13.

The message element is not shown in this table for two reasons. First, when it appears, it is *always* optional. Second, to emphasize that the message content is only to be used for informative purposes; it MUST NOTbe used as a vehicle for providing unique information that would inhibit a service’s interoperability.

#### Permitted Status Values

The following table provides a visual summary of the status values permitted.

|  |
| --- |
| **Possible Status Values Per Operation** |
| **Status****Values****Operation Description** | **success** | **failure** | **invalidId** | **canceled** | **canceledWithSensorFailure** | **sensorFailure** | **lockNotHeld** | **lockHeldByAnother** | **initializationNeeded** | **configurationNeeded** | **sensorBusy** | **sensorTimeout** | **unsupported** | **badValue** | **noSuchParameter** | **preparingDownload** |
| register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| unregister |  |  |  |  |  |  |  |  |  |  |  |  |  | **** |  |  |
| try lock |  |  |  |  |  |  |  | **** |  |  |  |  |  | **** |  |  |
| steal lock |  |  |  |  |  |  |  |  |  |  |  |  |  | **** |  |  |
| unlock |  |  |  |  |  |  |  | **** |  |  |  |  |  | **** |  |  |
| get service info |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| initialize |  |  |  | **** | **** | **** | **** | **** |  |  | **** | **** |  | **** |  |  |
| uninitialize |  |  |  | **** | **** | **** | **** | **** |  |  | **** | **** |  | **** |  |  |
| get configuration | **** | **** | **** | **** | **** | **** | **** | **** | **** | **** | **** | **** |  | **** |  |  |
| set configuration | **** | **** | **** | **** | **** | **** | **** | **** | **** |  | **** | **** | **** | **** | **** |  |
| capturebegin captureend capture |  |  |  | **** | **** | **** | **** | **** | **** | **** | **** | **** |  | **** |  |  |
| download |  |  |  |  |  |  |  |  |  |  |  |  |  | **** |  | **** |
| get download info |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| thrifty download |  |  |  |  |  |  |  |  |  |  |  |  | **** | **** |  | **** |
| get sensor data |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| cancel |  |  |  |  |  |  | **** | **** |  |  |  |  |  | **** |  |  |
| get sensor status |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

The presence (absence) of a symbol in a cell indicates that the respective status may (may not) be returned by the corresponding operation.

Example: The register operation may only return a Result with a Status that contains either success or failure. The unregister operation may only return success, failure, invalidId, sensorBusy, or badValue.

The visual summary does not imply that services may return these values arbitrarily—the services MUSTadhere to the behaviors as specified in their respective sections.

## Documentation Conventions

Each WS-BD operation is documented according to the following conventions.

### General Information

Each operation begins with the following tabular summary:

|  |  |
| --- | --- |
| **Description** | A short description of the operation |
| **URL Template** | The suffix used to access the operation. These take the form/resourceNameor/resourceName/{URL\_parameter\_1}/…/{URL\_parameter\_N}Each parameter, {URL\_parameter...} MUSTbe replaced, in-line with that parameter’s value. A single, optional parameter, [Optional\_parameter], is allowed. If present, it MUST be the last component of the URL. It MUST be either replaced, in-line with the parameter’s value or omitted from the URL.Parameters have no explicit names, other than defined by this document or reported back to the client within the contents of a badFields element.It is assumed that consumers of the service will prepend the URL to the service endpoint as appropriate.Example: The resource resourceName hosted at the endpointhttp://example.com/Servicewould be accessible viahttp://example.com/Service/resourceName |
| **HTTP Method**  | The HTTP method that triggers the operation, i.e., GET, POST, PUT, or DELETE |
| **URL Parameters** | A description of the URL-embedded operation parameters. For each parameter the following details are provided:* the name of the parameter
* the expected data type (§3)
* a description of the parameter
 |
| **Input Payload** | A description of the content, if any, to be posted to the service as input to an operation. |
| **Idempotent** | Yes—the operation is idempotent (§2.4.7).No—the operation is not idempotent. |
| **Sensor Operation (Lock Required)** | Yes—the service may require exclusive control over the target biometric sensor.No—this operation does not require a lock. Given the concurrency model (§2.4.5) this value doubles as documentation as to whether or not a lock is required |

### Result Summary

This subsection summarizes the various forms of a Result that may be returned by the operation. Each row represents a distinct combination of permitted values & elements associated with a particular status. An operation that returns success MAY also provide additional information other than status.

|  |  |
| --- | --- |
| success | status="success"  |
| failure | status="failure"message\*=informative message describing failure |
| [status value] | status=status literal[required element name]=description of permitted contents of the element[optional element name]\*=description of permitted contents of the element |

For each row, the left column contains a permitted status value, and the right column contains a summary of the constraints on the Result when the status element takes that specific value. The vertical ellipses at the bottom of the table signify that the summary table may have additional rows that summarize other permitted status values.

Data types without an explicit namespace or namespace prefix are members of the wsbd namespace as defined in §3.1.

Element names suffixed with a ‘\*’ indicate that the element is *optional*.

### Usage Notes

Each of the following subsections describes behaviors & requirements that are specific to its respective operation.

### Unique Knowledge

For each operation, there is a brief description of whether or not the operation affords an opportunity for the server or client to exchange information unique to a particular implementation. The term “unique knowledge” is used to reflect the definition of interoperability referenced in §2.1.

### Return Values Detail

This subsection details the various return values that the operation may return. For each permitted status value, the following table details the Result requirements:

|  |  |
| --- | --- |
| **Status Value** | The particular status value |
| **Condition** | The service accepts the registration request |
| **Required Elements** | A list of the required elements. For each required element, the element name, its expected contents, and expected data type is listed If no namespace prefix is specified, then the wsbd namespace (§3.1) is inferred.For example,  badFields={"sessionId"} (StringArray, §3.7)Indicates that badFields is a required element, and that the contents of the element MUSTbe a wsbd:StringArray containing the single literal "sessionId". |
| **Optional Elements** | A list of the required elements. Listed for each optional element are the element names and its expected contents. |

Constraints and information unique to the particular operation/status combination may follow the table, but some status values have no trailing explanatory text.

A data type without an explicit namespace or namespace prefix implies it is a member of the wsbd namespace as defined in §3.1.

## Register

|  |  |
| --- | --- |
| **Description** | Open a new client-server session |
| **URL Template** | /register |
| **HTTP Method**  | POST |
| **URL Parameters** | None |
| **Input Payload** | None |
| **Idempotent** | No |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"sessionId=session id (UUID, §3.2) |
| failure | status="failure"message\*=informative message describing failure |

### Usage Notes

Register provides a unique identifier that can be used to associate a particular client with a server.

In a sequence of operations with a service, a register operation is likely one of the first operations performed by a client (get service info being the other). It is expected (but not required) that a client would perform a single registration during that client’s lifetime.

Design Note: By using an UUID, as opposed to the source IP address, a server can distinguish among clients sharing the same originating IP address (i.e., multiple clients on a single machine, or multiple machines behind a firewall). Additionally, a UUID allows a client (or collection of clients) to determine client identity rather than enforcing a particular model (§2.4.3).

### Unique Knowledge

As specified, the register operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The register operation MUSTreturn a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service accepts the registration request |
| **Required Elements** | status (Status, §3.12)the literal “success”sessionId (UUID, §3.2)an identifier that can be used to identify a session |
| **Optional Elements** | None |

The “register” operation MUST NOT provide a sessionId of 00000000-0000-0000-0000-000000000000.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot accept the registration request |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Registration might fail if there are too many sessions already registered with a service. The message element SHALL only be used for informational purposes. Clients MUST NOT depend on particular contents of the message element to control client behavior.

See §4 and §A.2 for how a client can use sensor metadata to determine the maximum number of current sessions a service can support.

## Unregister

|  |  |
| --- | --- |
| **Description** | Close a client-server session |
| **URL Template** | /register/{sessionId} |
| **HTTP Method**  | DELETE |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session to remove |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| sensorBusy | status="sensorBusy" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

Unregister closes a client-server session. Although not strictly necessary, clients SHOULD unregister from a service when it is no longer needed. Given the lightweight nature of sessions, services SHOULD support (on the order of) thousands of concurrent sessions, but this cannot be guaranteed, particularly if the service is running within limited computational resources. Conversely, clients SHOULDassume that the number of concurrent sessions that a service can support is limited. (See §A.2 for details on connection metadata.)

#### Inactivity

A service MAY automatically unregister a client after a period of inactivity, or if demand on the service requires that least-recently used sessions be dropped. This is manifested by a client receiving a status of invalidId without a corresponding unregistration. Services SHALL set the inactivity timeout to a value specified in minutes. (See §A.2 for details on connection metadata.)

#### Sharing Session Ids

A session id is not a secret, but clients that share session ids run the risk of having their session prematurely terminated by a rogue peer client. This behavior is permitted, but discouraged. See §2.4 for more information about client identity and the assumed security models.

#### Locks & Pending Sensor Operations

If a client that holds the service lock unregisters, then a service MUSTalso release the service lock, with one exception. If the unregistering client both holds the lock and is responsible for a pending sensor operation, the service MUSTreturn sensorBusy (See §6.4.4.3).

### Unique Knowledge

As specified, the unregister operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The unregister operation MUSTreturn a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service accepted the unregistration request |
| **Required Elements** | status (Status, §3.12)the literal “success” |
| **Optional Elements** | None |

If the unregistering client currently holds the service lock, and the requesting client is not responsible for any pending sensor operation, then successful unregistration MUSTalso release the service lock.

As a consequence of idempotency, a session id does not need to ever have been registered successfully in order to *un*register successfully. Consequently, the unregister operation cannot return a status of invalidId.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service could not unregister the session. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

In practice, failure to unregister is expected to be a rare occurrence. Failure to unregister might occur if the service experiences a fault with an external system (such as a centralized database used to track session registration and unregistration)

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The service could not unregister the session because the biometric sensor is currently performing a sensor operation within the session being unregistered. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

This status MUST only be returned if (a) the sensor is busy and (b) the client making the request holds the lock (i.e., the session id provided matches that associated with the current service lock). Any client that does not hold the session lock MUST NOT result in a sensorBusy status.

Example: The following sequence diagram illustrates a client that cannot unregister (Client A) and a client that can unregister (Client B). After the initialize operation completes (Step 6), Client A can unregister (Steps 7-8).



**Figure 7**. Example of how an unregister operation can result in sensorBusy.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

## Try Lock

|  |  |
| --- | --- |
| **Description** | Try to obtain the service lock |
| **URL Template** | /lock/{sessionId} |
| **HTTP Method**  | POST |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting the service lock |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| lockHeldByAnother | status="lockHeldByAnother" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The try lock operation attempts to obtain the service lock. The word “try” is used to indicate that the call always returns immediately; it does not block until the lock is obtained. See §2.4.5 for detailed information about the WS-BD concurrency and locking model.

### Unique Knowledge

As specified, the try lock cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The try lock operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service was successfully locked to the provided session id. |
| **Required Elements** | status (Status, §3.12)the literal “success” |
| **Optional Elements** | None |

See §2.4.5 for detailed information about the WS-BD concurrency and locking model. Cancellation MUST have no effect on pending sensor operations (§6.6.2.3).

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service could not be locked to the provided session id. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST reserve a failure status to report system or internal failures and prevent the acquisition of the lock. Most try lock operations that do not succeed will not produce a failure status, but more likely a lockHeldByAnother status (See §6.5.4.3 for an example).

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The service could not be locked to the provided session id because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

Example: The following sequence diagram illustrates a client that cannot obtain the lock (Client B) because it is held by another client (Client A).



**Figure 8**. Example of a scenario yielding a lockHeldByAnother result.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Steal Lock

|  |  |
| --- | --- |
| **Description** | Forcibly obtain the lock away from a peer client |
| **URL Template** | /lock/{sessionId} |
| **HTTP Method**  | PUT |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting the service lock |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The steal lock operation allows a client to forcibly obtain the lock away from another client that already holds the lock. The purpose of this operation is to prevent a client that experiences a fatal error from forever preventing another client access to the service, and therefore, the biometric sensor.

#### Avoid Lock Stealing

Developers and integrators SHOULD endeavor to reserve lock stealing for exceptional circumstances—such as when a fatal error prevents a client from releasing a lock. Lock stealing SHOULD NOT be used as the primary mechanism in which peer clients coordinate biometric sensor use.

#### Lock Stealing Prevention Period (LSPP)

To assist in coordinating access among clients and to prevent excessive lock stealing, a service maytrigger a time period that forbids lock stealing for each sensor operation. For convenience, this period of time will be referred to as the *lock stealing prevention period (LSPP).*

During the LSPP, all attempts to steal the service lock will fail. Consequently, if a client experiences a fatal failure during a sensor operation, then all peer clients need to wait until the service re-enables lock stealing.

All services SHOULD implement a non-zero LSPP. The recommended time for the LSPP is on the order of 100 seconds. Services that enforce an LSPP MUST start the LSPP immediately before sovereign sensor control is required. Conversely, services SHOULD NOT enforce an LSPP unless absolutely necessary.

If a request provides an invalid sessionId, then the operation SHALL return an invalidId status instead of a failure regardless of the LSPP threshold and whether or not it has expired. A failure signifies that the state of the service is still within the LSPP threshold and the provided sessionId is valid.

A service MAY reinitiate a LSPP when an operation yields an undesirable result, such as failure. This would allow a client to attempt to resubmit the request or recover without worrying about whether or not the lock is still owned by the client’s session. When an operation yields a desirable result, the service SHOULD restart the LSPP. This would allow the client to call multiple successful operations without needing to worry about whether or not the lock is still owned by the client’s session.

An LSPP ends after a fixed amount of time has elapsed, unless another sensor operation restarts the LSPP. Services SHOULD keep the length of the LSPP fixed throughout the service’s lifecycle. It is recognized, however, that there may be use cases in which a variable LSPP timespan is desirable or required. Regardless, when determining the appropriate timespan, implementers shouldcarefully consider the tradeoffs between preventing excessive lock stealing, versus forcing all clients to wait until a service re-enables lock stealing.

#### Cancellation & (Lack of) Client Notification

Lock stealing MUSThave no effect on any currently running sensor operations. It is possible that a client initiates a sensor operation, has its lock stolen away, yet the operation completes successfully. *Subsequent* sensor operations would yield a lockNotHeld status, which a client could use to indicate that their lock was stolen away from them. Services SHOULDbe implemented such that the LSPP is longer than any sensor operation.

### Unique Knowledge

As specified, the steal lock operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The steal lock operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service was successfully locked to the provided session id. |
| **Required Elements** | status (Status, §3.12)the literal “success” |
| **Optional Elements** | None |

See §2.4.5 for detailed information about the WS-BD concurrency and locking model. Cancellation MUST have no effect on pending sensor operations (§6.6.2.3).

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service could not be locked to the provided session id. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Most steal lock operations that yield a failure status will do so because the service receives a lock stealing request during a lock stealing prevention period (§6.6.2.2). Services MUST also reserve a failure status for other non-LSPP failures that prevent the acquisition of the lock.

Implementers MAY choose to use the optional message field to provide more information to an end-user as to the specific reasons for the failure. However (as with all other failure status results), clients MUST NOT depend on any particular content to make this distinction.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Unlock

|  |  |
| --- | --- |
| **Description** | Release the service lock |
| **URL Template** | /lock/{sessionId} |
| **HTTP Method**  | DELETE |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session releasing the service lock |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| sensorBusy | status="sensorBusy" |
| lockHeldByAnother | status="lockHeldByAnother" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The unlock operation releases a service lock, making locking available to other clients.

See §2.4.5 for detailed information about the WS-BD concurrency and locking model.

### Unique Knowledge

As specified, the unlock operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The unlock operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service returned to an unlocked state. |
| **Required Elements** | status (Status, §3.12)the literal “success” |
| **Optional Elements** | None |

Upon releasing the lock, a client is no longer permitted to perform any sensor operations (§2.4.5). By idempotency (§2.4.7), if a client already has released the lock, subsequent unlock operations SHOULD also return success.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service could not be transitioned into an unlocked state. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST reserve a failure status to report system or internal failures and prevent the release of the service lock. The occurrence of unlock operations that fail is expected to be rare.

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The service could not unlock the session because the biometric sensor is currently performing a sensor operation within the session being unlocked. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

This status MUST only be returned if (a) the sensor is busy and (b) the client making the request holds the lock (i.e., the session id provided matches that associated with the current service lock). Any client that does not hold the session lock MUST NOT result in a sensorBusy status.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Get Service Info

|  |  |
| --- | --- |
| **Description** | Retrieve metadata about the service that does not depend on session-specific information, or sovereign control of the target biometric sensor |
| **URL Template** | /info |
| **HTTP Method**  | GET  |
| **URL Parameters** | None |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"metadata=dictionary containing service metadata (Dictionary, §3.3) |
| failure | status="failure"message\*=informative message describing failure |

### Usage Notes

The get service info operation provides information about the service and target biometric sensor. This operation MUST return information that is both (a) independent of session, and (b) does not require sovereign biometric sensor control. In other words, services MUST NOT control the target biometric sensor during a get service info operation itself. Implementations MAY (and are encouraged to) use service startup time to query the biometric sensor directly to create a cache of information and capabilities for get service info operations. The service should keep a cache of sensor and service metadata to reduce the amount of operations that query the sensor as this can be a lengthy operation.

The get service info operation does *not* require that a client be registered with the service. Unlike other operations, it does *not* take a session id as a URL parameter.

See §4.1 for information about the metadata returned from this operation.

Example: The following represents a ‘raw’ request to get the service’s metadata.

GET http://10.0.0.8:8000/Service/info HTTP/1.1

Content-Type: application/xml

Host: 10.0.0.8:8000

Example: The following is the ‘raw’ response from the above request. The metadata element of the result contains a Dictionary (§3.3) of parameter names and parameter information represented as a Parameter (§3.4).

HTTP/1.1 200 OK

Content-Length: 2931

Content-Type: application/xml; charset=utf-8

Server: Microsoft-HTTPAPI/2.0

Date: Tue, 03 Jan 2012 14:54:51 GMT

<result

 xmlns="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0"

 xmlns:xs="http://www.w3.org/2001/XMLSchema"

 xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">

 <status>success</status>

 <metadata>

 <item>

 <key>width</key>

 <value xsi:type="Parameter">

 <name>width</name>

 <type>xs:unsignedInt</type>

 <defaultValue xsi:type="xs:int">800</defaultValue>

 <allowedValues>

 <allowedValue xsi:type="xs:int">1280</allowedValue>

 <allowedValue xsi:type="xs:int">960</allowedValue>

 <allowedValue xsi:type="xs:int">800</allowedValue>

 <allowedValue xsi:type="xs:int">640</allowedValue>

 <allowedValue xsi:type="xs:int">424</allowedValue>

 <allowedValue xsi:type="xs:int">416</allowedValue>

 <allowedValue xsi:type="xs:int">352</allowedValue>

 <allowedValue xsi:type="xs:int">320</allowedValue>

 </allowedValues>

 </value>

 </item>

 <item>

 <key>height</key>

 <value xsi:type="Parameter">

 <name>height</name>

 <type>xs:unsignedInt</type>

 <defaultValue xsi:type="xs:int">600</defaultValue>

 <allowedValues>

 <allowedValue xsi:type="xs:int">720</allowedValue>

 <allowedValue xsi:type="xs:int">600</allowedValue>

 <allowedValue xsi:type="xs:int">544</allowedValue>

 <allowedValue xsi:type="xs:int">480</allowedValue>

 <allowedValue xsi:type="xs:int">448</allowedValue>

 <allowedValue xsi:type="xs:int">360</allowedValue>

 <allowedValue xsi:type="xs:int">288</allowedValue>

 <allowedValue xsi:type="xs:int">240</allowedValue>

 <allowedValue xsi:type="xs:int">144</allowedValue>

 <allowedValue xsi:type="xs:int">120</allowedValue>

 </allowedValues>

 </value>

 </item>

 <item>

 <key>frameRate</key>

 <value xsi:type="Parameter">

 <name>frameRate</name>

 <type>xs:unsignedInt</type>

 <defaultValue xsi:type="xs:int">30</defaultValue>

 <allowedValues>

 <allowedValue xsi:type="xs:int">30</allowedValue>

 <allowedValue xsi:type="xs:int">15</allowedValue>

 <allowedValue xsi:type="xs:int">10</allowedValue>

 </allowedValues>

 </value>

 </item>

 <item>

 <key>modality</key>

 <value xsi:type="Parameter">

 <name>modality</name>

 <type>xs:string</type>

 <readOnly>true</readOnly>

 <defaultValue xsi:type="xs:string">face</defaultValue>

 </value>

 </item>

 <item>

 <key>submodality</key>

 <value xsi:type="Parameter">

 <name>submodality</name>

 <type>xs:string</type>

 <readOnly>true</readOnly>

 <defaultValue xsi:type="xs:string">frontalFace</defaultValue>

 </value>

 </item>

 </metadata>

</result>

### Unique Knowledge

As specified, the get service info can be used to obtain knowledge about unique characteristics of a service. Through get service info, a service may expose implementation and/or service-specific configuration parameter names and values that are not defined in this document (see Appendix A for further information on parameters).

### Return Values Detail

The get service info operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service provides service metadata |
| **Required Elements** | status (Status, §3.12)the literal "success"metadata (Dictionary, §3.3)information about the service metadata |
| **Optional Elements** | None |

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot provide service metadata |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

## Initialize

|  |  |
| --- | --- |
| **Description** | Initialize the target biometric sensor |
| **URL Template** | /initialize/{sessionId} |
| **HTTP Method**  | POST  |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting initialization |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| sensorTimeout | status="sensorTimeout" |
| sensorFailure | status="sensorFailure" |
| sensorBusy | status="sensorBusy" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The initialize operation prepares the target biometric sensor for (other) sensor operations.

Some biometric sensors have no requirement for explicit initialization. In that case, the service SHOULD immediately return a success result.

Services SHOULD directly map this operation to the initialization of the target biometric sensor, unless the service can reliably determine that the target biometric sensor is in a fully operational state. In other words, a service may decide to immediately return success if there is a reliable way to detect if the target biometric sensor is currently in an initialized state. This style of “short circuit” evaluation could reduce initialization times. However, a service that always initializes the target biometric sensor would enable the ability of a client to attempt a manual reset of a sensor that has entered a faulty state. This is particularly useful in physically separated service implementations where the connection between the target biometric sensor and the web service host may be less reliable than an integrated implementation.

### Unique Knowledge

As specified, the initialize operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service successfully initialized the target biometric sensor |
| **Required Elements** | statusthe literal "success" |
| **Optional Elements** | None |

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service experienced a fault that prevented successful initialization. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A failure status MUST only be used to report failures that occurred within the web service, not within the target biometric sensor (§6.9.4.9, §6.9.4.4)

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | Initialization could not be performed because the target biometric sensor took too long to complete the initialization request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See A.2 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The initialization failed due to a failure within the target biometric sensor |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.9.4.2).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | Initialization could not be performed because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | Initialization could not be performed because the requesting client does not hold the lock |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | Initialization could not be performed because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The initialization operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The initialization operation was interrupted by a cancellation request and the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to reattempt the initialization request to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Uninitialize

|  |  |
| --- | --- |
| **Description** | Uninitiatize the target biometric sensor |
| **URL Template** | /initialize/{sessionId} |
| **HTTP Method**  | DELETE |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting initialization |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | Yes |

### Return Values Detail

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| sensorTimeout | status="sensorTimeout" |
| sensorFailure | status="sensorFailure" |
| sensorBusy | status="sensorBusy" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Note

The uninitialize operation closes connection to the target biometric sensor for (other) sensor operations.

Some biometric sensors have no requirement for explicit uninitialization. In that case, the service SHOULD immediately return a success result.

### Unique Knowledge

As specified, the uninitialize operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service

### Return Values Detail

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service successfully uninitialized the target biometric sensor |
| **Required Elements** | statusthe literal "success" |
| **Optional Elements** | None |

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service experienced a fault that prevented successful uninitialization. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A failure status MUST only be used to report failures that occurred within the web service, not within the target biometric sensor (§6.9.4.9, §6.9.4.4)

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | Uninitialization could not be performed because the target biometric sensor took too long to complete the uninitialization request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See A.2 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The uninitialization failed due to a failure within the target biometric sensor |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.9.4.2).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | Uninitialization could not be performed because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | Uninitialization could not be performed because the requesting client does not hold the lock |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | Uninitialization could not be performed because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The uninitialization operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The uninitialization operation was interrupted by a cancellation request and the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to reattempt the initialization request to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Get Configuration

|  |  |
| --- | --- |
| **Description** | Retrieve metadata about the target biometric sensor’s current configuration |
| **URL Template** | /configure/{sessionId} |
| **HTTP Method**  | GET  |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting the configuration |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"metadata=current configuration of the sensor (Dictionary, §3.3) |
| failure | status="failure"message\*=informative message describing failure |
| **configurationNeeded** | status="configurationNeeded" |
| **initializationNeeded** | status="initializationNeeded" |
| sensorTimeout | status="sensorTimeout" |
| sensorFailure | status="sensorFailure" |
| sensorBusy | status="sensorBusy" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The get configuration operation retrieves the service’s current configuration.

Example: The following represents a ‘raw’ request to retrieve the current configuration information of the service.

GET http://10.0.0.8:8000/Service/configure/d745cd19-facd-4f91-8774-aac5ca9766a2 HTTP/1.1

Content-Type: application/xml

Host: 10.0.0.8:8000

Example: The following is the ‘raw’ response from the previous request. The metadata element in the result contains a Dictionary (§3.3) of parameter names and their respective values.

HTTP/1.1 200 OK

Content-Length: 554

Content-Type: application/xml; charset=utf-8

Server: Microsoft-HTTPAPI/2.0

Date: Tue, 03 Jan 2012 14:57:29 GMT

<result xmlns="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0"

 xmlns:i="http://www.w3.org/2001/XMLSchema-instance">

 <status>success</status>

 <metadata>

 <item>

 <key>width</key>

 <value i:type="a:int" xmlns:a="http://www.w3.org/2001/XMLSchema">800</value>

 </item>

 <item>

 <key>height</key>

 <value i:type="a:int" xmlns:a="http://www.w3.org/2001/XMLSchema">600</value>

 </item>

 <item>

 <key>frameRate</key>

 <value i:type="a:int" xmlns:a="http://www.w3.org/2001/XMLSchema">15</value>

 </item>

 </metadata>

</result>

### Unique Knowledge

As specified, the get configuration can be used to obtain knowledge about unique characteristics of a service. Through get configuration, a service may expose implementation and/or service-specific configuration parameter names and values that are not explicitly described in this document.

### Return Values Detail

The get configuration operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service provides the current configuration |
| **Required Elements** | status (Status, §3.12)the literal “success”metadata (Dictionary, §3.3)the target biometric sensor’s current configuration |
| **Optional Elements** | None |

See §4.2 for information regarding configurations.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot provide the current configuration due to service (not target biometric sensor) error. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST only use this status to report failures that occur within the web service, not the target biometric sensor (see §6.11.4.11, §6.11.4.6).

#### Configuration Needed

|  |  |
| --- | --- |
| **Status Value** | configurationNeeded |
| **Condition** | The configuration could not be queried because the target biometric sensor has not been initialized. |
| **Required Elements** | status (Status, §3.12)the literal “configurationNeeded” |
| **Optional Elements** | None |

Services MAY require configuration to be set before a configuration can be retrieved if a service does not provide a valid default configuration.

#### Initialization Needed

|  |  |
| --- | --- |
| **Status Value** | initializationNeeded |
| **Condition** | The configuration could not be queried because the target biometric sensor has not been initialized. |
| **Required Elements** | status (Status, §3.12)the literal “initializationNeeded” |
| **Optional Elements** | None |

Services SHOULD be able to provide the sensors configuration without initialization; however, this is not always possible. Robust clients SHOULDassume that configuration will require initialization.

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | The configuration could not be queried because the target biometric sensor took too long to complete the request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See A.2 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The configuration could not be queried due to a failure within the target biometric sensor. |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.9.4.2).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The configuration could not be queried because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | The configuration could not be queried because the requesting client does not hold the lock. |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The configuration could not be queried because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The get configuration operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The get configuration operation was interrupted by a cancellation request during which the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to perform initialization to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Set Configuration

|  |  |
| --- | --- |
| **Description** | Set the target biometric sensor’s configuration |
| **URL Template** | /configure/{sessionId} |
| **HTTP Method**  | POST  |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session setting the configuration |
| **Input Payload** | Desired sensor configuration (Dictionary, §3.3) |
| **Idempotent** | Yes |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| **initializationNeeded** | status="initializationNeeded" |
| sensorTimeout | status="sensorTimeout" |
| sensorFailure | status="sensorFailure" |
| sensorBusy | status="sensorBusy" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| unsupported | status="unsupported"badFields={field names} (StringArray, §3.7) |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) *(or)*status="badValue"badFields={field names} (StringArray, §3.7) |
| noSuchParameter | status="unsupported"badFields={field names} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The set configuration operation sets the configuration of a service’s target biometric sensor.

#### Input Payload Information

The set configuration operation is the only operation that takes input within the body of the HTTP request. The desired configuration MUST be sent as a single Dictionary (§3.3) element named configuration. See §4.2 for information regarding configurations. See Appendix C for a complete XML Schema for this specification. The root element of the configuration data MUST conform to the following XML definition:

<xs:element name="configuration" type="wsbd:Dictionary" nillable="true"/>

Example: The following represents a ‘raw’ request to configure a service at http://10.0.0.8:8000/Sensor such that width=800, height=600, and frameRate=15. (In this example, each value element contains fully qualified namespace information, although this is not necessary.)

POST http://10.0.0.8:8000/Service/configure/d745cd19-facd-4f91-8774-aac5ca9766a2 HTTP/1.1

Content-Type: application/xml

Host: 10.0.0.8:8000

Content-Length: 459

Expect: 100-continue

<configuration xmlns:i="http://www.w3.org/2001/XMLSchema-instance" xmlns="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0">

 <item>

 <key>width</key>

 <value xmlns:d3p1="http://www.w3.org/2001/XMLSchema" i:type="d3p1:int">800</value>

 </item>

 <item>

 <key>height</key>

 <value xmlns:d3p1="http://www.w3.org/2001/XMLSchema" i:type="d3p1:int">600</value>

 </item>

 <item>

 <key>frameRate</key>

 <value xmlns:d3p1="http://www.w3.org/2001/XMLSchema" i:type="d3p1:int">15</value>

 </item>

</configuration>

More information regarding the use of the xmlns attribute can be found in [XMLNS].

### Unique Knowledge

The set configuration canbe used to provide knowledge about unique characteristics to a service. Through set configuration, a client MAY provide implementation and/or service-specific parameter names and values that are not defined in this document (see Appendix A for further information on parameters).

### Return Values Detail

The set configuration operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service was able to successfully set the full configuration  |
| **Required Elements** | status (Status, §3.12)the literal “success” |
| **Optional Elements** | None |

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot set the desired configuration due to service (not target biometric sensor) error. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure  |

Services MUST only use this status to report failures that occur within the web service, not the target biometric sensor (see §6.12.4.10, §6.12.4.5).

#### Initialization Needed

|  |  |
| --- | --- |
| **Status Value** | initializationNeeded |
| **Condition** | The configuration could not be set because the target biometric sensor has not been initialized. |
| **Required Elements** | status (Status, §3.12)the literal “initializationNeeded” |
| **Optional Elements** | None |

Services SHOULD be able to set the configuration without initialization; however, this is not strictly necessary or always possible. Similarly, robust clients SHOULD assume that setting configuration will require initialization.

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | The configuration could not be set because the target biometric sensor took too long to complete the request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See A.2 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The configuration could not be set due to a failure within the target biometric sensor. |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.12.4.2). Errors with the configuration itself SHALL be reported via an unsupported (§6.12.4.11), badValue (§6.12.4.12), or badValue status (§6.12.4.13).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The configuration could not be set because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | The configuration could not be queried because the requesting client does not hold the lock. |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The configuration could not be set because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The set configuration operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The set configuration operation was interrupted by a cancellation request during which the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to perform initialization to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Unsupported

|  |  |
| --- | --- |
| **Status Value** | unsupported |
| **Condition** | The requested configuration contains one or more values that are syntactically and semantically valid, but not supported by the service. |
| **Required Elements** | status (Status, §3.12)the literal “unsupported”badFields (StringArray, §3.7)an array that contains the field name(s) that corresponding to the unsupported value(s) |
| **Optional Elements** | None |

Returning *multiple* fields allows a service to indicate that a particular *combination* of parameters is not supported by a service. See §6.1.2 for additional information on how services MUST handle parameter failures.

Example: A WS-BD service utilizes a very basic off-the-shelf web camera with limited capabilities. This camera has three parameters that are all dependent on each other: ImageHeight, ImageWidth, and FrameRate. The respective allowed values for each parameter might look like: {240, 480, 600, 768}, {320, 640, 800, 1024}, and {5, 10, 15, 20, 30}. Configuring the sensor will return unsupported when the client tries to set ImageHeight=768, ImageWidth=1024, and FrameRate=30; this camera might not support capturing images of a higher resolution at a fast frame rate. Another example is configuring the sensor to use ImageHeight=240 and ImageWidth=1024; as this is a very basic web camera, it might not support capturing images at this resolution. In both cases, the values provided for each parameter are individually valid but the overall validity is dependent on the combination of parameters

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | Either:1. The provided session id is not a well-formed UUID, or,
2. The requested configuration contains a parameter value that is either syntactically (e.g., an inappropriate data type) or semantically (e.g., a value outside of an acceptable range) invalid.
 |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains either 1. the single field name, “sessionId”, or
2. the field name(s) that contain invalid value(s)
 |
| **Optional Elements** | None |

Notice that for the set configuration operation, an invalid URL parameter *or* one or more invalid input payload parameters can trigger a badValue status.

See §6.1.2 for general information on how services MUST handle parameter failures.

#### No Such Parameter

|  |  |
| --- | --- |
| **Status Value** | noSuchParameter |
| **Condition** | The requested configuration contains a parameter name that is not recognized by the service. |
| **Required Elements** | status (Status, §3.12)the literal “noSuchParameter”badFields (StringArray, §3.7)an array that contains the field name(s) that are not recognized by the service |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

## Capture

|  |  |
| --- | --- |
| **Description** | Capture biometric data |
| **URL Template** | /capture/{sessionId} |
| **HTTP Method**  | POST  |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting the capture |
| **Input Payload** | None |
| **Idempotent** | No |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"captureIds={identifiers of captured data} (UuidArray, §3.8) |
| failure | status="failure"message\*=informative message describing failure |
| configurationNeeded | status="configurationNeeded" |
| initializationNeeded | status="initializationNeeded" |
| sensorTimeout | status="sensorTimeout" |
| sensorFailure | status="sensorFailure" |
| sensorBusy | status="sensorBusy" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The capture operation triggers biometric acquisition. On success, the operation returns one or more identifiers, or *capture id*s. Naturally, the capture operation is *not* idempotent. Each capture operation returns unique identifiers—each execution returning references that are particular to that capture. Clients then can retrieve the captured data itself by passing a *capture id* as a URL parameter to the download operation.

Multiple *capture ids* are supported to accommodate sensors that return collections of biometric data. For example, a multi-sensor array might save an image per sensor. A mixed-modality sensor might assign a different capture id for each modality.

Important Note: The capture operation MAY include some post-acquisition processing. Although post-acquisition processing is directly tied to the capture operation, its effects are primarily on data transfer, and is therefore discussed in detail within the download operation documentation (§6.16.2.2)

#### Providing Timing Information

Depending on the sensor, a capture operation may take anywhere from milliseconds to tens of seconds to execute. (It is possible to have even longer running capture operations than this, but special accommodations may need to be made on the server and client side to compensate for typical HTTP timeouts.) By design, there is no explicit mechanism for a client to determine how long a capture operation will take. However, services can provide “hints” through capture timeout information (A.3.4), and clients can automatically adjust their own timeouts and behavior accordingly.

### Unique Knowledge

As specified, the capture operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The capture operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service successfully performed a biometric acquisition |
| **Required Elements** | status (Status, §3.12)the literal “success”captureIds (UuidArray, §3.8)one more UUIDs that uniquely identify the data acquired by the operation |
| **Optional Elements** | None |

See the usage notes for capture (§6.13.2) and download (§6.16.2) for full detail.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot perform the capture due to a service (not target biometric sensor) error. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure  |

Services MUST only use this status to report failures that occur within the web service, not the target biometric sensor (see §6.13.4.11, §6.13.4.6). A service may fail at capture if there is not enough internal storage available to accommodate the captured data (§A.4).

#### Configuration Needed

|  |  |
| --- | --- |
| **Status Value** | configurationNeeded |
| **Condition** | The capture could not be set because the target biometric sensor has not been configured. |
| **Required Elements** | status (Status, §3.12)the literal “configurationNeeded” |
| **Optional Elements** | None |

A service SHOULDoffer a default configuration to allow capture to be performed without an explicit configuration. Regardless, for robustness, clients SHOULD assume that capture requires configuration.

#### Initialization Needed

|  |  |
| --- | --- |
| **Status Value** | initializationNeeded |
| **Condition** | The service could not perform a capture because the target biometric sensor has not been initialized. |
| **Required Elements** | status (Status, §3.12)the literal “initializationNeeded” |
| **Optional Elements** | None |

Services SHOULD be able perform capture without explicit initialization. However, the specification recognizes that this is not always possible, particularly for physically separated implementations. Regardless, for robustness, clients SHOULD assume that setting configuration will require initialization.

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | The service could not perform a capture because the target biometric sensor took too long to complete the request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See §A.3 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The service could perform the capture due to a failure within the target biometric sensor. |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.13.4.2).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The service could not perform a capture because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | The service could not perform a capture because the requesting client does not hold the lock. |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The service could not perform a capture because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The capture operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The capture operation was interrupted by a cancellation request during which the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to perform initialization to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Begin Capture

|  |  |
| --- | --- |
| **Description** | Starts the capture of biometric data and returns immediately after the capture starts |
| **URL Template** | /capture/{sessionId}/async |
| **HTTP Method**  | POST  |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting the capture |
| **Input Payload** | None |
| **Idempotent** | No |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| configurationNeeded | status="configurationNeeded" |
| initializationNeeded | status="initializationNeeded" |
| sensorTimeout | status="sensorTimeout" |
| sensorFailure | status="sensorFailure" |
| sensorBusy | status="sensorBusy" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The begin capture operation, used with the end capture operation, allows for asynchronous captures and captures over a duration of time. With the capture operation, the sensor MUST capture data from a single moment. However, some biometrics, such as voice and signature, use variable length data. While a capture operation could capture voice data with a set length, the asynchronous capture functions allow the client to start the recording and then record the desired length of data. Sensors which do not support asynchronous captures MUST immediately return success when begin capture is called, and perform the entire capture sequence when end capture is called. This guarantees that on a sensor that does not support asynchronous captures, the client will get the same result with a call to capture as with calls to begin capture and end capture.

### Unique Knowledge

As specified, the begin capture operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The begin capture operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service successfully started the biometric acquisition |
| **Required Elements** | status (Status, §3.12)the literal “success”captureIds (UuidArray, §3.8)one more UUIDs that uniquely identify the data acquired by the operation |
| **Optional Elements** | None |

See the usage notes for capture (§6.13.2), *begin c*apture (§6.14.2), end capture (§6.15.2), and download (§6.16.2) for full detail.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot perform the capture due to a service (not target biometric sensor) error. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure  |

Services MUST only use this status to report failures that occur within the web service, not the target biometric sensor (see §6.13.4.11, §6.13.4.6). A service may fail at capture if there is not enough internal storage available to accommodate the captured data (§A.4).

#### Configuration Needed

|  |  |
| --- | --- |
| **Status Value** | configurationNeeded |
| **Condition** | The capture could not be set because the target biometric sensor has not been configured. |
| **Required Elements** | status (Status, §3.12)the literal “configurationNeeded” |
| **Optional Elements** | None |

A service SHOULDoffer a default configuration to allow capture to be performed without an explicit configuration. Regardless, for robustness, clients SHOULDassume that capture requires configuration.

#### Initialization Needed

|  |  |
| --- | --- |
| **Status Value** | initializationNeeded |
| **Condition** | The service could not perform a capture because the target biometric sensor has not been initialized. |
| **Required Elements** | status (Status, §3.12)the literal “initializationNeeded” |
| **Optional Elements** | None |

Services SHOULDbe able perform capture without explicit initialization. However, the specification recognizes that this is not always possible, particularly for physically separated implementations. Regardless, for robustness, clients SHOULDassume that setting configuration will require initialization.

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | The service could not perform a capture because the target biometric sensor took too long to complete the request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See §A.3 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The service could perform the capture due to a failure within the target biometric sensor. |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.13.4.2).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The service could not perform a capture because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | The service could not perform a capture because the requesting client does not hold the lock. |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The service could not perform a capture because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The begin capture operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The begin capture operation was interrupted by a cancellation request during which the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to perform initialization to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## End Capture

|  |  |
| --- | --- |
| **Description** | Ends the asynchronous capture of sensor data, blocking if necessary |
| **URL Template** | /capture/{sessionId}/async |
| **HTTP Method**  | PUT  |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting the capture |
| **Input Payload** | None |
| **Idempotent** | No |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"captureIds={identifiers of captured data} (UuidArray, §3.8) |
| failure | status="failure"message\*=informative message describing failure |
| invalidId | status="invalidId"badFields={"sessionId"} (StringArray, §3.7) |
| canceled | status="canceled" |
| canceledWithSensorFailure | status="canceledWithSensorFailure" |
| sensorFailure | status="sensorFailure" |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| sensorBusy | status="sensorBusy" |
| sensorTimeout | status="sensorTimeout" |
| badValue | status="badValue"badFields={"sessionId"} (StringArray, §3.7) |

### Usage Notes

The End Capture operation will behave slightly different depending on the type of sensor that is capturing the data:

* Automatic Capture: In the case of sensors that can automatically capture, if a frame has already been captured, the call returns immediately; otherwise, the call blocks until a frame is successfully captured.
* Manual Capture: In the case of sensors that cannot automatically select the best frame, End Capture records the current frame at the time End Capture is called to be returned by the download method.
* Variable Length Capture: In the case of variable length samples, End Capture ends the recording of data.

A call to End Capture does not return until the sensor has finished capturing a sample.

#### Transferrable Asynchronous Captures

Consider the following scenario with two clients, Alice and Bob. Alice and Bob both register with the service. Alice then obtains the lock and starts an asynchronous capture with Begin Capture. Then, Alice waits a while, and the Lock Stealing Prevention Period elapses. Bob then steals the lock. In accordance with the lock stealing specification, the lock stealing had no effect on the currently running capture. Thus, Bob can now call end capture and steal Alice’s capture data. Depending on the situation, this behavior may or may not be desirable. One case where it would be useful is if Alice started the capture, and then her computer crashed. She should then be able to register on another computer, steal the lock, and finish her capture without having to start over. However, it also means that one client can obtain another client’s biometric data, which may be a privacy concern. Thus, sensors MUST , in their sensor information (see §A.2), have a transferableAsycCapture flag.

#### Status Monitoring

During an asynchronous capture, the client may wish to get feedback from the sensor. This SHOULD be done using a live stream. If a sensor provides textual feedback, that can also be sent using a live stream.

### Unique Knowledge

As specified, the end capture operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The end capture operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service successfully started the biometric acquisition |
| **Required Elements** | status (Status, §3.12)the literal “success”captureIds (UuidArray, §3.8)one more UUIDs that uniquely identify the data acquired by the operation |
| **Optional Elements** | None |

See the usage notes for capture (§6.13.2), begin capture (§6.14.2), end capture (§6.15.2), and download (§6.16.2) for full detail.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot perform the capture due to a service (not target biometric sensor) error. Also returned if no asynchronous capture has been started. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure  |

Services MUST only use this status to report failures that occur within the web service, not the target biometric sensor (see §6.13.4.11, §6.13.4.6). A service may fail at capture if there is not enough internal storage available to accommodate the captured data (§A.4).

#### Sensor Timeout

|  |  |
| --- | --- |
| **Status Value** | sensorTimeout |
| **Condition** | The service could not perform a capture because the target biometric sensor took too long to complete the request. |
| **Required Elements** | status (Status, §3.12)the literal “sensorTimeout” |
| **Optional Elements** | None |

A service did not receive a timely response from the target biometric sensor. Note that this condition is distinct from the client’s originating HTTP request, which may have its own, independent timeout. (See §A.3 for information on how a client might determine timeouts.)

#### Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | sensorFailure |
| **Condition** | The service could perform the capture due to a failure within the target biometric sensor. |
| **Required Elements** | status (Status, §3.12)the literal “sensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A sensorFailure status MUST only be used to report failures that occurred within the target biometric sensor, not a failure within the web service (§6.13.4.2).

#### Sensor Busy

|  |  |
| --- | --- |
| **Status Value** | sensorBusy |
| **Condition** | The service could not perform a capture because the service is already performing a different sensor operation for the requesting client. |
| **Required Elements** | status (Status, §3.12)the literal “sensorBusy” |
| **Optional Elements** | None |

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | The service could not perform a capture because the requesting client does not hold the lock. |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The service could not perform a capture because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Canceled

|  |  |
| --- | --- |
| **Status Value** | canceled |
| **Condition** | The end capture operation was interrupted by a cancellation request. |
| **Required Elements** | status (Status, §3.12)the literal “canceled” |
| **Optional Elements** | None |

See §6.20.2.2 for information about what may trigger a cancellation.

#### Canceled with Sensor Failure

|  |  |
| --- | --- |
| **Status Value** | canceledWithSensorFailure |
| **Condition** | The end capture operation was interrupted by a cancellation request during which the target biometric sensor experienced a failure |
| **Required Elements** | status (Status, §3.12)the literal “canceledWithSensorFailure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services MUST return a canceledWithSensorFailure result if a cancellation request caused a failure within the target biometric sensor. Clients receiving this result may need to perform initialization to restore full functionality. See §6.20.2.2 for information about what may trigger a cancellation.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not registered with the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Download

|  |  |
| --- | --- |
| **Description** | Download the captured biometric data |
| **URL Template** | /download/{captureId} |
| **HTTP Method**  | GET |
| **URL Parameters** | {captureId} (UUID, §3.2)Identity of the captured data to download |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"metadata=sensor configuration and capture-specific metadata (Dictionary, §3.3, §4.3.1)sensorData=biometric data (xs:base64Binary) |
| failure | status="failure"message\*=informative message describing failure |
| preparingDownload | status="preparingDownload" |
| badValue | status="badValue"badFields={"captureId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"captureId"} (StringArray, §3.7) |

### Usage Notes

The download operation allows a client to retrieve biometric data acquired during a particular capture.

#### Capture and Download as Separate Operations

WS-BD decouples the acquisition operation (capture) from the data transfer (download) operation. This has two key benefits. First, it is a better fit for services that have post-acquisition processes. Second, it allows multiple clients to download the captured biometric data by exploiting the concurrent nature of HTTP. By making download a simple data transfer operation, service can handle multiple, concurrent downloads without requiring locking.

#### Services with Post-Acquisition Processing

A service does *not* need to make the captured data available immediately after capture; a service MAY have distinct acquisition and post-acquisition processes. The following are two examples of such services:

Example: A service exposing a fingerprint scanner also performs post processing on a fingerprint image—segmentation, quality assessment, and templatization.

Example: A service exposes a digital camera in which the captured image is not immediately available after a photo is taken; the image may need to be downloaded from the camera’s internal storage or from the camera to the host computer (in a physically separated implementation). If the digital camera was unavailable for an operation due to a data transfer, a client requesting a sensor operation would receive a sensorBusy status.

The first method is to perform the post-processing within the capture operation itself. I.e., capture not only blocks for the acquisition to be performed, but also blocks for the post-processing—returning when the post-processing is complete. This type of capture is the easier of the two to both (a) implement on the client, and (b) use by a client.

Example: Figure9 illustrates an example of a capture operation that includes post-processing. Once the post-processing is complete, capture ids are returned to the client.



**Figure 9**. Including post-processing in the capture operation means downloads are immediately available when capture completes. Unless specified, the status of all returned operations is success.

In the second method, post-processing MAY be performed by the web service *after* the capture operation returns. Capture ids are still returned to the client, but are in an intermediate state. This exposes a window of time in which the capture is complete, but the biometric data is not yet ready for retrieval or download. Data-related operations (download, get download info, and thrifty download) performed within this window return a preparingDownload status to clients to indicate that the captured data is currently in an intermediate state—captured, but not yet ready for retrieval.

Example: Figure 10 illustrates an example of a capture operation with separate post-processing. Returning to the example of the fingerprint scanner that transforms a raw biometric sample into a template after acquisition, assume that the service performs templatization after capture returns. During post-processing, requests for the captured data return preparingDownload, but the sensor itself is available for another capture operation.



**Figure 10**. Example of capture with separate post-acquisition processing that does involve the target biometric sensor. Because the post-acquisition processing does not involve the target biometric sensor, it is available for sensor operations. Unless specified, the status of all returned operations is success.

Services with an independent post-processing step SHOULDperform the post-processing on an independent unit of execution (e.g., a separate thread, or process). However, post-processing may include a sensor operation, which would interfere with incoming sensor requests.

Example: Figure11 illustrates another variation on a capture operation with separate post-processing. Return to the digital camera example, but assume that it is a physically separate implementation and capture operation returns immediately after acquisition. The service also has a post-acquisition process that downloads the image data from the camera to a computer. Like the previous example, during post-processing, requests for the captured data return preparingDownload. However, the sensor is *not* available for additional operations because the post-processing step requires complete control over the camera to transfer the images to the host machine: preparing them for download.



**Figure 11**. Example of capture with separate post-acquisition processing that does involve the target biometric sensor. Because the post-acquisition processing does not involve the target biometric sensor, it is available for sensor operations. Unless specified, the status of all returned operations is success.

Unless there is an advantage to doing so, when post-acquisition processing includes a sensor operation, implementers SHOULDavoid having a capture operation that returns directly after acquisition. In this case, even when the capture operation finishes, clients cannot perform a sensor operation until the post-acquisition processing is complete.

In general, implementers SHOULDtry to combine both the acquisition and post-acquisition processing into one capture operation—particularly if the delay due to post-acquisition processing is either operationally acceptable or a relatively insignificant contributor to the combined time.

A download operation MUST return failure if the post-acquisition processing cannot be completed successfully. Such failures cannot be reflected in the originating capture operation —that operation has already returned successfully with capture ids. Services MUST eventually resolve all preparingDownload statuses to success or failure. Through get service info, a service can provide information to a client on how long to wait after capture until a preparingDownload is fully resolved.

#### Client Notification

A client that receives a preparingDownload should poll the service until the requested data becomes available. However, through get service info, a service can provide “hints” to a client on how long to wait after capture until data can be downloaded (§A.3.5)

### Unique Knowledge

The download operation canbe used to provide metadata, which may be unique to the service, through the metadata element. See §4 for information regarding metadata.

### Return Values Detail

The download operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service can provide the requested data |
| **Required Elements** | status (Status, §3.12)the literal “success”metadata (Dictionary, §3.3)sensor metadata as it was at the time of capturesensorData (xs:base64Binary, [XSDPart2])the biometric data corresponding to the requested capture id, base-64 encoded |
| **Optional Elements** | None |

A successful download MUST populate the Result with all of the following information:

1. The status element MUST be populated with the Status literal “success”.
2. The metadata element MUST be populated with metadata of the biometric data and the configuration held by the MUST biometric sensor at the time of capture.
3. The sensorData element MUST contain the biometric data, base-64 encoded (xs:base64Binary), corresponding to the requested capture id.

See the usage notes for both capture (§6.13.2) and download (§6.16.2) for more detail regarding the conditions under which a service is permitted to accept or deny download requests.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot provide the requested data. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A service might not be able to provide the requested data due to failure in post-acquisition processing, a corrupted data store or other service or storage related failure.

#### Preparing Download

|  |  |
| --- | --- |
| **Status Value** | preparingDownload |
| **Condition** | The requested data cannot be provided because the service is currently performing a post-acquisition process—i.e., preparing it for download |
| **Required Elements** | status (Status, §3.12)the literal “preparingDownload” |
| **Optional Elements** | None |

See the usage notes for both capture (§6.13.2) and download (§6.16.2) for full detail.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided capture id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “captureId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided capture id is not recognized by the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “captureId” |
| **Optional Elements** | None |

A capture id is invalid if it was not returned by a capture operation. A capture id may become unrecognized by the service automatically if the service automatically clears storage space to accommodate new captures (§A.4).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Get Download Info

|  |  |
| --- | --- |
| **Description** | Get only the metadata associated with a particular capture |
| **URL Template** | /download/{captureId}/info |
| **HTTP Method**  | GET |
| **URL Parameters** | {captureId} (UUID, §3.2)Identity of the captured data to query |
| **Input Payload** | Not applicable |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"metadata=sensor configuration at the time of capture |
| failure | status="failure"message\*=informative message describing failure |
| preparingDownload | status="preparingDownload" |
| badValue | status="badValue"badFields={"captureId"} (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"captureId"} (StringArray, §3.7) |

### Usage Notes

Given the potential large size of some biometric data the get download info operation provides clients with a way to get information about the biometric data without needing to transfer the biometric data itself. It is logically equivalent to the download operation, but without any sensor data. Therefore, unless detailed otherwise, the usage notes for download (§6.16.2) also apply to get download info.

### Unique Knowledge

The get download info operation canbe used to provide metadata, which may be unique to the service, through the metadata element. See §4 for information regarding metadata.

### Return Values Detail

The get download info operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service can provide the requested data |
| **Required Elements** | status (Status, §3.12)the literal “success”metadata (Dictionary, §3.3)the sensor’s configuration as it was set at the time of capture |
| **Optional Elements** | None |

A successful get download info operation returns all of the same information as a successful download operation (§6.16.4.1), but without the sensor data.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot provide the requested data. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure  |

A service might not be able to provide the requested data due to failure in post-acquisition processing, a corrupted data store or other service or storage related failure.

#### Preparing Download

|  |  |
| --- | --- |
| **Status Value** | preparingDownload |
| **Condition** | The requested data cannot be provided because the service is currently performing a post-acquisition process—i.e., preparing it for download |
| **Required Elements** | status (Status, §3.12)the literal “preparingDownload” |
| **Optional Elements** | None |

See the usage notes for both capture (§6.13.2) and download (§6.16.2) for full detail.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided capture id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “captureId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided capture id is not recognized by the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “captureId” |
| **Optional Elements** | None |

A capture id is invalid if it was not returned by a capture operation. A capture id may become unrecognized by the service automatically if the service automatically clears storage space to accommodate new captures (§A.4).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Thrifty Download

|  |  |
| --- | --- |
| **Description** | Download a compact representation of the captured biometric data suitable for preview |
| **URL Template** | /download/{captureId}/{maxSize} |
| **HTTP Method**  | GET |
| **URL Parameters** | {captureId} (UUID, §3.2)Identity of the captured data to download{maxSize} (xs:string, [XSDPart2])Content-type dependent indicator of maximum permitted download size |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"metadata=minimal metadata describing the captured data (Dictionary, §3.3, §4.3.1)sensorData=biometric data (xs:base64Binary) |
| failure | status="failure"message\*=informative message describing failure |
| preparingDownload | status="preparingDownload" |
| unsupported | status="unsupported" |
| badValue | status="badValue"badFields=either "captureId", "maxSize", or both (StringArray, §3.7) |
| invalidId | status="invalidId"badFields={"captureId"} (StringArray, §3.7) |

### Usage Notes

The thrifty download operation allows a client to retrieve a compact representation of the biometric data acquired during a particular capture. It is logically equivalent to the download operation, but provides a compact version of the sensor data. Therefore, unless detailed otherwise, the usage notes for download (§6.16.2) also apply to get download info.

The suitability of the thrifty download data as a biometric is implementation-dependent. For some applications, the compact representation may be suitable for use within a biometric algorithm; for others, it may only serve the purpose of preview.

For images, the maxSize parameter describes the maximum image width or height (in pixels) that the service may return; dimensions SHALL NOT exceed maxSize. It is expected that servers will dynamically scale the captured data to fulfill a client request. This is not strictly necessary, however, as long as the maximum size requirements are met.

For non-images, the default behavior is to return unsupported. It is *possible* to use URL parameter maxSize as general purpose parameter with implementation-dependent semantics. (See the next section for details.)

### Unique Knowledge

The thrifty download operation canbe used to provide knowledge about unique characteristics to a service. Through thrifty download, a service MAY (a) redefine the semantics of maxSize or (b) provide a data in a format that does not conform to the explicit types defined in this document (see A.2 for content types).

### Return Values Detail

The thrifty download operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service can provide the requested data |
| **Required Elements** | status (Status, §3.12)the literal “success”metadata (Dictionary, §3.3)minimal representation of sensor metadata as it was at the time of capture. See §4.3.1 for information regarding minimal metadata.sensorData (xs:base64Binary, [XSDPart2])the biometric data corresponding to the requested capture id, base-64 encoded, scaled appropriately to the maxSize parameter. |
| **Optional Elements** | None |

For increased efficiency, a successful thrifty download operation only returns the sensor data, and a subset of associated metadata. The metadata returned SHOULDbe information that is absolutely essential to open or decode the returned sensor data.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service cannot provide the requested data. |
| **Required Elements** | status (Status, §3.12)the literal “failure” |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

A service might not be able to provide the requested data due to a corrupted data store or other service or storage related failure.

#### Preparing Download

|  |  |
| --- | --- |
| **Status Value** | preparingDownload |
| **Condition** | The requested data cannot be provided because the service is currently performing a post-acquisition process—i.e., preparing it for download |
| **Required Elements** | status (Status, §3.12)the literal “preparingDownload” |
| **Optional Elements** | None |

Like download, the availability of thrifty download data may also be affected by the sequencing of post-acquisition processing. See §6.16.2.2 for detail.

#### Unsupported

|  |  |
| --- | --- |
| **Status Value** | unsupported |
| **Condition** | The service does not support thrifty download, |
| **Required Elements** | status (Status, §3.12)the literal “unsupported” |
| **Optional Elements** | None |

Services that capture biometrics that are not image-based SHOULDreturn unsupported.

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided capture id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains one or both of the following fields: * “captureId” if the provided session id is not well-formed
* “maxSize” if the provided maxSize parameter is not well-formed
 |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided capture id is not recognized by the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “captureId” |
| **Optional Elements** | None |

A capture id is invalid if it does not correspond to a capture operation. A capture id may become unrecognized by the service automatically if the service automatically clears storage space to accommodate new captures (§A.4).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Get Sensor Data

|  |  |
| --- | --- |
| **Description** | Download a sensor data |
| **URL Template** | /download/{captureId}/raw/download/{captureId}/raw/[contentType] |
| **HTTP Method**  | GET |
| **URL Parameters** | {captureId} (UUID, §3.2)Identity of the captured data to download[contentType] (Appendix B)Optional – the captured data in the requested content type |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

This operation will not return a Result instance. It will return the sensor data in binary form via an HTTP response (See section §6 in [RFC2616]).

### Usage Notes

The get sensor data operation allows for the binary transfer of sensor data.

Values for the optional parameter, contentType, MUST conform to values specified in Appendix B. The value MUST be URL-encoded to allow for proper handling of potentially unsafe characters.

### Unique Knowledge

The get sensor data operation canbe used to provide metadata, which may be unique to the service, through the metadata element. See §4 for information regarding metadata.

## Cancel

|  |  |
| --- | --- |
| **Description** | Cancel the current sensor operation |
| **URL Template** | /cancel/{sessionId} |
| **HTTP Method**  | POST |
| **URL Parameters** | {sessionId} (UUID, §3.2)Identity of the session requesting cancellation |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | Yes |

### Result Summary

|  |  |
| --- | --- |
| success | status="success" |
| failure | status="failure"message\*=informative message describing failure |
| lockNotHeld | status="lockNotHeld" |
| lockHeldByAnother | status="lockHeldByAnother" |
| badValue | status="badValue"badFields={"sessionId"} |
| invalidId | status="invalidId" |

### Usage Notes

The cancel operation stops any currently running sensor operation; it has no effect on non-sensor operations. If cancellation of an active sensor operation is successful, cancel operation receives a success result, while the canceled operation receives a canceled (or canceledWithSensorFailure) result. As long as the operation is canceled, the cancel operation itself receives a success result, regardless if cancellation caused a sensor failure. In other words, if cancellation caused a fault within the target biometric sensor, as long as the sensor operation has stopped running, the cancel operation is considered to be successful.



**Figure 12.** Example sequence of events for a client initially requesting a capture followed by a cancellation request.

All services MUST provide cancellation for allsensor operations.

#### Canceling Non-Sensor Operations

Clients are responsible for canceling all non-sensor operations via client-side mechanisms only. Cancellation of sensor operations requires a separate service operation, since a service may need to “manually” interrupt a busy sensor. A service that had its client terminate a non-sensor operation would have no way to easily determine that a cancellation was requested.



**Figure 13.** Cancellations of non-sensor operations do not require a cancel operation to be requested to the service. An example of this is where a client initiates then cancels a download operation.

#### Cancellation Triggers

Typically, the client that originates the sensor operation to be cancelled also initiates the cancellation request. Because WSBD operations are performed synchronously, cancellations are typically initiated on a separate unit of execution such as an independent thread or process.

Notice that the only requirement to perform cancellation is that the *requesting* client holds the service lock. It is *not* a requirement that the client that originates the sensor operation to be canceled also initiates the cancellation request. Therefore, it is *possible* that a client may cancel the sensor operation initiated by another client. This occurs if a peer client (a) manages to steal the service lock before the sensor operation is completed, or (b) is provided with the originating client’s session id.

A service might also *self-initiate* cancellation. In normal operation, a service that does not receive a timely response from a target biometric sensor would return sensorTimeout. However, if the service’s internal timeout mechanism fails, a service may initiate a cancel operation itself. Implementers should use this as a “last resort” compensating action.

In summary, clients SHOULDbe designed to not expect to be able to match a cancelation notification to any specific request or operation.

### Unique Knowledge

As specified, the cancel operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The cancel operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service successfully canceled the sensor operation |
| **Required Elements** | statusthe literal "success" |
| **Optional Elements** | None |

See the usage notes for capture (§6.13.2) and download (§6.16.2) for full detail.

#### Failure

|  |  |
| --- | --- |
| **Status Value** | failure |
| **Condition** | The service could not cancel the sensor operation |
| **Required Elements** | status (Status, §3.12)the literal "failure" |
| **Optional Elements** | message (xs:string, [XSDPart2])an informative description of the nature of the failure |

Services SHOULDtry to return failure in a timely fashion—there is little advantage to a client if it receives the cancellation failure *after* the sensor operation to be canceled completes.

#### Lock Not Held

|  |  |
| --- | --- |
| **Status Value** | lockNotHeld |
| **Condition** | The service could cancel the operation because the requesting client does not hold the lock. |
| **Required Elements** | status (Status, §3.12)the literal “lockNotHeld” |
| **Optional Elements** | None |

Sensor operations require that the requesting client holds the service lock.

#### Lock Held by Another

|  |  |
| --- | --- |
| **Status Value** | lockHeldByAnother |
| **Condition** | The service could not cancel the operation because the lock is held by another client. |
| **Required Elements** | status (Status, §3.12)the literal “lockHeldByAnother” |
| **Optional Elements** | None |

#### Bad Value

|  |  |
| --- | --- |
| **Status Value** | badValue |
| **Condition** | The provided session id is not a well-formed UUID. |
| **Required Elements** | status (Status, §3.12)the literal “badValue”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

See §6.1.2 for general information on how services MUST handle parameter failures.

#### Invalid Id

|  |  |
| --- | --- |
| **Status Value** | invalidId |
| **Condition** | The provided session id is not recognized by the service. |
| **Required Elements** | status (Status, §3.12)the literal “invalidId”badFields (StringArray, §3.7)an array that contains the single field name, “sessionId” |
| **Optional Elements** | None |

A session id is invalid if it does not correspond to an active registration. A session id may become unregistered from a service through explicit unregistration or triggered automatically by the service due to inactivity (§A.2.2).

See §6.1.2 for general information on how services MUST handle parameter failures.

## Get Sensor Status

|  |  |
| --- | --- |
| **Description** | Get the current status of the sensor |
| **URL Template** | /status |
| **HTTP Method**  | GET |
| **URL Parameters** | None |
| **Input Payload** | None |
| **Idempotent** | Yes |
| **Sensor Operation** | No |

### Result Summary

|  |  |
| --- | --- |
| success | status="success"metadata=sensor status |

### Usage Notes

The primary purpose of this operation is to give a client a way to determine the current sensor status after a lock stealing operation. While no lock is required for this operation, if a client wants to be sure that between the time the sensor status is queried and the time an operation starts that no one else uses the sensor, the client SHALL obtain a lock before calling this method.

The sensor can be in any of the following states:

* ready
* initializing
* configuring
* capturing
* uninitializing
* canceling

Each state describes the current sensor operation. The “ready” state means that the sensor is ready to start another operation.

### Unique Knowledge

As specified, the get sensor status operation cannot be used to provide or obtain knowledge about unique characteristics of a client or service.

### Return Values Detail

The *get sensor* status operation MUST return a Result according to the following constraints.

#### Success

|  |  |
| --- | --- |
| **Status Value** | success |
| **Condition** | The service can provide the requested data |
| **Required Elements** | status (Status, §3.12)the literal “success”metadata (Dictionary, §3.3)contains one key, sensorStatus, with the status |
| **Optional Elements** | None |

# Conformance Profiles

This section of the specification describes the requirements around conformance to the WS-Biometric Devices specification.

### Conformance

Implementations claiming conformance to this specification, MUST make such a claim according to all three of the following factors.

1. If the implementation is *general* or *modality specific*
2. The operations that are implemented (§7.1.3)
3. If the implementation includes live preview (§5)

An implementation that is *modality* *specific MUST* implement the service information and configuration metadata according to their respective subsection. For example, a “fingerprint” conformant service MUST implement the service and configuration information according to §7.2. Note that it is possible to implement a fingerprint-based WS-Biometric Devices service without adhering to §7.2, however, such an implementation cannot claim *modality specific* conformance.

### Language

Conformance claims MUST take the form

 “WS-Biometric Devices [*modality*] Conformance Level *n* [LA]”

where

* [*modality*]is optional phrase that indicates if the implementation is modality specific
* *L\** is an indicator if the implementation supports live preview.
* Square brackets, [ ], are indicator to the reader of this specification that the phrase is optional; they are not to be included in the claim itself

For example, the phrase “WS-Biometric Devices Conformance Level 3” indicates that the implementation is (a) not modality specific (b) implements the operations *get service information*, *initialize, get configuration, capture, download*, and *get download information* and (c) does NOT support live preview. Likewise, the phrase “WS-Biometric Devices Fingerprint Conformance Level 1L” indicates that the implementation (a) implements the service information and configuration parameters as specified by §7.2, (b) implements all operations and (c) supports live-preview.

For implementations that support multiple modalities, then there SHALL be a conformance claim for each modality. For example, a converged device that supports machine readable documents, fingerprint (according to §7.2) and iris (according to §7.4) might claim “WS-Biometric Devices Conformance Level 2, WS-Biometric Devices Fingerprint Conformance Level 3L, and WS-Biometric Devices Iris Conformance Level 1.”

### Operations

The table below shows three levels of conformance to this specification. An ‘X’ represents that the operation requires functionality and implementation. For operations that lack the identifier, the service SHOULD implement the operation minimally by always returning success and related arbitrary data. Sending success and arbitrary data removes any concern from clients whether or not certain operations are supported by removing the responsibility of functionality and implementation from the implementer/service.

|  |  |  |  |
| --- | --- | --- | --- |
| Operation Conformance Level | 1 | 2 | 3 |
| Register (§6.3) | X |  |  |
| Unregister (§6.4) | X |  |  |
| Try Lock (§6.4.4.4) | X |  |  |
| Steal Lock (§6.5.4.4) | X |  |  |
| Unlock (§6.7) | X |  |  |
| Get Service Information (§6.8) | X | X | X |
| Initialize (§6.8.4.1) | X | X | X |
| Get Configuration (§6.11) | X | X | X |
| Set Configuration (§6.12) | X | X |  |
| Capture (§6.12.4.14) | X | X | X |
| Download (§6.13.4.13) | X | X | X |
| Get Download Information (§6.17) | X | X | X |
| Thrifty Download (§6.18) | X | X |  |
| Cancel (§6.20) | X | X |  |
| Get Sensor Data (§6.19) | X | X | X |
| Get Sensor Status (§6.21) | X | X | X |

#### Additional Supported Operations

|  |  |
| --- | --- |
| Operation | Identifier |
| Live Preview (§5) | L |
| Asynchronous Capture (§6.14, §6.15) | A |

## Fingerprint

### Service Information

#### Submodality

|  |  |
| --- | --- |
| **Formal Name** | submodality |
| **Description** | A distinct subtype of fingerprint modality, supported by the sensor. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | RightThumbFlatRightIndexFlatRightMiddleFlatRightRingFlatRightLittleFlatLeftThumbFlatLeftIndexFlatLeftMiddleFlatLeftRingFlatLeftLittleFlatUnknownFlatLeftSlapRightSlapThumbsSlapTwoFingerSlapUnknownSlapRightThumbRolledRightIndexRolledRightMiddleRolledRightRingRolledRightLittleRolledLeftThumbRolledLeftIndexRolledLeftMiddleRolledLeftRingRolledLeftLittleRolledUnknownRolled |

#### Image Size

|  |  |
| --- | --- |
| **Formal Name** | fingerprintImageSize |
| **Description** | The width and height of a resulting fingerprint image, in pixels. If this value is calculated after capture, this SHALL be the maximum width and height of a resulting image. |
| **Data Type** | resolution [§3.11] |
| **Required** | Yes |
| **Allowed Values** | The width element can be any positive integer value.The height element can be any positive integer value.The unit element, if defined, MUST be “pixel” or “pixels”. |

#### Image Content Type

|  |  |
| --- | --- |
| **Formal Name** | fingerprintImageContentType |
| **Description** | The data format of the resulting fingerprint image. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Any string value conformant with Appendix B, §B.2. |

#### Image Density

|  |  |
| --- | --- |
| **Formal Name** | fingerprintImageDensity |
| **Description** | The pixel density of a resulting image represented in pixels per inch (PPI). |
| **Data Type** | xs:int [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Any positive integer value. |

## Face

### Service Information

#### Submodality

|  |  |
| --- | --- |
| **Formal Name** | submodality |
| **Description** | A distinct subtype of face modality, supported by the sensor. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Face2dFace3d |

#### Image Size

|  |  |
| --- | --- |
| **Formal Name** | faceImageSize |
| **Description** | The width and height of a resulting face image, in pixels. If this value is calculated after capture, this SHALL be the maximum width and height of a resulting image. |
| **Data Type** | resolution [§3.11] |
| **Required** | Yes |
| **Allowed Values** | The width element can be any positive integer value.The height element can be any positive integer value.The unit element, if defined, MUST be “pixel” or “pixels”. |

#### Image Content Type

|  |  |
| --- | --- |
| **Formal Name** | faceImageContentType |
| **Description** | The data format of the resulting face image. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Any string value conformant with Appendix B, §B.2 |

## Iris

### Service Information

#### Submodality

|  |  |
| --- | --- |
| **Formal Name** | submodality |
| **Description** | A distinct subtype of iris modality, supported by the sensor. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | LeftIrisRightIrisBothIrises |

#### Image Size

|  |  |
| --- | --- |
| **Formal Name** | irisImageSize |
| **Description** | The width and height of a resulting iris image, in pixels. If this value is calculated after capture, this SHALL be the maximum width and height of a resulting image. |
| **Data Type** | resolution [§3.11] |
| **Required** | Yes |
| **Allowed Values** | The width element can be any positive integer value.The height element can be any positive integer value.The unit element, if defined, MUST be “pixel” or “pixels”. |

#### Image Content Type

|  |  |
| --- | --- |
| **Formal Name** | irisImageContentType |
| **Description** | The data format of the resulting iris image. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Any string value conformant with Appendix B, §B.2. |

## Unknown

### Service Information

#### Submodality

|  |  |
| --- | --- |
| **Formal Name** | submodality |
| **Description** | A distinct subtype of face modality, supported by the sensor. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Unknown |

#### Image Size

|  |  |
| --- | --- |
| **Formal Name** | UnknownImageSize |
| **Description** | The width and height of a resulting unknown image, in pixels. If this value is calculated after capture, this SHALL be the maximum width and height of a resulting image. |
| **Data Type** | resolution [§3.11] |
| **Required** | Yes |
| **Allowed Values** | The width element can be any positive integer value.The height element can be any positive integer value.The unit element, if defined, MUST be “pixel” or “pixels”. |

#### Image Content Type

|  |  |
| --- | --- |
| **Formal Name** | unknownImageContentType |
| **Description** | The data format of the resulting iris image. |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |
| **Allowed Values** | Any string value conformant with Appendix B, §B.2. |

1. Parameter Details

This appendix details the individual parameters available from a get service info operation. For each parameter, the following information is listed:

* The formal parameter name
* The expected data type of the parameter’s value
* If the service is required to implement the parameter
	1. Sensor Service

The following parameters describe information about the sensor and its supporting features

* + 1. Modality

|  |  |
| --- | --- |
| **Formal Name** | modality |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |

This parameter describes which modality or modalities are supported by the sensor.

The following table enumerates the list of modalities, as defined in [CBEFF2010], which provides the valid values for this field for currently identified modalities. Implementations are not limited to the following values, but SHALL use them if such modality is exposed. For example, if an implementation is exposing fingerprint capture capability, “Finger” SHALL be used. If an implementation is exposing an unlisted modality, it MAY use another value.

|  |  |
| --- | --- |
| Modality Value | Description |
| Scent | Information about the scent left by a subject |
| DNA | Information about a subject’s DNA |
| Ear | A subject’s ear image |
| Face | An image of the subject’s face, either in two or three dimensions |
| Finger | An image of one of more of the subject’s fingerprints |
| Foot | An image of one or both of the subject’s feet. |
| Vein | Information about a subject’s vein pattern |
| HandGeometry | The geometry of an subject’s hand |
| Iris | An image of one of both of the subject’s irises |
| Retina | An image of one or both of the subject’s retinas |
| Voice | Information about a subject’s voice |
| Gait | Information about a subject’s gait or ambulatory movement |
| Keystroke | Information about a subject’s typing patterns |
| LipMovement | Information about a subject’s lip movements |
| SignatureSign | Information about a subject’s signature or handwriting |
| Unknown | Unknown information about a subject’s biometric  |

* + 1. Submodality

|  |  |
| --- | --- |
| **Formal Name** | submodality |
| **Data Type** | xs:string [XSDPart2] |
| **Required** | Yes |

This parameter describes which submodalities are supported by the sensor. See §6.21 for submodality requirements for a particular modality.

* 1. Connections

The following parameters describe how the service handles session lifetimes and registrations.

* + 1. Last Updated

|  |  |
| --- | --- |
| **Formal Name** | lastUpdated |
| **Data Type** | xs:dateTime [XSDPart2] |
| **Required** | Yes |

This parameter provides a timestamp of when the service last *updated* the common info parameters (this parameter not withstanding). The timestamp MUST include time zone information. Implementers SHOULD expect clients to use this timestamp to detect if any cached values of the (other) common info parameters may have changed.

* + 1. Inactivity Timeout

|  |  |
| --- | --- |
| **Formal Name** | inactivityTimeout |
| **Data Type** | xs:nonNegativeInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes how long, in *seconds*, a session can be inactive before it may be automatically closed by the service. A value of ‘0’ indicates that the service never drops sessions due to inactivity.

Inactivity time is measured *per session*. Services MUST measure it as the time elapsed between (a) the time at which a client initiated the session’s most recent operation and (b) the current time. Services MUST only use the session id to determine a session’s inactivity time. For example, a service does not maintain different inactivity timeouts for requests that use the same session id, but originate from two different IP addresses. Services MAY wait longer than the inactivity timeout to drop a session, but MUST NOT drop inactive sessions any sooner than the inactivityTimeout parameter indicates.

* + 1. Maximum Concurrent Sessions

|  |  |
| --- | --- |
| **Formal Name** | maximumConcurrentSessions |
| **Data Type** | xs:positiveInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes the maximum number of concurrent sessions a service can maintain. Upon startup, a service MUST have zero concurrent sessions. When a client registers successfully (§6.3), the service increases its count of concurrent sessions by one. After successful unregistration (§6.4), the service decreases its count of concurrent sessions by one .

* + 1. Least Recently Used (LRU) Sessions Automatically Dropped

|  |  |
| --- | --- |
| **Formal Name** | autoDropLRUSessions |
| **Data Type** | xs:boolean [XSDPart2] |
| **Required** | Yes |

This parameter describes whether or not the service automatically unregisters the least-recently-used session when the service has reached its maximum number of concurrent sessions. If *true*, then upon receiving a registration request, the service MAY drop the least-recently used session if the maximum number of concurrent sessions has already been reached. If *false*, then any registration request that would cause the service to exceed its maximum number of concurrent sessions results in failure. The service SHALL NOT drop a session that currently holds the lock unless the session’s inactivity is outside of the inactivity timeout (§A.2.2) threshold.

* 1. Timeouts

Clients SHOULD NOT block indefinitely on any operation. However, since different services may differ significantly in the time they require to complete an operation, clients require a means to determine appropriate timeouts. The timeouts in this subsection describe how long a *service* waits until the service either returns sensorTimeout or initiates a service-side cancellation (§6.20.2.1). Services may wait longer than the times reported here, but, (under normal operations) MUST NOT report a sensorTimeout or initiate a cancellation before the reported time elapses. In other words, a client should be able to use these timeouts to help determine a reasonable upper bound on the time required for sensor operations.

Note that these timeouts do not include any round-trip and network delay—clients SHOULDadd an additional window to accommodate delays unique to that particular client-server relationship.

* + 1. Initialization Timeout

|  |  |
| --- | --- |
| **Formal Name** | initializationTimeout |
| **Data Type** | xs:positiveInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes how long, in *milliseconds*, a service will wait for a target biometric sensor to perform initialization before it returns sensorTimeout (§6.9.4.3) or initiates a service-side cancellation (§6.20.2.1).

* + 1. Get Configuration Timeout

|  |  |
| --- | --- |
| **Formal Name** | getConfigurationTimeout |
| **Data Type** | xs:positiveInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes how long, in *milliseconds*, a service will wait for a target biometric sensor to retrieve its configuration before it returns sensorTimeout (§6.11.4.5) or initiates a service-side cancellation (§6.20.2.1).

* + 1. Set Configuration Timeout

|  |  |
| --- | --- |
| **Formal Name** | setConfigurationTimeout |
| **Data Type** | xs:positiveInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes how long, in *milliseconds*, a service will wait for a target biometric sensor to set its configuration before it returns sensorTimeout (§6.12.4.4) or initiates a service-side cancellation (§6.20.2.1).

* + 1. Capture Timeout

|  |  |
| --- | --- |
| **Formal Name** | captureTimeout |
| **Data Type** | xs:positiveInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes how long, in *milliseconds*, a service will wait for a target biometric sensor to perform biometric acquisition before it returns sensorTimeout (§6.12.4.4) or initiates a service-side cancellation (§6.20.2.1).

* + 1. Post-Acquisition Processing Time

|  |  |
| --- | --- |
| **Formal Name** | postAcquisitionProcessingTime |
| **Data Type** | xs:nonNegativeInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes an upper bound on how long, in *milliseconds*, a service takes to perform post-acquisition processing. A client SHOULD NOTexpect to be able to download captured data *before* this time has elapsed. Conversely, this time also describes how long after a capture a server is permitted to return preparingDownload for the provided capture ids. A value of zero (‘0’) indicates that the service includes any post-acquisition processing within the capture operation or that no post-acquisition processing is performed.

* + 1. Lock Stealing Prevention Period

|  |  |
| --- | --- |
| **Formal Name** | lockStealingPreventionPeriod |
| **Data Type** | xs:nonNegativeInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes the length, in *milliseconds*, of the lock stealing prevention period (§6.6.2.2).

* 1. Storage

The following parameters describe how the service stores captured biometric data.

* + 1. Maximum Storage Capacity

|  |  |
| --- | --- |
| **Formal Name** | maximumStorageCapacity |
| **Data Type** | xs:positiveInteger [XSDPart2] |
| **Required** | Yes |

This parameter describes how much data, in bytes, the service is capable of storing.

* + 1. Least-Recently Used Capture Data Automatically Dropped

|  |  |
| --- | --- |
| **Formal Name** | lruCaptureDataAutomaticallyDropped |
| **Data Type** | xs:boolean [XSDPart2] |
| **Required** | Yes |

This parameter describes whether or not the service automatically deletes the least-recently-used capture to stay within its maximum storage capacity. If *true*, the service MAY automatically delete the least-recently used biometric data to accommodate for new data. If *false*, then any operation that would require the service to exceed its storage capacity would fail.

1. Content Type Data

This appendix contains a catalog of content types for use in conformance profiles and parameters. When possible, the identified data formats SHALL be used.

* 1. General Type

|  |  |
| --- | --- |
| application/xml | Extensible Markup Language (XML) **[XML]** |
| text/plain | Plaintext **[RFC2046]** |
| text/xml | Extensible Markup Language (XML) **[XML]** |
| text/event-stream | Server Sent Events **[SSE]** |

* 1. Image Formats

Refer to **[CMediaType]** for more information regarding a registered image type.

|  |  |
| --- | --- |
| image/jpeg | Joint Photographics Experts Group **[JPEG]** |
| image/png | Portable Network Graphics **[PNG]** |
| image/tiff | Tagged Image File Format **[TIFF]** |
| image/x-ms-bmp | Windows OS/2 Bitmap Graphics **[BMP]** |
| image/x-wsq | Wavelet Scalar Quantization (WSQ) **[WSQ]** |

* 1. Video Formats

Refer to **[CMediaType]** for more information regarding a registered video type.

|  |  |
| --- | --- |
| multipart/x-mixed-replace | multipart/x-mixed-replace **[HTML5]**  |
| video/h264 | H.264 Video Compression **[H264]** |
| video/mpeg | Moving Pictures Experts Group **[MPEG]** |
| video/quicktime | QuickTime File Format **[QTFF]** |
| video/x-avi | Audio Video Interleave **[AVI]** |
| video/x-ms-asf | Advanced Systems Format **[ASF]** |
| video/x-ms-asx | Advanced Stream Redirector **[ASX]** |
| video/x-ms-wmv | Windows Media Video **[ASF]** |

* 1. Audio Formats

Refer to **[CMediaType]** for more information regarding a registered audio type.

|  |  |
| --- | --- |
| audio/3gpp | 3rd Generation Partnership Project Multimedia files **[3GPP]** |
| audio/3gpp2 | 3rd Generation Partnership Project Multimedia files **[3GPP2]** |
| audio/mpeg | Moving Pictures Experts Group **[MPEG1]** |
| audio/ogg | Vorbis OGG Audio File **[OGG]** |
| audio/x-aiff | Audio Interchange File Format **[AIFF]** |
| audio/x-ms-wav | Waveform Audio File Format **[WAVE]** |
| audio/x-ms-wma | Windows Media Audio **[ASF]** |
| audio/x-sphere | NIST Speech Header Resources **[SPHERE]** |

* 1. General Biometric Formats

|  |  |
| --- | --- |
| x-biometric/x-ansi-nist-itl-2000 | Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial, & Scar Mark & Tattoo (SMT) Information **[AN2K]** |
| x-biometric/x-ansi-nist-itl-2007 | Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial, & Other Biometric Information – Part 1 **[AN2K7]** |
| x-biometric/x-ansi-nist-itl-2008 | Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial, & Other Biometric Information – Part 2: XML Version **[AN2K8]** |
| x-biometric/x-ansi-nist-itl-2011 | Information Technology: American National Standard for Information Systems—Data Format for the Interchange of Fingerprint, Facial & Other Biometric Information **[AN2K11]** |
| x-biometric/x-cbeff-2010 | Common Biometric Exchange Formats Framework with Support for Additional Elements **[CBEFF2010]** |
| x-biometric/x-cbeff-2015 | Common Biometric Exchange Formats Framework with Support for Additional Elements **[CBEFF2015]** |

* 1. ISO / Modality-Specific Formats

|  |  |
| --- | --- |
| x-biometric/x-iso-19794-2-05 | Finger Minutiae Data **[BDIF205]** |
| x-biometric/x-iso-19794-2-15 | Finger Minutiae Data **[BDIF215]** |
| x-biometric/x-iso-19794-3-06 | Finger Pattern Spectral Data **[BDIF306]** |
| x-biometric/x-iso-19794-4-05 | Finger Image Data **[BDIF405]** |
| x-biometric/x-iso-19794-4-15 | Finger Image Data **[BDIF415]** |
| x-biometric/x-iso-19794-5-05 | Face Image Data **[BDIF505]** |
| x-biometric/x-iso-19794-5-15 | Face Image Data **[BDIF515]** |
| x-biometric/x-iso-19794-6-05 | Iris Image Data **[BDIF605]** |
| x-biometric/x-iso-19794-6-11 | Iris Image Data **[BDIF611]** |
| x-biometric/x-iso-19794-6-15 | Iris Image Data **[BDIF615]** |
| x-biometric/x-iso-19794-7-07 | Signature/Sign Time Series Data **[BDIF707]** |
| x-biometric/x-iso-19794-7-15 | Signature/Sign Time Series Data **[BDIF715]** |
| x-biometric/x-iso-19794-8-06 | Finger Pattern Skeletal Data **[BDIF806]** |
| x-biometric/x-iso-19794-8-06 | Finger Pattern Skeletal Data **[BDIF814]** |
| x-biometric/x-iso-19794-9-07 | Vascular Image Data **[BDIF907]** |
| x-biometric/x-iso-19794-9-15 | Vascular Image Data **[BDIF915]** |
| x-biometric/x-iso-19794-10-07 | Hand Geometry Silhouette Data **[BDIF1007]** |

1. XML Schema

<?xml version="1.0"?>

<xs:schema xmlns:wsbd="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0"

 xmlns:xs="http://www.w3.org/2001/XMLSchema"

 targetNamespace="http://docs.oasis-open.org/bioserv/ns/wsbd-1.0"

 elementFormDefault="qualified">

 <xs:element name="configuration" type="wsbd:Dictionary" nillable="true" />

 <xs:element name="result" type="wsbd:Result" nillable="true" />

 <xs:complexType name="Result">

 <xs:sequence>

 <xs:element name="status" type="wsbd:Status" />

 <xs:element name="badFields" type="wsbd:StringArray" nillable="true" minOccurs="0" />

 <xs:element name="captureIds" type="wsbd:UuidArray" nillable="true" minOccurs="0" />

 <xs:element name="metadata" type="wsbd:Dictionary" nillable="true" minOccurs="0" />

 <xs:element name="message" type="xs:string" nillable="true" minOccurs="0" />

 <xs:element name="sensorData" type="xs:base64Binary" nillable="true" minOccurs="0" />

 <xs:element name="sessionId" type="wsbd:UUID" nillable="true" minOccurs="0" />

 </xs:sequence>

 </xs:complexType>

 <xs:simpleType name="UUID">

 <xs:restriction base="xs:string">

 <xs:pattern value="[\da-fA-F]{8}-[\da-fA-F]{4}-[\da-fA-F]{4}-[\da-fA-F]{4}-[\da-fA-F]{12}" />

 </xs:restriction>

 </xs:simpleType>

 <xs:simpleType name="Status">

 <xs:restriction base="xs:string">

 <xs:enumeration value="success" />

 <xs:enumeration value="failure" />

 <xs:enumeration value="invalidId" />

 <xs:enumeration value="canceled" />

 <xs:enumeration value="canceledWithSensorFailure" />

 <xs:enumeration value="sensorFailure" />

 <xs:enumeration value="lockNotHeld" />

 <xs:enumeration value="lockHeldByAnother" />

 <xs:enumeration value="initializationNeeded" />

 <xs:enumeration value="configurationNeeded" />

 <xs:enumeration value="sensorBusy" />

 <xs:enumeration value="sensorTimeout" />

 <xs:enumeration value="unsupported" />

 <xs:enumeration value="badValue" />

 <xs:enumeration value="noSuchParameter" />

 <xs:enumeration value="preparingDownload" />

 </xs:restriction>

 </xs:simpleType>

 <xs:simpleType name="SensorStatus">

 <xs:restriction base="xs:string">

 <xs:enumeration value="ready" />

 <xs:enumeration value="initializing" />

 <xs:enumeration value="configuring" />

 <xs:enumeration value="capturing" />

 <xs:enumeration value="uninitializing" />

 <xs:enumeration value="canceling"/>

 </xs:restriction>

 </xs:simpleType>

 <xs:simpleType name="Modality">

 <xs:restriction base="xs:string">

 <xs:enumeration value="Scent" />

 <xs:enumeration value="DNA" />

 <xs:enumeration value="Ear" />

 <xs:enumeration value="Face" />

 <xs:enumeration value="Finger" />

 <xs:enumeration value="Foot" />

 <xs:enumeration value="Vein" />

 <xs:enumeration value="HandGeometry" />

 <xs:enumeration value="Iris" />

 <xs:enumeration value="Retina" />

 <xs:enumeration value="Voice" />

 <xs:enumeration value="Gait" />

 <xs:enumeration value="Keystroke" />

 <xs:enumeration value="LipMovement" />

 <xs:enumeration value="SignatureSign" />

 <xs:enumeration value="Unknown" />

 </xs:restriction>

 </xs:simpleType>

 <xs:complexType name="Array">

 <xs:sequence>

 <xs:element name="element" type="xs:anyType" nillable="true" minOccurs="0" maxOccurs="unbounded" />

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="StringArray">

 <xs:sequence>

 <xs:element name="element" type="xs:string" nillable="true" minOccurs="0" maxOccurs="unbounded" />

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="UuidArray">

 <xs:sequence>

 <xs:element name="element" type="wsbd:UUID" nillable="true" minOccurs="0" maxOccurs="unbounded" />

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="ResourceArray">

 <xs:sequence>

 <xs:element name="element" type="wsbd:Resource" nillable="true" minOccurs="0" maxOccurs="unbounded" />

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="Dictionary">

 <xs:sequence>

 <xs:element name="item" minOccurs="0" maxOccurs="unbounded">

 <xs:complexType>

 <xs:sequence>

 <xs:element name="key" type="xs:string" nillable="true" />

 <xs:element name="value" type="xs:anyType" nillable="true" />

 </xs:sequence>

 </xs:complexType>

 </xs:element>

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="Parameter">

 <xs:sequence>

 <xs:element name="name" type="xs:string" nillable="true" />

 <xs:element name="type" type="xs:QName" nillable="true" />

 <xs:element name="readOnly" type="xs:boolean" minOccurs="0" />

 <xs:element name="supportsMultiple" type="xs:boolean" minOccurs="0" />

 <xs:element name="defaultValue" type="xs:anyType" nillable="true" />

 <xs:element name="allowedValues" nillable="true" minOccurs="0">

 <xs:complexType>

 <xs:sequence>

 <xs:element name="allowedValue" type="xs:anyType" nillable="true" minOccurs="0" maxOccurs="unbounded" />

 </xs:sequence>

 </xs:complexType>

 </xs:element>

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="Range">

 <xs:sequence>

 <xs:element name="minimum" type="xs:anyType" nillable="true" minOccurs="0" />

 <xs:element name="maximum" type="xs:anyType" nillable="true" minOccurs="0" />

 <xs:element name="minimumIsExclusive" type="xs:boolean" nillable="true" minOccurs="0" />

 <xs:element name="maximumIsExclusive" type="xs:boolean" nillable="true" minOccurs="0" />

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="Resolution">

 <xs:sequence>

 <xs:element name="width" type="xs:double" />

 <xs:element name="height" type="xs:double" />

 <xs:element name="unit" type="xs:string" nillable="true" minOccurs="0" />

 </xs:sequence>

 </xs:complexType>

 <xs:complexType name="Resource">

 <xs:sequence>

 <xs:element name="uri" type="xs:anyURI" />

 <xs:element name="contentType" type="xs:string" nillable="true" minOccurs="0" />

 <xs:element name="relationship" type="xs:string" nillable="true" minOccurs="0" />

 </xs:sequence>

 </xs:complexType>

</xs:schema>

1. Security (Informative)

This section is an informative appendix that provides security control recommendations for systems that include the use of WS-Biometric Devices.

Security requirements are context and organizational dependent. However, by providing general guidance, the OASIS Biometrics TC hopes to provide a common baseline that can be used to help ensure interoperability among components that leverage WS-Biometric Devices. If the approach to security varies widely among WS-BD enabled components, there is significantly less chance that off-the-shelf products will interoperate. This appendix is not a comprehensive security standard—therefore, updates to security guidance incorporated by reference should take precedence to any recommendation made here. In addition, security recommendations tend to be continuously updated, evolved, and improved; always seek the latest version of any of the referenced security specifications.

Further, the security controls described here are specific to the WS-Biometric Devices protocols and the components using it. It is assumed controls described here are only one component of an implementation’s overall security.

* 1. References

The following references are used in this Appendix and can provide more specific security guidance for the identified technology.

|  |  |  |
| --- | --- | --- |
| Abbreviation | Technology | Citation |
| [802.1x] | Port-based network access control | IEEE Standard 801.1X-2004, Institute of Electrical and Electronics Engineers, *Standard for Local and metropolitan area networks, Port-Based Network Access Control*, 2004. |
| [FIPS 197] | Advanced encryption standard | Federal Information Process Standards Publication 197. *Advanced Encryption Standard (AES)*. November 2001. |
| [OSI] | Network abstraction layers | ISO/IEC 7498-1:1994(E). *Open Systems Interconnect—Basic Reference Model: The Basic Model*.  |
| [800-38A] | Block cipher modes of operation | M. Dworkin. *Recommendation for Block Cipher Modes of Operation: Methods and Techniques*. NIST Special Publication 800-38A. December 2001. |
| [SP 800-60] | System sensitivity classifications | K. Stine, et al. *Guide for Mapping Types of Information and Information Systems to Security Categories*. NIST Special Publication 800-600, Volume 1, Revision 1. August 2008. |
| [SP 800-52] | Transport Layer Security (TLS) | T. Polk, S. Chokhani, and K. McKay. *DRAFT Guidelines for the Selection, Configuration, and Use of Transport Layer Security (TLS) Implementations*. NIST Special Publication 800-52 Revision 1. September 2013. |
| [SP 800-77] | IPSEC | S. Frankel, K. Kent, R. Lewkowski, A. Orebaugh, R. Ritchey, S. Sharma. *Guide to IPsec VPNs*. NIST Special Publication 800-77. December 2005. |
| [SP 800-97] | Wireless network security | S. Frankel, B. Eydt, L. Owens, K. Scarfone. *Establishing Wireless Robust Security Networks, A Guide to IEEE 802.11i*. NIST Special Publication 800-97. February 2007. |
| [SP 800-113] | SSL VPN | S. Frankel, P. Hoffman, A. Orebaugh, R. Park. *Guide to SSL VPNs*. NIST Special Publication 800-113. July 2008. |

* 1. Overview

WS-Biometric Devices components are only useful in the context of the system within which they participate. Therefore, recommended security controls are defined with respect to two orthogonal characteristics of those enclosing systems:

1. An *overall sensitivity level* of *low* (L), *medium* (M), or *high* (H) defines a set of recommended security controls. These levels roughly, but not directly, correspond to those defined in [NIST SP 800-60]. The 800-60 level accompanies other information as inputs for determining the set of recommended controls specific for WS-BD. For the sake of disambiguation, “L,” “M,” or “H” will refer to a set of controls recommended by this appendix.
2. For each sensitivity level, a set of controls is recommended to be applied at a particular layer of abstraction. For each sensitivity level, recommendations are made for controls to be applied at the *network, transport* and/or *application* level. These levels roughly, but not directly, correspond to the network, transport, and application layers defined in the OSI model [OSI].
	1. Control Set Determination

The following criteria are recommended for helping users and system owners in identifying a recommended set of security controls.

* + 1. “L” Security Control Criteria

The set of “L” controls are recommended if, for a given system, each of the following three clauses are true:

1. The system is used in a *non-production* environment **or** has an overall NIST SP 800-60 sensitivity of “Low”
2. All WS-Biometric Devices clients and servers reside within the same trusted network
3. The network that provides the WS-Biometric Devices interconnectivity network is completely isolated **or** otherwise security separated from untrusted networks with a strong buffer such as a comprehensive network firewall.

Examples that may qualify for “L” security controls are the use of WS-Biometric devices:

* In product development, testing, or other research where no real biometric data is stored or captured
* Across physical or logical components that are within an embedded device with other physical or logical controls that make it difficult to access or surreptitiously monitor the channels that carry WS-Biometric Devices traffic.
	+ 1. “M” Security Control Criteria

The set of “M” controls are recommended if, for a given system, each of the following three clauses are true:

1. The system is used in a *production* environment **or** the system has an overall NIST SP 800-60 sensitivity of “Medium”
2. All WS-Biometric Devices clients and servers reside within the same trusted network
3. The system’s network is either completely isolated or otherwise security separated from untrusted networks with a buffer such as a firewall.

Examples that may qualify for “M” security controls are the use of WS-Biometric devices:

* In an identification enrollment station, where WS-Biometric Devices is used as a “wire replacement” for other less interoperable connectors. The WS-Biometric Devices network could be composed solely of the enrollment workstation and a biometric device with an Ethernet cable between them.
* In a border screening application in which attended workstations in physically secure locations are used to submit biometrics to various law enforcement watch lists.
	+ 1. “H” Security Control Criteria

The set of “H” controls are recommended if the overall system has an NIST SP 800-60 sensitivity of “High” **or** if WS-Biometric Devices is used across an untrusted network.

* 1. Recommended & Candidate Security Controls

The following table outlines the candidate & recommended security controls. *Recommended* security controls are likely to be relevant and beneficial for all systems of a particular category. *Candidate* controls are those that are likely to more application and implementation specific.

Candidate controls are marked with an asterisk (\*). For example, in all “L” systems, any wireless networking should use WPA-2 Personal with 256-bit strength encryption (or better), and is therefore RECOMMENDED. However, the use of TLS is a *candidate* since an “L” system might comprise a communications channel that is physically isolated or otherwise embedded in a system. In that case, foregoing TLS may be an acceptable tradeoff.

There may be a degree of redundancy among these controls; for example, multiple layers of encryption. However, using multiple layers of security also affords more granular policy enforcement. For example, IPSEC may allow the communications among one set of systems, but TLS client certificates would restrict WS-Biometric Devices communications to a particularly trustworthy subset.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | L | M | H |
| Network Layer | Wired | None | 802.1x and/or IPSEC\* | IPSEC |
| Wireless | WPA-2 Personal  | WPA-2 Enterprise  | WPA-2 Enterprise |
| Transport Layer | TLS [SP 800-52] | TLS [SP 800-52] | TLS with client certificates [SP 800-52] |
| Application Layer | None | Biometric payload encryption with AES\* | Full payload encryption with AES |

* + 1. “L” Security Controls

**Network.** No network security controls are recommended for wired networks. For wireless networks, WPA-2, personal or enterprise mode is recommended.

**Transport.** TLS as described in [800-52]; the use of client certificates is optional.

**Application.** No application layer security control is recommended.

* + 1. “M” Security Controls

**Network.** Networks should be secured with 802.1x [802.1x] and/or IPSEC [SP 800-77].

**Transport.** TLS as described in [800-52]; the use of client certificates is optional.

**Application.** All biometric data (the contents of a Result’s sensorData) should be encrypted with AES as described in [FIPS 197] and [SP 800-38A].

* + 1. “H” Security Controls

**Network.** Networks should be secured with an IPSEC [800-77].

**Transport.** TLS with client certificates as described in [800-52].

**Application.** All biometric data (the contents of a Result’s sensorData) should be encrypted with AES as described in [FIPS 197] and [SP 800-38A].

1. Acknowledgments

The following individuals have participated in the creation of this specification and are gratefully acknowledged:

Participants:

Abbie Barbir, Aetna
Dwayne Bock, U.S. Bank

Adam Dale, US Department of Defense (DoD)

Angela Dormagen, US Department of Defense (DoD)

Sander Fieten, Individual

Kayee Hanoaka, NIST

Mr. Kevin Mangold, NIST
Karen Marshall, NIST

Dr. Raul Sanchez-Reillo, Carlos III University of Madrid

Julian White, United Kingdom Cabinet Office

Past Participants:

Almog Aley-Raz, Nuance

Mr. Jeremiah Bruce, US Department of Homeland Security

Mr. Doron Cohen, SafeNet, Inc.

Robin Cover, OASIS

Matthias de Haan, Tandent Vision Science, Inc

Mr. Francisco Diez-Jimeno, Carlos III University of Madrid

Dr. Jeff Dunne, Johns Hopkins University Applied Physics Laboratory

Mr. Chet Ensign, OASIS

Richard Friedhoff, Tandent Vision Science, Inc

Bob Gupta, Viometric, LLC

Emily Jay, NIST

Mr. Ken Kamakura, Fujitsu Limited

Dr. Ross Micheals, NIST

Derek Northrope, Fujitsu Limited

Mr Tony Pham, Bank of America

Dr. Raul Sanchez-Reillo, Carlos III University of Madrid

Mrs. Dee Schur, OASIS

Mr. Jeffrey Shultz, US Department of Defense (DoD)

Casey Smith, Tandent Vision Science, Inc

Mr. Kevin Strickland, Tandent Vision Science, Inc

Cathy Tilton, Daon

Mr. Ryan Triplett, Booz Allen Hamilton

Ms. Maria Vachino, Johns Hopkins University Applied Physics Laboratory

Mr. Steven Venable, Lockheed Martin

Anne Wang, 3M HIS

Youngrock Yoon, Tandent Vision Science, Inc

Notable Contributions and Support

Jacob Glueck

Authors of initial NIST specification

Ross J. Micheals

Kevin Mangold

Matt Aronoff

Kristen Greene

Kayee Kwong

Karen Marshall

Acknowledgments listed in initial NIST specification

The authors thank the following individuals and organizations for their participation in the creation of this specification.

Biometric Standards Working Group, Department of Defense

Michael Albright, Vision and Security Technology Laboratory, University of Colorado at Colorado Springs

Senaka Balasuriya, SolidBase Consulting

Terrance Boult, Vision and Security Technology Laboratory, University of Colorado at Colorado Springs

Leslie Collica, Information Technology Laboratory, National Institute of Standards and Technology

Tod Companion, Science & Technology Directorate, Department of Homeland Security

Bert Coursey, Science & Technology Directorate, Department of Homeland Security

Nick Crawford, Government Printing Office

Donna Dodson, Information Technology Laboratory, National Institute of Standards and Technology

Valerie Evanoff, Biometric Center of Excellence, Federal Bureau of Investigation

Rhonda Farrell, Booz Allen Hamilton

Michael Garris, Information Technology Laboratory, National Institute of Standards and Technology

Phillip Griffin, Booz Allen Hamilton

Dwayne Hill, Biometric Standards Working Group, Department of Defense

Rick Lazarick, Computer Sciences Corporation

John Manzo, Biometric Center of Excellence, Federal Bureau of Investigation

Charles Romine, Information Technology Laboratory, National Institute of Standards and Technology

James St. Pierre, Information Technology Laboratory, National Institute of Standards and Technology

Scott Swann, Federal Bureau of Investigation

Ashit Talukder, Information Technology Laboratory, National Institute of Standards and Technology

Cathy Tilton, Daon Inc.

Ryan Triplett, Biometric Standards Working Group, Department of Defense

Bradford Wing, Information Technology Laboratory, National Institute of Standards and Technology

1. Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| **Revision** | **Date** | **Editor** | **Changes Made** |
| WD 01 | 2016-05-09 | Kevin Mangold,Kayee Hanaoka | Initial draft derived from Biometrics TC version. |
| WD 02 | 2016-08-16 | Kevin Mangold,Kayee Hanaoka | New asynchronous capture operations, raw sensor data download, get sensor status  |